  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: The nuclear structure in nearby AGN at 3-500 Schwarzschild radii resolut
 Exp. Code:  gs032a  


Schedule Version:       1.30
Processed by SCHED version:  11.10  Version 11.1 Beta of about April 26, 201

PI:       Tuomas Savolainen

Address:  MPIfR Bonn
          Auf dem Huegel 69
          53121 Bonn, Germany
 

Phone:    +49 (228) 525 473
EMAIL:    tsavolainen@mpifr-bonn.mpg.de
Fax:
Phone during observation: +49 (172) 408 2561

Observing mode: C/K-band, dual-pol

Notes:    C/K-band, Radioastron-compatible frequency setup
          P-CAL is ON
          Tsys is ON, auto-level (AGC) is ON
          Please, send Mk5 disk packs to MPIfR-Bonn

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               The nuclear structure in nearby AGN at 3-500 Schwarzschild radii resolut
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  22 Sep 2013   Day 265 ---

 ---------- K-band VLBI scans ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00
 Next scan bandwidths:      16.00     16.00     16.00     16.00

06 10 00  0316+413     23 19 18  41.0  59.6 -4.0     -82.5     0        0   06 10 00
06 19 30  ---          23 28 50  42.8  59.8 -3.9     -83.8   570       18   06 10 01

06 20 30  0316+413     23 29 50  43.0  59.9 -3.8     -84.0    54       18   06 20 30
06 30 00  ---          23 39 22  44.8  60.1 -3.7     -85.4   570       37   06 20 31

06 31 00  0316+413     23 40 22  44.9  60.1 -3.7     -85.6    54       37   06 31 00
06 40 30  ---          23 49 53  46.7  60.3 -3.5     -87.0   570       55   06 31 01

06 41 30  0316+413     23 50 54  46.9  60.3 -3.5     -87.2    54       55   06 41 30
06 50 00  ---          23 59 25  48.5  60.4 -3.4     -88.5   510       71   06 41 31

 ---------- K-band GRT-only VLBI scans ----------

06 56 00  0355+508     00 05 26  42.6  47.0 -3.9     -92.0   339       71   06 56 00
06 58 00  ---          00 07 26  42.9  47.0 -3.9     -92.4   120       75   06 56 01

06 59 00  0307+380     00 08 26  51.8  65.7 -3.1     -87.4    35       75   06 59 00
07 01 00  ---          00 10 27  52.2  65.7 -3.0     -87.7   120       79   06 59 01

07 02 40  0316+413     00 12 07  50.9  60.4 -3.1     -90.6    88       79   07 02 40
07 12 10  ---          00 21 39  52.7  60.3 -3.0     -92.3   570       97   07 02 41

07 13 30  0316+413     00 22 59  52.9  60.3 -3.0     -92.5    74       97   07 13 30
07 23 00  ---          00 32 30  54.7  60.1 -2.8     -94.2   570      115   07 13 31

07 24 40  0307+380     00 34 11  56.9  65.8 -2.6     -91.3    88      115   07 24 40
07 26 40  ---          00 36 11  57.3  65.7 -2.6     -91.6   120      119   07 24 41

 ---------- 09:20 min gap for Effelsberg pointing ----------

07 27 10  0316+413     00 36 41  55.5  60.0 -2.7     -95.0    18      119   07 27 10
07 32 10  ---          00 41 42  56.4  59.9 -2.7     -96.0   300      129   07 27 11

07 33 30  0316+413     00 43 02  56.7  59.8 -2.6     -96.2    74      129   07 33 30
07 43 00  ---          00 52 34  58.4  59.4 -2.5     -98.2   570      147   07 33 31

07 44 50  0355+508     00 54 24  50.2  45.6 -3.1    -102.6    85      147   07 44 50
07 46 50  ---          00 56 24  50.5  45.4 -3.1    -103.0   120      151   07 44 51
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               The nuclear structure in nearby AGN at 3-500 Schwarzschild radii resolut
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  22 Sep 2013   Day 265 ---

07 48 20  0307+380     00 57 55  61.5  65.2 -2.2     -95.4    61      151   07 48 20
07 50 20  ---          00 59 55  61.9  65.2 -2.2     -95.8   120      155   07 48 21

07 52 10  0316+413     01 01 45  60.1  58.9 -2.3    -100.1    98      155   07 52 10
07 59 00  ---          01 08 36  61.4  58.4 -2.2    -101.7   410      168   07 52 11

08 04 20  0316+413     01 13 57  62.4  57.9 -2.1    -103.0   314      168   08 04 20
08 08 20  ---          01 17 58  63.1  57.5 -2.0    -104.0   240      176   08 04 21

 ---------- K-band VLBI scans ----------

08 10 00  0316+413     01 19 38  63.4  57.4 -2.0    -104.4    94      176   08 10 00
08 19 30  ---          01 29 10  65.1  56.3 -1.9    -107.0   570      194   08 10 01

08 20 30  0316+413     01 30 10  65.3  56.1 -1.8    -107.3    54      194   08 20 30
08 30 00  ---          01 39 41  67.0  54.7 -1.7    -110.2   570      212   08 20 31

08 31 00  0316+413     01 40 42  67.1  54.5 -1.7    -110.5    54      212   08 31 00
08 40 30  ---          01 50 13  68.8  52.8 -1.5    -113.7   570      230   08 31 01

08 41 30  0316+413     01 51 13  69.0  52.6 -1.5    -114.1    54      230   08 41 30
08 50 00  ---          01 59 45  70.4  50.6 -1.4    -117.4   510      247   08 41 31

 ---------- C-band GRT-only VLBI scans ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

08 50 30  0316+413     02 00 15  70.5  50.4 -1.3    -117.6    15      247   08 50 30
09 00 00  ---          02 09 46  72.0  47.7 -1.2    -121.8   570      265   08 50 31

09 01 30  0307+380     02 11 17  75.4  54.3 -1.0    -117.1    76      265   09 01 30
09 03 30  ---          02 13 17  75.7  53.5 -1.0    -118.1   120      269   09 01 31

09 05 00  0316+413     02 14 47  72.8  46.0 -1.1    -124.2    76      269   09 05 00
09 11 00  ---          02 20 48  73.7  43.7 -1.0    -127.4   360      280   09 05 01

 Next scan frequencies:  15368.00  15368.00  15384.00  15384.00
 Next BBC frequencies:     768.00    768.00    784.00    784.00

09 13 50  0316+413     02 23 39  74.2  42.5 -1.0    -129.0   155      280   09 13 50
09 18 30  ---          02 28 19  74.8  40.4 -0.9    -131.8   280      289   09 13 51
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               The nuclear structure in nearby AGN at 3-500 Schwarzschild radii resolut
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  22 Sep 2013   Day 265 ---

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

09 19 50  0316+413     02 29 40  75.0  39.7 -0.9    -132.7    65      289   09 19 50
09 24 30  ---          02 34 20  75.6  37.3 -0.8    -135.8   280      298   09 19 51

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

09 25 50  0316+413     02 35 41  75.8  36.6 -0.8    -136.7    74      298   09 25 50
09 30 30  ---          02 40 21  76.4  33.9 -0.7    -140.1   280      307   09 25 51

09 31 00  0307+380     02 40 51  80.0  37.6 -0.5    -138.0    15      307   09 31 00
09 33 00  ---          02 42 52  80.3  35.9 -0.5    -140.0   120      311   09 31 01

 Next scan frequencies:  15368.00  15368.00  15384.00  15384.00
 Next BBC frequencies:     768.00    768.00    784.00    784.00

09 35 40  0316+413     02 45 32  77.0  30.6 -0.6    -144.2   145      311   09 35 40
09 40 20  ---          02 50 13  77.5  27.3 -0.5    -148.2   280      320   09 35 41

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

09 41 40  0316+413     02 51 33  77.6  26.3 -0.5    -149.4    74      320   09 41 40
09 46 40  ---          02 56 34  78.0  22.4 -0.4    -154.1   300      330   09 41 41

 ---------- K-band VLBI scans ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

10 00 00  0316+413     03 09 56  78.9  10.5 -0.2    -167.9   793      330   10 00 00
10 09 30  ---          03 19 28  79.1   1.3 -0.0    -178.5   570      348   10 00 01

10 10 30  0316+413     03 20 28  79.1   0.3 -0.0    -179.7    54      348   10 10 30
10 20 00  ---          03 29 59  78.9  -9.0  0.2     169.6   570      366   10 10 31

10 21 00  0316+413     03 31 00  78.9 -10.0  0.2     168.5    54      366   10 21 00
10 30 30  ---          03 40 31  78.4 -18.7  0.3     158.4   570      385   10 21 01

10 31 30  0316+413     03 41 31  78.3 -19.5  0.3     157.4    54      385   10 31 30
10 40 00  ---          03 50 03  77.6 -26.3  0.5     149.3   510      401   10 31 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

10 44 10  0316+413     03 54 13  77.2 -29.4  0.6     145.7   243      401   10 44 10
10 53 40  ---          04 03 45  76.1 -35.4  0.7     138.2   570      419   10 44 11
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               The nuclear structure in nearby AGN at 3-500 Schwarzschild radii resolut
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  22 Sep 2013   Day 265 ---

10 54 40  0307+380     04 04 45  76.7 -51.3  0.9     121.1    41      419   10 54 40
10 56 40  ---          04 06 45  76.3 -52.2  0.9     120.0   120      423   10 54 41

 Next scan frequencies:  15368.00  15368.00  15384.00  15384.00
 Next BBC frequencies:     768.00    768.00    784.00    784.00

10 59 20  0316+413     04 09 26  75.3 -38.5  0.8     134.2   141      423   10 59 20
11 03 40  ---          04 13 47  74.7 -40.7  0.9     131.5   260      431   10 59 21

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

11 05 00  0316+413     04 15 07  74.5 -41.3  0.9     130.6    74      431   11 05 00
11 09 20  ---          04 19 28  73.9 -43.2  1.0     128.1   260      440   11 05 01

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

11 10 40  0316+413     04 20 48  73.7 -43.7  1.0     127.3    74      440   11 10 40
11 15 00  ---          04 25 08  73.1 -45.4  1.1     125.0   260      448   11 10 41

11 15 40  0307+380     04 25 49  73.0 -58.3  1.2     111.2    23      448   11 15 40
11 17 40  ---          04 27 49  72.6 -58.7  1.3     110.4   120      452   11 15 41

 Next scan frequencies:  15368.00  15368.00  15384.00  15384.00
 Next BBC frequencies:     768.00    768.00    784.00    784.00

11 19 50  0316+413     04 29 59  72.3 -47.1  1.2     122.6   113      452   11 19 50
11 24 10  ---          04 34 20  71.6 -48.5  1.2     120.6   260      460   11 19 51

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

11 25 30  0316+413     04 35 40  71.4 -48.9  1.2     120.0    74      460   11 25 30
11 30 10  ---          04 40 21  70.6 -50.2  1.3     118.0   280      469   11 25 31

 Next scan frequencies:  15368.00  15368.00  15384.00  15384.00
 Next BBC frequencies:     768.00    768.00    784.00    784.00

11 32 20  0316+413     04 42 31  70.3 -50.8  1.4     117.1   124      469   11 32 20
11 35 40  ---          04 45 52  69.7 -51.6  1.4     115.7   200      476   11 32 21

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

11 37 00  0316+413     04 47 12  69.5 -51.9  1.4     115.2    74      476   11 37 00
11 40 20  ---          04 50 33  68.9 -52.6  1.5     114.0   200      482   11 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               The nuclear structure in nearby AGN at 3-500 Schwarzschild radii resolut
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  22 Sep 2013   Day 265 ---

 Next scan frequencies:  15368.00  15368.00  15384.00  15384.00
 Next BBC frequencies:     768.00    768.00    784.00    784.00

11 42 30  0316+413     04 52 43  68.5 -53.1  1.5     113.2   124      482   11 42 30
11 45 50  ---          04 56 04  68.0 -53.7  1.6     112.1   200      488   11 42 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

11 47 10  0316+413     04 57 24  67.7 -54.0  1.6     111.6    74      488   11 47 10
11 50 30  ---          05 00 44  67.2 -54.5  1.7     110.5   200      495   11 47 11

 ---------- K-band VLBI scans ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

11 55 00  0316+413     05 05 15  66.4 -55.3  1.7     109.1   264      495   11 55 00
12 04 30  ---          05 14 47  64.7 -56.6  1.9     106.3   570      513   11 55 01

12 05 30  0316+413     05 15 47  64.5 -56.7  1.9     106.1    54      513   12 05 30
12 15 00  ---          05 25 18  62.8 -57.7  2.1     103.6   570      531   12 05 31

12 16 00  0316+413     05 26 18  62.6 -57.8  2.1     103.3    54      531   12 16 00
12 25 30  ---          05 35 50  60.8 -58.6  2.3     101.0   570      550   12 16 01

12 26 30  0316+413     05 36 50  60.7 -58.7  2.3     100.8    54      550   12 26 30
12 35 00  ---          05 45 22  59.1 -59.2  2.4      98.9   510      566   12 26 31

 ---------- multi-frequency VLBA-only scans ----------

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

12 35 10  0316+413     05 45 32  59.1 -59.2  2.4      98.9     4      566   12 35 10
12 39 10  ---          05 49 32  58.3 -59.4  2.5      98.0   240      574   12 35 11

 Next scan frequencies:  15368.00  15368.00  15384.00  15384.00
 Next BBC frequencies:     768.00    768.00    784.00    784.00

12 39 20  0316+413     05 49 42  58.3 -59.5  2.5      98.0     4      574   12 39 20
12 43 20  ---          05 53 43  57.5 -59.6  2.5      97.2   240      581   12 39 21

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

12 43 30  0316+413     05 53 53  57.5 -59.6  2.6      97.1     4      581   12 43 30
12 47 30  ---          05 57 54  56.8 -59.8  2.6      96.3   240      589   12 43 31
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               The nuclear structure in nearby AGN at 3-500 Schwarzschild radii resolut
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  22 Sep 2013   Day 265 ---

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

12 47 40  0316+413     05 58 04  56.7 -59.8  2.6      96.3     4      589   12 47 40
12 51 40  ---          06 02 04  56.0 -60.0  2.7      95.5   240      597   12 47 41

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

12 51 50  0316+413     06 02 14  56.0 -60.0  2.7      95.5     4      597   12 51 50
12 55 50  ---          06 06 15  55.2 -60.1  2.8      94.7   240      604   12 51 51

 Next scan frequencies:  15368.00  15368.00  15384.00  15384.00
 Next BBC frequencies:     768.00    768.00    784.00    784.00

12 56 00  0316+413     06 06 25  55.2 -60.1  2.8      94.7     4      604   12 56 00
13 00 00  ---          06 10 26  54.4 -60.2  2.8      94.0   240      612   12 56 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra1cm2.set
   Matching groups in ./freq.sess313rdbe.dat:
     v1cm_b3

   Setup group:   30         Station: VLBA_FD           Total bit rate:   256
   Format: MARK5B            Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1     15.1     12.4

  The following frequency sets based on these setups were used.

   Frequency Set:  31  Setup file default.
   LO sum=   22236.00  22236.00  22236.00  22236.00
   BBC fr=     736.00    736.00    736.00    736.00
   Bandwd=      16.00     16.00     16.00     16.00
    Matching frequency sets:  31  32  33  34  35  36  37  38  39  40

   Track assignments are: 
    track1=   2,  4,  6,  8
    barrel=roll_off 


 ======== Setup file: ra6cm2.set
   Matching groups in ./freq.sess313rdbe.dat:
     vc_d

   Setup group:    7         Station: VLBA_FD           Total bit rate:   256
   Format: MARK5B            Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.1      4.1     15.1

  The following frequency sets based on these setups were used.

   Frequency Set:  26  Setup file default.
   LO sum=   4836.00  4836.00  4836.00  4836.00
   BBC fr=    736.00   736.00   736.00   736.00
   Bandwd=     16.00    16.00    16.00    16.00
    Matching frequency sets:  26  27  28  29  30  41  42  43  44  45

   Track assignments are: 
    track1=   2,  4,  6,  8
    barrel=roll_off 


 ======== Setup file: ra2cm2.set
   Matching groups in ./freq.sess313rdbe.dat:
     v2cm_d3         Fourth 2cm filter

   Setup group:   60         Station: VLBA_FD           Total bit rate:   256
   Format: MARK5B            Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14600.00  14600.00  14600.00  14600.00
   Net SB=         U         U         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         U         U         U         U
   IF    =        B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.6     11.4     11.4

  The following frequency sets based on these setups were used.

   Frequency Set:  46  Setup file default.
   LO sum=   15368.00  15368.00  15384.00  15384.00
   BBC fr=     768.00    768.00    784.00    784.00
   Bandwd=      16.00     16.00     16.00     16.00
    Matching frequency sets:  46  47  48  49  50  51  52  53  54  55

   Track assignments are: 
    track1=   2,  4,  6,  8
    barrel=roll_off 


 ======== Setup file: ra7mm2.set
   Matching groups in ./freq.sess313rdbe.dat:
     v7mm_c8

   Setup group:   49         Station: VLBA_FD           Total bit rate:   256
   Format: MARK5B            Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         U         U         U         U
   IF    =        A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=  15.1      7.6     11.6

  The following frequency sets based on these setups were used.

   Frequency Set:  56  Setup file default.
   LO sum=   43120.00  43120.00  43136.00  43136.00
   BBC fr=     720.00    720.00    736.00    736.00
   Bandwd=      16.00     16.00     16.00     16.00
    Matching frequency sets:  56  57  58  59  60  61  62  63  64  65

   Track assignments are: 
    track1=   2,  4,  6,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 23.552455       0.00
                     85 16 41.77889    * 85 00 00.00000      84 55 21.51327        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for the TS to look at

   J0310+3814        03 07 37.554068   * 03 10 49.879926     03 11 44.922072       0.13
 * 0307+380          38 03 34.47086    * 38 14 53.83785      38 17 54.30640        0.10
                     ./sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 6526 observations

   J0319+4130        03 16 29.567260   * 03 19 48.160090     03 20 44.982340       1.30
 * 0316+413          41 19 51.91699    * 41 30 42.10412      41 33 32.92264        2.72
   3C84              ./sources.vlba
   J0319+41          GSFC 2011B astro solution      9957 Observations

   J0359+5057        03 55 45.261370   * 03 59 29.747271     04 00 33.763079       0.16
 * 0355+508          50 49 20.28582    * 50 57 50.16177      50 59 56.63384        0.10
   J0359+50          ./sources.vlba
   NRAO150           rfc_2012b Petrov, 2012, unpublished 18568 observations

   J0542+4951        05 38 43.517523   * 05 42 36.137900     05 43 41.187682       0.16
   0538+498          49 49 42.83711    * 49 51 07.23374      49 51 12.22607        0.11
 * 3C147             ./sources.vlba
   J0542+49          rfc_2012b Petrov, 2012, unpublished 1742 observations



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra6cm2.set            4                                 6.958     0.000
  0307+380   ra6cm2.set            4 9 10 11 12 13 16 17 18 20 +     0.833    32.222
             ra1cm2.set            1 7 8 14 15 19 22 31              1.033    16.467
  0316+413   ra6cm2.set            4 9 10 11 12 13 16 17 18 20 +    15.406   436.095
             ra1cm2.set            1 7 8 14 15 19 22 31             16.272   201.912
             ra7mm2.set            24 56                             0.656    29.222
             ra2cm2.set            25 46                             0.644    28.611
             ps/vla_x_pointing.set 21                                0.208     0.000
  0355+508   ra6cm2.set            4 9 10 11 12 13 16 17 20 26       0.500    17.167
             ra1cm2.set            1 7 8 14 15 19 22 31              0.500     8.017
  3C147      ra6cm2.set            23                                0.067     0.000
             ra1cm2.set            22                                0.067     0.000
             ra7mm2.set            24                                0.067     0.000
             ra2cm2.set            25                                0.067     0.000


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA              84.6
   0307+380           121.0
   0316+413           118.0
   0355+508           107.6
   3C147               92.0

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

