  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GMVA Sep 25-29, 2014
 Exp. Code:  c142a   


Schedule Version:       9.00
Processed by SCHED version:  11.30  Version 11.3 update 1.  April 14, 2014

PI:       Global mm-VLBI Array (GMVA)

Address:  Max-Planck-Institut fuer Radioastronomie
          Auf dem Huegel 69
          53121 Bonn
          Germany

Phone:    0049-228-525-295
EMAIL:    tkrichbaum@mpifr-bonn.mpg.de
Fax:      0049-2257-301-106
Phone during observation: 0049-2257-301-155

Observing mode: 2048-16-2

Notes:    3mm RDBE_PFB, VLBA 7mm autopeak
          3mm dual polarisation
          measure Tsys before AND after VLBI scan and provide tau
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00
 Next scan bandwidths:      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                            32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00

00 57 06  P-VXSGR      18 20 22  37.1 183.3  0.2       3.1     0        0   Stopped 
00 58 06  ---          18 21 22  37.1 183.6  0.2       3.3    60        0           

 ---------- Following scan added by Sched for reference pointing ----------

00 58 12  P-VXSGR      18 21 28  37.1 183.6  0.2       3.4     0        0   Stopped 
00 59 12  ---          18 22 28  37.0 183.9  0.2       3.6    60        0           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 00 00  1510-089     18 23 16  29.6 236.7  3.2      46.8     3        0   01 00 00
01 07 00  ---          18 30 18  28.3 238.1  3.3      47.7   420      108   01 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

01 07 20  1510-089     18 30 38  28.3 238.1  3.3      47.7    14      108   01 07 20
01 10 40  ---          18 33 58  27.6 238.7  3.3      48.2   200      159   01 07 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 12 08  P-VXSGR      18 35 26  36.8 187.7  0.4       7.1    43      159   Stopped 
01 13 08  ---          18 36 26  36.7 187.9  0.5       7.4    60      159           

 ---------- Following scan added by Sched for reference pointing ----------

01 13 14  P-VXSGR      18 36 32  36.7 188.0  0.5       7.4     0      159   Stopped 
01 14 14  ---          18 37 32  36.7 188.3  0.5       7.7    60      159           
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 15 01  1510-089     18 38 20  26.8 239.5  3.4      48.7     3      159   01 15 01
01 22 01  ---          18 45 21  25.5 240.8  3.5      49.5   420      267   01 15 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

01 22 21  1510-089     18 45 41  25.5 240.9  3.5      49.6    14      267   01 22 21
01 25 41  ---          18 49 02  24.8 241.5  3.6      50.0   200      318   01 22 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 27 08  P-VXSGR      18 50 29  36.2 191.9  0.7      11.1    44      318   Stopped 
01 28 08  ---          18 51 29  36.2 192.2  0.7      11.3    60      318           

 ---------- Following scan added by Sched for reference pointing ----------

01 28 14  P-VXSGR      18 51 35  36.2 192.2  0.7      11.4     0      318   Stopped 
01 29 14  ---          18 52 36  36.1 192.5  0.7      11.6    60      318           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 30 01  1510-089     18 53 22  24.0 242.2  3.7      50.4     3      318   01 30 01
01 37 01  ---          19 00 23  22.7 243.4  3.8      51.2   420      426   01 30 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

01 37 21  1510-089     19 00 43  22.6 243.5  3.8      51.2    14      426   01 37 21
01 40 41  ---          19 04 04  22.0 244.0  3.8      51.6   200      477   01 37 22
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 42 09  P-VXSGR      19 05 33  35.4 196.1  0.9      15.0    46      477   Stopped 
01 43 09  ---          19 06 33  35.4 196.4  1.0      15.2    60      477           

 ---------- Following scan added by Sched for reference pointing ----------

01 43 15  P-VXSGR      19 06 39  35.4 196.4  1.0      15.2     0      477   Stopped 
01 44 15  ---          19 07 39  35.3 196.7  1.0      15.5    60      477           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 45 01  1510-089     19 08 25  21.1 244.7  3.9      52.0     4      477   01 45 01
01 52 01  ---          19 15 26  19.7 245.9  4.0      52.7   420      585   01 45 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

01 52 21  1510-089     19 15 46  19.7 245.9  4.0      52.7    14      585   01 52 21
01 55 41  ---          19 19 07  19.0 246.4  4.1      53.0   200      636   01 52 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 57 11  P-VXSGR      19 20 36  34.4 200.2  1.2      18.7    49      636   Stopped 
01 58 11  ---          19 21 36  34.3 200.5  1.2      19.0    60      636           

 ---------- Following scan added by Sched for reference pointing ----------

01 58 17  P-VXSGR      19 21 42  34.3 200.5  1.2      19.0     0      636   Stopped 
01 59 17  ---          19 22 43  34.3 200.7  1.2      19.2    60      636           
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 00 01  1510-089     19 23 27  18.2 247.1  4.2      53.4     4      636   02 00 01
02 07 01  ---          19 30 28  16.8 248.2  4.3      54.0   420      744   02 00 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

02 07 21  1510-089     19 30 48  16.7 248.2  4.3      54.0    14      744   02 07 21
02 10 41  ---          19 34 09  16.0 248.7  4.3      54.3   200      795   02 07 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 12 12  P-VXSGR      19 35 40  33.2 204.1  1.4      22.3    49      795   Stopped 
02 13 12  ---          19 36 40  33.1 204.4  1.5      22.6    60      795           

 ---------- Following scan added by Sched for reference pointing ----------

02 13 18  P-VXSGR      19 36 46  33.1 204.4  1.5      22.6     0      795   Stopped 
02 14 18  ---          19 37 46  33.0 204.7  1.5      22.8    60      795           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 15 01  1510-089     19 38 30  15.2 249.4  4.4      54.7     0      795   02 15 01
02 22 01  ---          19 45 31  13.7 250.4  4.5      55.2   420      903   02 15 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

02 22 21  1510-089     19 45 51  13.7 250.5  4.5      55.2    14      903   02 22 21
02 25 41  ---          19 49 11  13.0 250.9  4.6      55.5   200      954   02 22 22
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 27 09  P-VXSGR      19 50 39  31.8 207.9  1.7      25.8    42      954   Stopped 
02 28 09  ---          19 51 39  31.7 208.1  1.7      26.0    60      954           

 ---------- Following scan added by Sched for reference pointing ----------

02 28 15  P-VXSGR      19 51 45  31.7 208.1  1.7      26.0     0      954   Stopped 
02 29 15  ---          19 52 46  31.6 208.4  1.7      26.2    60      954           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 30 01  1510-089     19 53 32  12.1 251.6  4.7      55.8     0      954   02 30 01
02 37 01  ---          20 00 33  10.7 252.6  4.8      56.2   420     1062   02 30 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

02 37 21  1510-089     20 00 53  10.6 252.6  4.8      56.3    14     1062   02 37 21
02 40 41  ---          20 04 14   9.9 253.1  4.8      56.5   200     1113   02 37 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 42 49  3C454.3      20 06 22  49.1 100.8 -2.8     -61.7    11     1113   Stopped 
02 43 49  ---          20 07 22  49.3 101.0 -2.8     -61.6    60     1113           

 ---------- Following scan added by Sched for reference pointing ----------

02 43 55  3C454.3      20 07 28  49.3 101.0 -2.8     -61.6     0     1113   Stopped 
02 44 55  ---          20 08 28  49.5 101.2 -2.8     -61.5    60     1113           
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 45 01  3C454.3      20 08 35  49.5 101.2 -2.8     -61.5     0     1113   02 45 01
02 52 01  ---          20 15 36  51.0 102.4 -2.7     -61.1   420     1221   02 45 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

02 52 21  3C454.3      20 15 56  51.1 102.5 -2.6     -61.0    14     1221   02 52 21
02 55 41  ---          20 19 16  51.8 103.1 -2.6     -60.8   200     1272   02 52 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 57 49  3C454.3      20 21 24  52.2 103.5 -2.6     -60.6   121     1272   Stopped 
02 58 49  ---          20 22 25  52.4 103.7 -2.5     -60.5    60     1272           

 ---------- Following scan added by Sched for reference pointing ----------

02 58 55  3C454.3      20 22 31  52.5 103.7 -2.5     -60.5     0     1272   Stopped 
02 59 55  ---          20 23 31  52.7 103.9 -2.5     -60.4    60     1272           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 00 01  3C454.3      20 23 37  52.7 104.0 -2.5     -60.4     0     1272   03 00 01
03 07 01  ---          20 30 38  54.2 105.4 -2.4     -59.8   420     1379   03 00 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

03 07 21  3C454.3      20 30 58  54.2 105.4 -2.4     -59.7    14     1379   03 07 21
03 10 41  ---          20 34 19  54.9 106.1 -2.3     -59.4   200     1431   03 07 22
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

03 12 49  3C454.3      20 36 27  55.4 106.6 -2.3     -59.2   121     1431   Stopped 
03 13 49  ---          20 37 27  55.6 106.8 -2.3     -59.1    60     1431           

 ---------- Following scan added by Sched for reference pointing ----------

03 13 55  3C454.3      20 37 33  55.6 106.8 -2.3     -59.1     0     1431   Stopped 
03 14 55  ---          20 38 33  55.8 107.1 -2.3     -59.0    60     1431           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 15 01  3C454.3      20 38 40  55.8 107.1 -2.3     -58.9     0     1431   03 15 01
03 22 01  ---          20 45 41  57.2 108.7 -2.2     -58.1   420     1538   03 15 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

03 22 21  3C454.3      20 46 01  57.3 108.8 -2.1     -58.1    14     1538   03 22 21
03 25 41  ---          20 49 21  58.0 109.6 -2.1     -57.6   200     1590   03 22 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

03 27 11  P-WXPSC      20 50 51  28.6  91.8 -4.3     -61.8    24     1590   Stopped 
03 28 11  ---          20 51 51  28.8  92.0 -4.3     -61.8    60     1590           

 ---------- Following scan added by Sched for reference pointing ----------

03 28 17  P-WXPSC      20 51 57  28.8  92.0 -4.3     -61.8     0     1590   Stopped 
03 29 17  ---          20 52 58  29.0  92.1 -4.2     -61.8    60     1590           
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 30 00  3C84         20 53 41  15.2  50.3 -6.5     -62.3     6     1590   03 30 00
03 37 00  ---          21 00 42  16.4  51.0 -6.3     -63.3   420     1697   03 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

03 37 20  3C84         21 01 02  16.4  51.0 -6.3     -63.3    14     1697   03 37 20
03 40 40  ---          21 04 23  17.0  51.3 -6.3     -63.8   200     1749   03 37 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

03 42 48  3C84         21 06 31  17.3  51.5 -6.2     -64.1   121     1749   Stopped 
03 43 48  ---          21 07 31  17.5  51.6 -6.2     -64.2    60     1749           

 ---------- Following scan added by Sched for reference pointing ----------

03 43 54  3C84         21 07 37  17.5  51.6 -6.2     -64.3     0     1749   Stopped 
03 44 54  ---          21 08 37  17.7  51.7 -6.2     -64.4    60     1749           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 45 00  3C84         21 08 43  17.7  51.7 -6.2     -64.4     0     1749   03 45 00
03 52 00  ---          21 15 45  18.9  52.2 -6.1     -65.4   420     1856   03 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

03 52 20  3C84         21 16 05  19.0  52.3 -6.1     -65.4    14     1856   03 52 20
03 55 40  ---          21 19 25  19.5  52.5 -6.0     -65.9   200     1908   03 52 21
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

03 57 48  3C84         21 21 33  19.9  52.7 -6.0     -66.2   121     1908   Stopped 
03 58 48  ---          21 22 34  20.1  52.8 -6.0     -66.3    60     1908           

 ---------- Following scan added by Sched for reference pointing ----------

03 58 54  3C84         21 22 40  20.1  52.8 -6.0     -66.4     0     1908   Stopped 
03 59 54  ---          21 23 40  20.2  52.9 -6.0     -66.5    60     1908           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 00 00  3C84         21 23 46  20.3  52.9 -6.0     -66.5     0     1908   04 00 00
04 07 00  ---          21 30 47  21.5  53.4 -5.8     -67.5   420     2015   04 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

04 07 20  3C84         21 31 07  21.5  53.5 -5.8     -67.5    14     2015   04 07 20
04 10 40  ---          21 34 28  22.1  53.7 -5.8     -68.0   200     2067   04 07 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 12 48  3C84         21 36 36  22.5  53.9 -5.7     -68.3   121     2067   Stopped 
04 13 48  ---          21 37 36  22.7  54.0 -5.7     -68.4    60     2067           

 ---------- Following scan added by Sched for reference pointing ----------

04 13 54  3C84         21 37 42  22.7  54.0 -5.7     -68.4     0     2067   Stopped 
04 14 54  ---          21 38 42  22.8  54.0 -5.7     -68.6    60     2067           
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 15 00  3C84         21 38 48  22.9  54.1 -5.7     -68.6     0     2067   04 15 00
04 22 00  ---          21 45 50  24.1  54.6 -5.6     -69.5   420     2174   04 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

04 22 20  3C84         21 46 10  24.1  54.6 -5.6     -69.6    14     2174   04 22 20
04 25 40  ---          21 49 30  24.7  54.8 -5.5     -70.0   200     2226   04 22 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 27 48  3C84         21 51 38  25.1  55.0 -5.5     -70.3   121     2226   Stopped 
04 28 48  ---          21 52 38  25.3  55.0 -5.5     -70.5    60     2226           

 ---------- Following scan added by Sched for reference pointing ----------

04 28 54  3C84         21 52 44  25.3  55.0 -5.5     -70.5     0     2226   Stopped 
04 29 54  ---          21 53 45  25.5  55.1 -5.5     -70.6    60     2226           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 30 00  3C84         21 53 51  25.5  55.1 -5.4     -70.6     0     2226   04 30 00
04 37 00  ---          22 00 52  26.7  55.6 -5.3     -71.6   420     2333   04 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

04 37 20  3C84         22 01 12  26.8  55.6 -5.3     -71.6    14     2333   04 37 20
04 40 40  ---          22 04 33  27.4  55.8 -5.3     -72.1   200     2385   04 37 21
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 42 48  3C84         22 06 41  27.8  56.0 -5.2     -72.4   121     2385   Stopped 
04 43 48  ---          22 07 41  28.0  56.0 -5.2     -72.5    60     2385           

 ---------- Following scan added by Sched for reference pointing ----------

04 43 54  3C84         22 07 47  28.0  56.0 -5.2     -72.5     0     2385   Stopped 
04 44 54  ---          22 08 47  28.2  56.1 -5.2     -72.7    60     2385           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 45 00  3C84         22 08 53  28.2  56.1 -5.2     -72.7     0     2385   04 45 00
04 52 00  ---          22 15 54  29.4  56.6 -5.1     -73.6   420     2492   04 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

04 52 20  3C84         22 16 15  29.5  56.6 -5.1     -73.7    14     2492   04 52 20
04 55 40  ---          22 19 35  30.1  56.8 -5.0     -74.1   200     2544   04 52 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 57 29  P-TXCAM      22 21 24  19.8  35.6 -6.7     -64.2    80     2544   Stopped 
04 58 29  ---          22 22 25  19.9  35.7 -6.7     -64.4    60     2544           

 ---------- Following scan added by Sched for reference pointing ----------

04 58 35  P-TXCAM      22 22 31  19.9  35.7 -6.7     -64.4     0     2544   Stopped 
04 59 35  ---          22 23 31  20.1  35.7 -6.6     -64.6    60     2544           
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 00 00  3C111        22 23 56  19.1  56.4 -5.9     -65.6     2     2544   05 00 00
05 07 00  ---          22 30 57  20.4  57.0 -5.8     -66.5   420     2651   05 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

05 07 20  3C111        22 31 17  20.4  57.1 -5.8     -66.5    14     2651   05 07 20
05 10 40  ---          22 34 38  21.1  57.3 -5.7     -66.9   200     2703   05 07 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 12 48  3C84         22 36 46  33.2  57.7 -4.7     -76.5    96     2703   Stopped 
05 13 48  ---          22 37 46  33.4  57.8 -4.7     -76.6    60     2703           

 ---------- Following scan added by Sched for reference pointing ----------

05 13 54  3C84         22 37 52  33.4  57.8 -4.7     -76.6     0     2703   Stopped 
05 14 54  ---          22 38 52  33.6  57.8 -4.7     -76.8    60     2703           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 15 00  3C84         22 38 58  33.6  57.8 -4.7     -76.8     0     2703   05 15 00
05 22 00  ---          22 45 59  34.9  58.2 -4.6     -77.8   420     2810   05 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

05 22 20  3C84         22 46 19  34.9  58.2 -4.6     -77.8    14     2810   05 22 20
05 25 40  ---          22 49 40  35.6  58.4 -4.5     -78.3   200     2862   05 22 21
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 27 48  3C84         22 51 48  35.9  58.5 -4.5     -78.6   121     2862   Stopped 
05 28 48  ---          22 52 48  36.1  58.5 -4.5     -78.7    60     2862           

 ---------- Following scan added by Sched for reference pointing ----------

05 28 54  3C84         22 52 54  36.1  58.5 -4.5     -78.7     0     2862   Stopped 
05 29 54  ---          22 53 54  36.3  58.6 -4.4     -78.9    60     2862           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 30 00  3C84         22 54 01  36.4  58.6 -4.4     -78.9     0     2862   05 30 00
05 37 00  ---          23 01 02  37.6  58.9 -4.3     -79.9   420     2969   05 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

05 37 20  3C84         23 01 22  37.7  58.9 -4.3     -79.9    14     2969   05 37 20
05 40 40  ---          23 04 42  38.3  59.0 -4.3     -80.4   200     3021   05 37 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 42 48  3C84         23 06 51  38.7  59.1 -4.2     -80.7   121     3021   Stopped 
05 43 48  ---          23 07 51  38.9  59.1 -4.2     -80.8    60     3021           

 ---------- Following scan added by Sched for reference pointing ----------

05 43 54  3C84         23 07 57  38.9  59.1 -4.2     -80.8     0     3021   Stopped 
05 44 54  ---          23 08 57  39.1  59.2 -4.2     -81.0    60     3021           
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 45 00  3C84         23 09 03  39.1  59.2 -4.2     -81.0     0     3021   05 45 00
05 52 00  ---          23 16 04  40.4  59.4 -4.1     -82.0   420     3128   05 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

05 52 20  3C84         23 16 24  40.5  59.5 -4.1     -82.0    14     3128   05 52 20
05 55 40  ---          23 19 45  41.1  59.6 -4.0     -82.5   200     3179   05 52 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 57 48  3C84         23 21 53  41.5  59.6 -4.0     -82.8   121     3179   Stopped 
05 58 48  ---          23 22 53  41.7  59.7 -4.0     -83.0    60     3179           

 ---------- Following scan added by Sched for reference pointing ----------

05 58 54  3C84         23 22 59  41.7  59.7 -4.0     -83.0     0     3179   Stopped 
05 59 54  ---          23 23 59  41.9  59.7 -3.9     -83.1    60     3179           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 00 00  3C84         23 24 06  41.9  59.7 -3.9     -83.1     0     3179   06 00 00
06 07 00  ---          23 31 07  43.2  59.9 -3.8     -84.2   420     3287   06 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

06 07 20  3C84         23 31 27  43.3  59.9 -3.8     -84.2    14     3287   06 07 20
06 10 40  ---          23 34 47  43.9  60.0 -3.8     -84.7   200     3338   06 07 21
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 12 48  3C84         23 36 56  44.3  60.0 -3.7     -85.0   121     3338   Stopped 
06 13 48  ---          23 37 56  44.5  60.1 -3.7     -85.2    60     3338           

 ---------- Following scan added by Sched for reference pointing ----------

06 13 54  3C84         23 38 02  44.5  60.1 -3.7     -85.2     0     3338   Stopped 
06 14 54  ---          23 39 02  44.7  60.1 -3.7     -85.4    60     3338           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 15 00  3C84         23 39 08  44.7  60.1 -3.7     -85.4     0     3338   06 15 00
06 22 00  ---          23 46 09  46.0  60.2 -3.6     -86.4   420     3446   06 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

06 22 20  3C84         23 46 29  46.1  60.2 -3.6     -86.5    14     3446   06 22 20
06 25 40  ---          23 49 50  46.7  60.3 -3.5     -87.0   200     3497   06 22 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 27 25  P-TXCAM      23 51 35  31.7  39.7 -5.2     -81.2    67     3497   Stopped 
06 28 25  ---          23 52 35  31.9  39.7 -5.2     -81.4    60     3497           

 ---------- Following scan added by Sched for reference pointing ----------

06 28 31  P-TXCAM      23 52 41  31.9  39.7 -5.2     -81.4     0     3497   Stopped 
06 29 31  ---          23 53 41  32.0  39.8 -5.1     -81.6    60     3497           
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 30 00  3C111        23 54 11  35.9  62.9 -4.4     -76.6     5     3497   06 30 00
06 37 00  ---          00 01 12  37.3  63.3 -4.3     -77.4   420     3605   06 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

06 37 20  3C111        00 01 32  37.3  63.3 -4.3     -77.5    14     3605   06 37 20
06 40 40  ---          00 04 52  38.0  63.5 -4.2     -77.9   200     3656   06 37 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 42 48  3C84         00 07 00  49.9  60.4 -3.2     -89.8    97     3656   Stopped 
06 43 48  ---          00 08 01  50.1  60.4 -3.2     -89.9    60     3656           

 ---------- Following scan added by Sched for reference pointing ----------

06 43 54  3C84         00 08 07  50.1  60.4 -3.2     -89.9     0     3656   Stopped 
06 44 54  ---          00 09 07  50.3  60.4 -3.2     -90.1    60     3656           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 45 00  3C84         00 09 13  50.3  60.4 -3.2     -90.1     0     3656   06 45 00
06 52 00  ---          00 16 14  51.6  60.4 -3.1     -91.3   420     3764   06 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

06 52 20  3C84         00 16 34  51.7  60.4 -3.1     -91.4    14     3764   06 52 20
06 55 40  ---          00 19 55  52.3  60.4 -3.0     -91.9   200     3815   06 52 21
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 57 48  3C84         00 22 03  52.7  60.3 -3.0     -92.3   121     3815   Stopped 
06 58 48  ---          00 23 03  52.9  60.3 -3.0     -92.5    60     3815           

 ---------- Following scan added by Sched for reference pointing ----------

06 58 54  3C84         00 23 09  52.9  60.3 -3.0     -92.5     0     3815   Stopped 
06 59 54  ---          00 24 09  53.1  60.3 -2.9     -92.7    60     3815           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 00 00  3C84         00 24 16  53.1  60.3 -2.9     -92.7     0     3815   07 00 00
07 07 00  ---          00 31 17  54.5  60.2 -2.8     -94.0   420     3923   07 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

07 07 20  3C84         00 31 37  54.5  60.2 -2.8     -94.0    14     3923   07 07 20
07 10 40  ---          00 34 57  55.1  60.1 -2.8     -94.7   200     3974   07 07 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 12 48  3C84         00 37 05  55.5  60.0 -2.7     -95.1   121     3974   Stopped 
07 13 48  ---          00 38 06  55.7  60.0 -2.7     -95.3    60     3974           

 ---------- Following scan added by Sched for reference pointing ----------

07 13 54  3C84         00 38 12  55.7  60.0 -2.7     -95.3     0     3974   Stopped 
07 14 54  ---          00 39 12  55.9  60.0 -2.7     -95.5    60     3974           
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 15 00  3C84         00 39 18  55.9  60.0 -2.7     -95.5     0     3974   07 15 00
07 22 00  ---          00 46 19  57.3  59.7 -2.6     -96.9   420     4082   07 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

07 22 20  3C84         00 46 39  57.3  59.7 -2.6     -96.9    14     4082   07 22 20
07 25 40  ---          00 50 00  57.9  59.5 -2.5     -97.6   200     4133   07 22 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 27 48  3C84         00 52 08  58.3  59.4 -2.5     -98.1   121     4133   Stopped 
07 28 48  ---          00 53 08  58.5  59.4 -2.5     -98.3    60     4133           

 ---------- Following scan added by Sched for reference pointing ----------

07 28 54  3C84         00 53 14  58.5  59.4 -2.5     -98.3     0     4133   Stopped 
07 29 54  ---          00 54 14  58.7  59.3 -2.4     -98.5    60     4133           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 30 00  3C84         00 54 20  58.7  59.3 -2.4     -98.5     0     4133   07 30 00
07 37 00  ---          01 01 22  60.0  58.9 -2.3    -100.0   420     4241   07 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

07 37 20  3C84         01 01 42  60.1  58.9 -2.3    -100.1    14     4241   07 37 20
07 40 40  ---          01 05 02  60.7  58.6 -2.3    -100.9   200     4292   07 37 21
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 42 48  3C84         01 07 10  61.1  58.5 -2.2    -101.4   121     4292   Stopped 
07 43 48  ---          01 08 10  61.3  58.4 -2.2    -101.6    60     4292           

 ---------- Following scan added by Sched for reference pointing ----------

07 43 54  3C84         01 08 16  61.3  58.4 -2.2    -101.6     0     4292   Stopped 
07 44 54  ---          01 09 17  61.5  58.3 -2.2    -101.9    60     4292           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 45 00  3C84         01 09 23  61.5  58.3 -2.2    -101.9     0     4292   07 45 00
07 52 00  ---          01 16 24  62.8  57.7 -2.1    -103.6   420     4400   07 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

07 52 20  3C84         01 16 44  62.8  57.7 -2.1    -103.7    14     4400   07 52 20
07 55 40  ---          01 20 05  63.5  57.3 -2.0    -104.5   200     4451   07 52 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 57 22  3C84         01 21 47  63.8  57.1 -2.0    -105.0    95     4451   Stopped 
07 58 22  ---          01 22 47  63.9  57.0 -2.0    -105.2    60     4451           

 ---------- Following scan added by Sched for reference pointing ----------

07 58 28  3C84         01 22 53  64.0  57.0 -2.0    -105.3     0     4451   Stopped 
07 59 28  ---          01 23 53  64.1  56.9 -1.9    -105.5    60     4451           
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 00 00  3C111        01 24 25  53.5  66.2 -2.9     -88.3     3     4451   08 00 00
08 07 00  ---          01 31 27  54.9  66.2 -2.8     -89.3   420     4559   08 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 07 20  3C111        01 31 47  54.9  66.2 -2.8     -89.4    14     4559   08 07 20
08 10 40  ---          01 35 07  55.6  66.2 -2.7     -89.9   200     4610   08 07 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 12 48  3C84         01 37 15  66.5  55.1 -1.7    -109.4    99     4610   Stopped 
08 13 48  ---          01 38 15  66.7  55.0 -1.7    -109.7    60     4610           

 ---------- Following scan added by Sched for reference pointing ----------

08 13 54  3C84         01 38 21  66.7  54.9 -1.7    -109.7     0     4610   Stopped 
08 14 54  ---          01 39 22  66.9  54.8 -1.7    -110.1    60     4610           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 15 00  3C84         01 39 28  66.9  54.8 -1.7    -110.1     0     4610   08 15 00
08 22 00  ---          01 46 29  68.1  53.5 -1.6    -112.4   420     4718   08 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 22 20  3C84         01 46 49  68.2  53.4 -1.6    -112.5    14     4718   08 22 20
08 25 40  ---          01 50 10  68.8  52.8 -1.5    -113.7   200     4769   08 22 21
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 27 48  3C84         01 52 18  69.1  52.3 -1.5    -114.5   121     4769   Stopped 
08 28 48  ---          01 53 18  69.3  52.1 -1.5    -114.8    60     4769           

 ---------- Following scan added by Sched for reference pointing ----------

08 28 54  3C84         01 53 24  69.3  52.1 -1.5    -114.9     0     4769   Stopped 
08 29 54  ---          01 54 24  69.5  51.9 -1.4    -115.3    60     4769           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 30 00  3C84         01 54 30  69.5  51.8 -1.4    -115.3     0     4769   08 30 00
08 37 00  ---          02 01 31  70.7  50.1 -1.3    -118.1   420     4877   08 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 37 20  3C84         02 01 51  70.7  50.0 -1.3    -118.2    14     4877   08 37 20
08 40 40  ---          02 05 12  71.3  49.1 -1.3    -119.7   200     4928   08 37 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 42 48  3C84         02 07 20  71.6  48.4 -1.2    -120.6   121     4928   Stopped 
08 43 48  ---          02 08 20  71.8  48.1 -1.2    -121.1    60     4928           

 ---------- Following scan added by Sched for reference pointing ----------

08 43 54  3C84         02 08 26  71.8  48.1 -1.2    -121.1     0     4928   Stopped 
08 44 54  ---          02 09 27  72.0  47.8 -1.2    -121.6    60     4928           
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 45 00  3C84         02 09 33  72.0  47.8 -1.2    -121.6     0     4928   08 45 00
08 52 00  ---          02 16 34  73.1  45.4 -1.1    -125.1   420     5036   08 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 52 20  3C84         02 16 54  73.1  45.2 -1.1    -125.3    14     5036   08 52 20
08 55 40  ---          02 20 15  73.6  43.9 -1.0    -127.1   200     5087   08 52 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 57 48  3C84         02 22 22  74.0  43.1 -1.0    -128.3   121     5087   Stopped 
08 58 48  ---          02 23 23  74.1  42.6 -1.0    -128.8    60     5087           

 ---------- Following scan added by Sched for reference pointing ----------

08 58 54  3C84         02 23 29  74.1  42.6 -1.0    -128.9     0     5087   Stopped 
08 59 54  ---          02 24 29  74.3  42.2 -0.9    -129.5    60     5087           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 00 00  3C84         02 24 35  74.3  42.1 -0.9    -129.5     0     5087   09 00 00
09 07 00  ---          02 31 36  75.3  38.8 -0.8    -133.9   420     5195   09 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 07 20  3C84         02 31 56  75.3  38.6 -0.8    -134.1    14     5195   09 07 20
09 10 40  ---          02 35 17  75.7  36.8 -0.8    -136.4   200     5246   09 07 21
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 12 48  3C84         02 37 25  76.0  35.6 -0.7    -137.9   121     5246   Stopped 
09 13 48  ---          02 38 25  76.1  35.1 -0.7    -138.7    60     5246           

 ---------- Following scan added by Sched for reference pointing ----------

09 13 54  3C84         02 38 31  76.2  35.0 -0.7    -138.7     0     5246   Stopped 
09 14 54  ---          02 39 31  76.3  34.4 -0.7    -139.5    60     5246           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 15 00  3C84         02 39 38  76.3  34.3 -0.7    -139.5     0     5246   09 15 00
09 22 00  ---          02 46 39  77.1  29.8 -0.6    -145.1   420     5354   09 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 22 20  3C84         02 46 59  77.1  29.6 -0.6    -145.4    14     5354   09 22 20
09 25 40  ---          02 50 19  77.5  27.2 -0.5    -148.3   200     5405   09 22 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 27 55  P-IKTAU      02 52 35  66.1 140.0 -1.0     -34.4    48     5405   Stopped 
09 28 55  ---          02 53 35  66.2 140.5 -1.0     -34.0    60     5405           
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 30 00  3C111        02 54 40  71.1  61.2 -1.4    -106.7     0     5405   09 30 00
09 37 00  ---          03 01 41  72.4  59.9 -1.3    -109.1   420     5513   09 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 37 20  3C111        03 02 01  72.4  59.8 -1.3    -109.2    14     5513   09 37 20
09 40 40  ---          03 05 22  73.1  59.0 -1.2    -110.4   200     5564   09 37 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 42 48  3C84         03 07 30  78.7  12.9 -0.2    -165.2    88     5564   Stopped 
09 43 48  ---          03 08 30  78.8  11.9 -0.2    -166.2    60     5564           

 ---------- Following scan added by Sched for reference pointing ----------

09 43 54  3C84         03 08 36  78.8  11.8 -0.2    -166.4     0     5564   Stopped 
09 44 54  ---          03 09 36  78.8  10.9 -0.2    -167.4    60     5564           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 45 00  3C84         03 09 43  78.8  10.8 -0.2    -167.6     0     5564   09 45 00
09 52 00  ---          03 16 44  79.0   4.0 -0.1    -175.4   420     5672   09 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 52 20  3C84         03 17 04  79.0   3.7 -0.1    -175.8    14     5672   09 52 20
09 55 40  ---          03 20 24  79.1   0.4 -0.0    -179.5   200     5723   09 52 21
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 57 47  3C84         03 22 32  79.1  -1.7  0.0     178.0   121     5723   Stopped 
09 58 47  ---          03 23 32  79.1  -2.7  0.0     176.9    60     5723           

 ---------- Following scan added by Sched for reference pointing ----------

09 58 53  3C84         03 23 38  79.1  -2.8  0.0     176.8     0     5723   Stopped 
09 59 53  ---          03 24 39  79.0  -3.8  0.1     175.7    60     5723           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 00 00  3C84         03 24 45  79.0  -3.9  0.1     175.5     0     5723   10 00 00
10 07 00  ---          03 31 46  78.9 -10.7  0.2     167.7   420     5831   10 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 07 20  3C84         03 32 06  78.8 -11.0  0.2     167.4    14     5831   10 07 20
10 10 40  ---          03 35 27  78.7 -14.1  0.2     163.8   200     5882   10 07 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 12 47  3C84         03 37 35  78.6 -16.0  0.3     161.5   121     5882   Stopped 
10 13 47  ---          03 38 35  78.5 -16.9  0.3     160.5    60     5882           

 ---------- Following scan added by Sched for reference pointing ----------

10 13 53  3C84         03 38 41  78.5 -17.0  0.3     160.4     0     5882   Stopped 
10 14 53  ---          03 39 41  78.4 -17.9  0.3     159.3    60     5882           
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 15 00  3C84         03 39 48  78.4 -18.0  0.3     159.2     0     5882   10 15 00
10 22 00  ---          03 46 49  77.9 -23.8  0.4     152.3   420     5990   10 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 22 20  3C84         03 47 09  77.9 -24.1  0.4     152.0    14     5990   10 22 20
10 25 40  ---          03 50 29  77.5 -26.6  0.5     149.0   200     6041   10 22 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 27 48  3C84         03 52 37  77.3 -28.2  0.5     147.1   121     6041   Stopped 
10 28 48  ---          03 53 37  77.2 -28.9  0.5     146.2    60     6041           

 ---------- Following scan added by Sched for reference pointing ----------

10 28 54  3C84         03 53 43  77.2 -29.0  0.5     146.2     0     6041   Stopped 
10 29 54  ---          03 54 44  77.1 -29.7  0.6     145.3    60     6041           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 30 00  3C84         03 54 50  77.1 -29.7  0.6     145.2     0     6041   10 30 00
10 37 00  ---          04 01 51  76.3 -34.3  0.7     139.7   420     6149   10 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 37 20  3C84         04 02 11  76.3 -34.5  0.7     139.4    14     6149   10 37 20
10 40 40  ---          04 05 32  75.8 -36.4  0.7     137.0   200     6200   10 37 21
Schedule for VLBA_FD   (Code Fd )                                   Page  28
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 42 48  3C84         04 07 40  75.6 -37.6  0.8     135.5   121     6200   Stopped 
10 43 48  ---          04 08 40  75.4 -38.1  0.8     134.8    60     6200           

 ---------- Following scan added by Sched for reference pointing ----------

10 43 54  3C84         04 08 46  75.4 -38.1  0.8     134.7     0     6200   Stopped 
10 44 54  ---          04 09 46  75.3 -38.7  0.8     134.1    60     6200           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 45 00  3C84         04 09 52  75.3 -38.7  0.8     134.0     0     6200   10 45 00
10 52 00  ---          04 16 54  74.3 -42.1  0.9     129.6   420     6308   10 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 52 20  3C84         04 17 14  74.3 -42.2  0.9     129.4    14     6308   10 52 20
10 55 40  ---          04 20 34  73.8 -43.6  1.0     127.5   200     6359   10 52 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 58 41  P-RCNC       04 23 35  33.0  95.9 -3.9     -60.9    73     6359   Stopped 
10 59 41  ---          04 24 35  33.2  96.1 -3.9     -60.9    60     6359           
Schedule for VLBA_FD   (Code Fd )                                   Page  29
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 00 00  OJ287        04 24 55  28.8  82.6 -4.5     -65.3     2     6359   11 00 00
11 07 00  ---          04 31 56  30.3  83.4 -4.4     -65.5   420     6467   11 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 07 20  OJ287        04 32 16  30.4  83.4 -4.4     -65.5    14     6467   11 07 20
11 10 40  ---          04 35 37  31.1  83.8 -4.3     -65.6   200     6518   11 07 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 12 34  P-RCNC       04 37 31  35.9  98.0 -3.7     -60.5    96     6518   Stopped 
11 13 34  ---          04 38 31  36.2  98.1 -3.6     -60.4    60     6518           

 ---------- Following scan added by Sched for reference pointing ----------

11 13 40  P-RCNC       04 38 37  36.2  98.1 -3.6     -60.4     0     6518   Stopped 
11 14 40  ---          04 39 37  36.4  98.3 -3.6     -60.4    60     6518           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 15 00  OJ287        04 39 57  32.0  84.3 -4.3     -65.7     2     6518   11 15 00
11 22 00  ---          04 46 59  33.5  85.1 -4.1     -65.9   420     6626   11 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 22 20  OJ287        04 47 19  33.6  85.1 -4.1     -65.9    14     6626   11 22 20
11 25 40  ---          04 50 39  34.3  85.5 -4.1     -65.9   200     6677   11 22 21
Schedule for VLBA_FD   (Code Fd )                                   Page  30
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 28 55  3C84         04 53 54  68.4 -53.3  1.6     112.8    88     6677   Stopped 
11 29 55  ---          04 54 55  68.2 -53.5  1.6     112.5    60     6677           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 30 01  3C84         04 55 01  68.2 -53.5  1.6     112.4     0     6677   11 30 01
11 37 01  ---          05 02 02  66.9 -54.7  1.7     110.1   420     6785   11 30 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 37 21  3C84         05 02 22  66.9 -54.8  1.7     110.0    14     6785   11 37 21
11 40 41  ---          05 05 43  66.3 -55.3  1.7     109.0   200     6836   11 37 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 43 39  P-RCNC       05 08 41  42.5 102.9 -3.1     -58.9    57     6836   Stopped 
11 44 39  ---          05 09 41  42.7 103.1 -3.1     -58.8    60     6836           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 45 00  OJ287        05 10 02  38.5  87.8 -3.8     -66.2     2     6836   11 45 00
11 52 00  ---          05 17 03  40.0  88.7 -3.6     -66.3   420     6944   11 45 01
Schedule for VLBA_FD   (Code Fd )                                   Page  31
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 52 20  OJ287        05 17 24  40.0  88.7 -3.6     -66.3    14     6944   11 52 20
11 55 40  ---          05 20 44  40.8  89.1 -3.6     -66.3   200     6995   11 52 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 58 55  3C84         05 23 59  63.0 -57.6  2.1     103.9    83     6995   Stopped 
11 59 55  ---          05 25 00  62.8 -57.7  2.1     103.7    60     6995           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 00 01  3C84         05 25 06  62.8 -57.7  2.1     103.6     0     6995   12 00 01
12 07 01  ---          05 32 07  61.5 -58.3  2.2     101.9   420     7103   12 00 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 07 21  3C84         05 32 27  61.5 -58.3  2.2     101.8    14     7103   12 07 21
12 10 41  ---          05 35 48  60.9 -58.6  2.2     101.1   200     7154   12 07 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 13 37  P-RCNC       05 38 45  48.8 108.6 -2.6     -56.4    50     7154   Stopped 
12 14 37  ---          05 39 45  49.0 108.8 -2.6     -56.3    60     7154           
Schedule for VLBA_FD   (Code Fd )                                   Page  32
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 15 00  OJ287        05 40 07  44.9  91.6 -3.3     -66.3     2     7154   12 15 00
12 22 00  ---          05 47 08  46.4  92.6 -3.1     -66.2   420     7262   12 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 22 20  OJ287        05 47 28  46.5  92.6 -3.1     -66.2    14     7262   12 22 20
12 25 40  ---          05 50 49  47.2  93.1 -3.1     -66.2   200     7313   12 22 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 28 55  3C84         05 54 04  57.5 -59.6  2.6      97.1    78     7313   Stopped 
12 29 55  ---          05 55 04  57.3 -59.7  2.6      96.9    60     7313           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 30 01  3C84         05 55 11  57.3 -59.7  2.6      96.9     0     7313   12 30 01
12 37 01  ---          06 02 12  56.0 -59.9  2.7      95.5   420     7420   12 30 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 37 21  3C84         06 02 32  55.9 -60.0  2.7      95.5    14     7420   12 37 21
12 40 41  ---          06 05 52  55.3 -60.1  2.8      94.8   200     7472   12 37 22
Schedule for VLBA_FD   (Code Fd )                                   Page  33
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 43 36  P-RCNC       06 08 48  54.7 115.5 -2.1     -52.5    42     7472   Stopped 
12 44 36  ---          06 09 48  54.9 115.7 -2.1     -52.3    60     7472           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 45 00  OJ287        06 10 12  51.4  95.9 -2.8     -65.7     2     7472   12 45 00
12 52 00  ---          06 17 13  52.9  97.0 -2.6     -65.4   420     7579   12 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 52 20  OJ287        06 17 33  53.0  97.1 -2.6     -65.4    14     7579   12 52 20
12 55 40  ---          06 20 54  53.7  97.6 -2.6     -65.2   200     7631   12 52 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 58 55  3C84         06 24 09  51.9 -60.4  3.1      91.5    74     7631   Stopped 
12 59 55  ---          06 25 09  51.7 -60.4  3.1      91.4    60     7631           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 00 01  3C84         06 25 16  51.7 -60.4  3.1      91.3     0     7631   13 00 01
13 07 01  ---          06 32 17  50.4 -60.4  3.2      90.2   420     7738   13 00 02
Schedule for VLBA_FD   (Code Fd )                                   Page  34
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 07 21  3C84         06 32 37  50.3 -60.4  3.2      90.1    14     7738   13 07 21
13 10 41  ---          06 35 57  49.7 -60.4  3.3      89.5   200     7790   13 07 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 13 35  P-RCNC       06 38 52  60.4 124.4 -1.6     -46.5    35     7790   Stopped 
13 14 35  ---          06 39 52  60.5 124.7 -1.6     -46.2    60     7790           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 15 00  OJ287        06 40 17  57.8 101.1 -2.3     -64.0     0     7790   13 15 00
13 22 00  ---          06 47 18  59.3 102.5 -2.1     -63.4   420     7897   13 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 22 20  OJ287        06 47 38  59.3 102.6 -2.1     -63.4    14     7897   13 22 20
13 25 40  ---          06 50 59  60.0 103.3 -2.1     -63.1   200     7949   13 22 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 28 55  3C84         06 54 14  46.2 -60.2  3.6      86.6    71     7949   Stopped 
13 29 55  ---          06 55 14  46.1 -60.2  3.6      86.5    60     7949           
Schedule for VLBA_FD   (Code Fd )                                   Page  35
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 30 01  3C84         06 55 21  46.0 -60.2  3.6      86.5     0     7949   13 30 01
13 37 01  ---          07 02 22  44.7 -60.1  3.7      85.4   420     8056   13 30 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 37 21  3C84         07 02 42  44.7 -60.1  3.7      85.3    14     8056   13 37 21
13 40 41  ---          07 06 02  44.0 -60.0  3.8      84.8   200     8108   13 37 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 43 31  P-RCNC       07 08 53  65.3 136.4 -1.1     -37.3    23     8108   Stopped 
13 44 31  ---          07 09 53  65.4 136.9 -1.1     -36.9    60     8108           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 45 00  OJ287        07 10 22  64.1 107.8 -1.8     -60.7     0     8108   13 45 00
13 52 00  ---          07 17 23  65.5 109.8 -1.6     -59.5   420     8215   13 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 52 20  OJ287        07 17 43  65.5 109.9 -1.6     -59.5    14     8215   13 52 20
13 55 40  ---          07 21 04  66.2 110.8 -1.6     -58.9   200     8267   13 52 21
Schedule for VLBA_FD   (Code Fd )                                   Page  36
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 58 55  3C84         07 24 19  40.6 -59.5  4.1      82.2    66     8267   Stopped 
13 59 55  ---          07 25 19  40.5 -59.4  4.1      82.0    60     8267           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 00 01  3C84         07 25 25  40.4 -59.4  4.1      82.0     0     8267   14 00 01
14 07 01  ---          07 32 27  39.1 -59.2  4.2      81.0   420     8374   14 00 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 07 21  3C84         07 32 47  39.1 -59.2  4.2      81.0    14     8374   14 07 21
14 10 41  ---          07 36 07  38.5 -59.1  4.3      80.5   200     8426   14 07 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 13 27  P-RCNC       07 38 53  69.1 152.8 -0.6     -23.7     7     8426   Stopped 
14 14 27  ---          07 39 53  69.2 153.4 -0.6     -23.2    60     8426           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 15 00  OJ287        07 40 27  70.0 117.6 -1.3     -54.3     0     8426   14 15 00
14 22 00  ---          07 47 28  71.3 120.6 -1.1     -52.1   420     8533   14 15 01
Schedule for VLBA_FD   (Code Fd )                                   Page  37
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 22 20  OJ287        07 47 48  71.4 120.7 -1.1     -51.9    14     8533   14 22 20
14 25 40  ---          07 51 09  72.0 122.3 -1.1     -50.7   200     8585   14 22 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 28 55  3C84         07 54 24  35.1 301.7  4.6      77.9    59     8585   Stopped 
14 29 55  ---          07 55 24  34.9 301.8  4.6      77.8    60     8585           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 30 01  3C84         07 55 30  34.9 301.8  4.6      77.8     0     8585   14 30 01
14 37 01  ---          08 02 32  33.6 302.2  4.7      76.8   420     8692   14 30 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 37 21  3C84         08 02 52  33.6 302.2  4.7      76.8    14     8692   14 37 21
14 40 41  ---          08 06 12  33.0 302.3  4.8      76.3   200     8744   14 37 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 43 21  P-RLEO       08 08 52  60.0 124.5 -1.7     -46.3    25     8744   Stopped 
14 44 21  ---          08 09 52  60.1 124.9 -1.6     -46.0    60     8744           
Schedule for VLBA_FD   (Code Fd )                                   Page  38
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 45 00  OJ287        08 10 32  75.3 133.5 -0.8     -41.6     2     8744   14 45 00
14 52 00  ---          08 17 33  76.4 138.7 -0.6     -37.2   420     8851   14 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 52 20  OJ287        08 17 53  76.4 139.0 -0.6     -36.9    14     8851   14 52 20
14 55 40  ---          08 21 14  76.9 141.8 -0.6     -34.5   200     8903   14 52 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 58 55  3C84         08 24 29  29.7 303.4  5.1      73.8    72     8903   Stopped 
14 59 55  ---          08 25 29  29.5 303.4  5.1      73.7    60     8903           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 00 01  3C84         08 25 35  29.5 303.4  5.1      73.7     0     8903   15 00 01
15 07 01  ---          08 32 37  28.2 303.9  5.2      72.7   420     9010   15 00 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 07 21  3C84         08 32 57  28.1 303.9  5.2      72.7    14     9010   15 07 21
15 10 41  ---          08 36 17  27.5 304.1  5.3      72.2   200     9062   15 07 22
Schedule for VLBA_FD   (Code Fd )                                   Page  39
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 12 49  3C84         08 38 25  27.2 304.2  5.3      71.9   121     9062   Stopped 
15 13 49  ---          08 39 25  27.0 304.3  5.3      71.8    60     9062           

 ---------- Following scan added by Sched for reference pointing ----------

15 13 55  3C84         08 39 31  27.0 304.3  5.3      71.8     0     9062   Stopped 
15 14 55  ---          08 40 32  26.8 304.4  5.3      71.6    60     9062           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 15 01  3C84         08 40 38  26.8 304.4  5.3      71.6     0     9062   15 15 01
15 22 01  ---          08 47 39  25.5 304.9  5.4      70.7   420     9169   15 15 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 22 21  3C84         08 47 59  25.5 304.9  5.5      70.6    14     9169   15 22 21
15 25 41  ---          08 51 20  24.9 305.1  5.5      70.2   200     9220   15 22 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 27 21  P-RCNC       08 53 00  69.3 205.4  0.6      22.2     4     9220   Stopped 
15 28 21  ---          08 54 00  69.2 206.1  0.6      22.7    60     9220           

 ---------- Following scan added by Sched for reference pointing ----------

15 28 27  P-RCNC       08 54 06  69.2 206.1  0.6      22.8     0     9220   Stopped 
15 29 27  ---          08 55 06  69.1 206.8  0.6      23.3    60     9220           
Schedule for VLBA_FD   (Code Fd )                                   Page  40
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 30 01  0827+243     08 55 40  81.6 220.7  0.4      37.9     2     9220   15 30 01
15 37 01  ---          09 02 41  80.5 228.4  0.5      44.9   420     9328   15 30 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 37 21  0827+243     09 03 01  80.5 228.8  0.5      45.1    14     9328   15 37 21
15 40 41  ---          09 06 22  79.9 231.8  0.6      47.8   200     9379   15 37 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 42 49  3C84         09 08 30  21.9 306.4  5.8      67.8     6     9379   Stopped 
15 43 49  ---          09 09 30  21.7 306.5  5.8      67.7    60     9379           

 ---------- Following scan added by Sched for reference pointing ----------

15 43 55  3C84         09 09 36  21.7 306.5  5.8      67.6     0     9379   Stopped 
15 44 55  ---          09 10 37  21.5 306.5  5.8      67.5    60     9379           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 45 01  3C84         09 10 43  21.5 306.5  5.8      67.5     0     9379   15 45 01
15 52 01  ---          09 17 44  20.3 307.1  5.9      66.5   420     9487   15 45 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 52 21  3C84         09 18 04  20.2 307.1  6.0      66.5    14     9487   15 52 21
15 55 41  ---          09 21 25  19.7 307.4  6.0      66.0   200     9538   15 52 22
Schedule for VLBA_FD   (Code Fd )                                   Page  41
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 57 49  3C84         09 23 33  19.3 307.6  6.0      65.7   121     9538   Stopped 
15 58 49  ---          09 24 33  19.1 307.6  6.1      65.6    60     9538           

 ---------- Following scan added by Sched for reference pointing ----------

15 58 55  3C84         09 24 39  19.1 307.7  6.1      65.6     0     9538   Stopped 
15 59 55  ---          09 25 39  18.9 307.7  6.1      65.4    60     9538           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 00 01  3C84         09 25 45  18.9 307.7  6.1      65.4     0     9538   16 00 01
16 07 01  ---          09 32 46  17.7 308.3  6.2      64.4   420     9646   16 00 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 07 21  3C84         09 33 06  17.7 308.4  6.2      64.4    14     9646   16 07 21
16 10 41  ---          09 36 27  17.1 308.6  6.3      63.9   200     9697   16 07 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 12 49  3C84         09 38 35  16.7 308.8  6.3      63.6   121     9697   Stopped 
16 13 49  ---          09 39 35  16.6 308.9  6.3      63.5    60     9697           

 ---------- Following scan added by Sched for reference pointing ----------

16 13 55  3C84         09 39 41  16.6 308.9  6.3      63.5     0     9697   Stopped 
16 14 55  ---          09 40 41  16.4 309.0  6.3      63.3    60     9697           
Schedule for VLBA_FD   (Code Fd )                                   Page  42
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 15 01  3C84         09 40 48  16.4 309.0  6.3      63.3     0     9697   16 15 01
16 22 01  ---          09 47 49  15.2 309.6  6.5      62.3   420     9805   16 15 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 22 21  3C84         09 48 09  15.2 309.7  6.5      62.3    14     9805   16 22 21
16 25 41  ---          09 51 29  14.6 310.0  6.5      61.8   200     9856   16 22 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 27 21  P-RCNC       09 53 10  60.8 234.7  1.6      45.8     1     9856   Stopped 
16 28 21  ---          09 54 10  60.7 235.0  1.6      46.0    60     9856           

 ---------- Following scan added by Sched for reference pointing ----------

16 28 27  P-RCNC       09 54 16  60.6 235.0  1.6      46.1     0     9856   Stopped 
16 29 27  ---          09 55 17  60.5 235.4  1.6      46.3    60     9856           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 30 01  OJ287        09 55 50  72.8 235.6  1.0      49.1     1     9856   16 30 01
16 37 01  ---          10 02 51  71.5 239.0  1.1      51.7   420     9964   16 30 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 37 21  OJ287        10 03 11  71.5 239.1  1.1      51.8    14     9964   16 37 21
16 40 41  ---          10 06 32  70.8 240.6  1.2      53.0   200    10015   16 37 22
Schedule for VLBA_FD   (Code Fd )                                   Page  43
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 42 24  P-RCNC       10 08 15  58.1 239.6  1.8      49.3    70    10015   Stopped 
16 43 24  ---          10 09 15  57.9 239.9  1.9      49.5    60    10015           

 ---------- Following scan added by Sched for reference pointing ----------

16 43 30  P-RCNC       10 09 21  57.9 239.9  1.9      49.5     0    10015   Stopped 
16 44 30  ---          10 10 22  57.7 240.2  1.9      49.7    60    10015           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 45 01  0827+243     10 10 53  67.1 259.6  1.7      68.0     4    10015   16 45 01
16 52 01  ---          10 17 54  65.6 261.0  1.8      68.6   420    10123   16 45 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 52 21  0827+243     10 18 14  65.5 261.1  1.8      68.7    14    10123   16 52 21
16 55 41  ---          10 21 34  64.8 261.8  1.8      68.9   200    10174   16 52 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 57 21  P-RCNC       10 23 15  55.3 243.8  2.1      52.0    74    10174   Stopped 
16 58 21  ---          10 24 15  55.1 244.1  2.1      52.2    60    10174           

 ---------- Following scan added by Sched for reference pointing ----------

16 58 27  P-RCNC       10 24 21  55.1 244.1  2.1      52.2     0    10174   Stopped 
16 59 27  ---          10 25 21  54.9 244.4  2.1      52.4    60    10174           
Schedule for VLBA_FD   (Code Fd )                                   Page  44
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 00 01  OJ287        10 25 55  67.1 247.8  1.5      58.0     2    10174   17 00 01
17 07 01  ---          10 32 56  65.7 250.0  1.6      59.4   420    10282   17 00 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 07 21  OJ287        10 33 16  65.6 250.0  1.6      59.4    14    10282   17 07 21
17 10 41  ---          10 36 37  64.9 251.0  1.7      60.0   200    10333   17 07 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 12 25  P-RCNC       10 38 21  52.3 247.6  2.3      54.3    71    10333   Stopped 
17 13 25  ---          10 39 21  52.1 247.8  2.4      54.4    60    10333           

 ---------- Following scan added by Sched for reference pointing ----------

17 13 31  P-RCNC       10 39 27  52.1 247.8  2.4      54.4     0    10333   Stopped 
17 14 31  ---          10 40 27  51.9 248.0  2.4      54.6    60    10333           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 15 01  0827+243     10 40 58  60.7 265.2  2.2      70.0     5    10333   17 15 01
17 22 01  ---          10 47 59  59.2 266.3  2.3      70.2   420    10441   17 15 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 22 21  0827+243     10 48 19  59.1 266.3  2.3      70.2    14    10441   17 22 21
17 25 41  ---          10 51 39  58.4 266.8  2.3      70.3   200    10492   17 22 22
Schedule for VLBA_FD   (Code Fd )                                   Page  45
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 27 21  P-RCNC       10 53 20  49.3 250.9  2.6      56.1    75    10492   Stopped 
17 28 21  ---          10 54 20  49.1 251.1  2.6      56.2    60    10492           

 ---------- Following scan added by Sched for reference pointing ----------

17 28 27  P-RCNC       10 54 26  49.1 251.1  2.6      56.2     0    10492   Stopped 
17 29 27  ---          10 55 26  48.9 251.3  2.6      56.3    60    10492           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 30 01  OJ287        10 56 00  60.9 255.8  2.0      62.6     2    10492   17 30 01
17 37 01  ---          11 03 01  59.5 257.3  2.1      63.3   420    10600   17 30 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 37 21  OJ287        11 03 21  59.4 257.4  2.1      63.4    14    10600   17 37 21
17 40 41  ---          11 06 42  58.7 258.1  2.2      63.7   200    10651   17 37 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 42 25  P-RCNC       11 08 26  46.2 253.9  2.9      57.6    72    10651   Stopped 
17 43 25  ---          11 09 26  46.0 254.1  2.9      57.7    60    10651           

 ---------- Following scan added by Sched for reference pointing ----------

17 43 31  P-RCNC       11 09 32  46.0 254.1  2.9      57.7     0    10651   Stopped 
17 44 31  ---          11 10 33  45.8 254.3  2.9      57.8    60    10651           
Schedule for VLBA_FD   (Code Fd )                                   Page  46
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 45 01  0827+243     11 11 02  54.2 269.5  2.7      70.5     5    10651   17 45 01
17 52 01  ---          11 18 04  52.7 270.4  2.8      70.5   420    10759   17 45 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 52 21  0827+243     11 18 24  52.6 270.4  2.8      70.5    14    10759   17 52 21
17 55 41  ---          11 21 44  51.9 270.8  2.8      70.5   200    10810   17 52 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 57 23  P-RLEO       11 23 26  60.7 233.9  1.6      45.2    67    10810   Stopped 
17 58 23  ---          11 24 26  60.6 234.3  1.6      45.5    60    10810           

 ---------- Following scan added by Sched for reference pointing ----------

17 58 29  P-RLEO       11 24 32  60.5 234.3  1.6      45.5     0    10810   Stopped 
17 59 29  ---          11 25 33  60.4 234.7  1.6      45.7    60    10810           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 00 01  OJ287        11 26 05  54.6 261.6  2.5      65.0     5    10810   18 00 01
18 07 01  ---          11 33 06  53.1 262.8  2.6      65.3   420    10918   18 00 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 07 21  OJ287        11 33 26  53.0 262.9  2.6      65.3    14    10918   18 07 21
18 10 41  ---          11 36 47  52.3 263.4  2.7      65.5   200    10969   18 07 22
Schedule for VLBA_FD   (Code Fd )                                   Page  47
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 12 25  P-RCNC       11 38 31  39.9 259.1  3.4      59.6    73    10969   Stopped 
18 13 25  ---          11 39 32  39.7 259.3  3.4      59.7    60    10969           

 ---------- Following scan added by Sched for reference pointing ----------

18 13 31  P-RCNC       11 39 38  39.7 259.3  3.4      59.7     0    10969   Stopped 
18 14 31  ---          11 40 38  39.5 259.5  3.4      59.7    60    10969           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 15 01  0827+243     11 41 07  47.8 273.1  3.2      70.3     5    10969   18 15 01
18 22 01  ---          11 48 09  46.3 273.9  3.3      70.2   420    11077   18 15 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 22 21  0827+243     11 48 29  46.2 274.0  3.3      70.1    14    11077   18 22 21
18 25 41  ---          11 51 49  45.5 274.3  3.3      70.1   200    11128   18 22 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 27 27  P-RLEO       11 53 36  55.2 243.2  2.1      51.6    76    11128   Stopped 
18 28 27  ---          11 54 36  55.0 243.5  2.1      51.7    60    11128           

 ---------- Following scan added by Sched for reference pointing ----------

18 28 33  P-RLEO       11 54 42  55.0 243.5  2.1      51.8     0    11128   Stopped 
18 29 33  ---          11 55 42  54.8 243.8  2.1      51.9    60    11128           
Schedule for VLBA_FD   (Code Fd )                                   Page  48
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 30 01  OJ287        11 56 10  48.2 266.3  3.0      66.1     4    11128   18 30 01
18 37 01  ---          12 03 11  46.6 267.3  3.1      66.2   420    11236   18 30 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 37 21  OJ287        12 03 31  46.6 267.4  3.1      66.2    14    11236   18 37 21
18 40 41  ---          12 06 52  45.9 267.8  3.2      66.2   200    11287   18 37 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 42 26  P-RCNC       12 08 36  33.5 263.7  3.9      60.8    73    11287   Stopped 
18 43 26  ---          12 09 37  33.3 263.8  3.9      60.9    60    11287           

 ---------- Following scan added by Sched for reference pointing ----------

18 43 32  P-RCNC       12 09 43  33.3 263.8  3.9      60.9     0    11287   Stopped 
18 44 32  ---          12 10 43  33.1 264.0  3.9      60.9    60    11287           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 45 01  0827+243     12 11 12  41.3 276.4  3.7      69.5     5    11287   18 45 01
18 52 01  ---          12 18 13  39.8 277.2  3.8      69.3   420    11395   18 45 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 52 21  0827+243     12 18 34  39.7 277.2  3.8      69.3    14    11395   18 52 21
18 55 41  ---          12 21 54  39.0 277.6  3.8      69.2   200    11446   18 52 22
Schedule for VLBA_FD   (Code Fd )                                   Page  49
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 57 30  P-RLEO       12 23 44  49.2 250.3  2.6      55.7    81    11446   Stopped 
18 58 30  ---          12 24 44  49.0 250.6  2.6      55.9    60    11446           

 ---------- Following scan added by Sched for reference pointing ----------

18 58 36  P-RLEO       12 24 50  49.0 250.6  2.6      55.9     0    11446   Stopped 
18 59 36  ---          12 25 50  48.8 250.8  2.6      56.0    60    11446           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 00 01  OJ287        12 26 15  41.7 270.4  3.5      66.3     3    11446   19 00 01
19 07 01  ---          12 33 16  40.2 271.2  3.6      66.3   420    11554   19 00 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 07 21  OJ287        12 33 36  40.1 271.3  3.6      66.3    14    11554   19 07 21
19 10 41  ---          12 36 57  39.4 271.7  3.7      66.3   200    11605   19 07 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 12 28  P-RCNC       12 38 44  27.0 267.8  4.4      61.4    75    11605   Stopped 
19 13 28  ---          12 39 44  26.8 267.9  4.4      61.4    60    11605           

 ---------- Following scan added by Sched for reference pointing ----------

19 13 34  P-RCNC       12 39 50  26.8 268.0  4.4      61.4     0    11605   Stopped 
19 14 34  ---          12 40 50  26.6 268.1  4.4      61.4    60    11605           
Schedule for VLBA_FD   (Code Fd )                                   Page  50
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 15 01  0827+243     12 41 17  34.9 279.6  4.2      68.4     2    11605   19 15 01
19 22 01  ---          12 48 18  33.4 280.3  4.3      68.1   420    11713   19 15 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 22 21  0827+243     12 48 38  33.3 280.3  4.3      68.1    14    11713   19 22 21
19 25 41  ---          12 51 59  32.6 280.7  4.3      67.9   200    11764   19 22 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 27 32  P-RLEO       12 53 51  43.0 256.1  3.1      58.4    82    11764   Stopped 
19 28 32  ---          12 54 51  42.8 256.3  3.1      58.5    60    11764           

 ---------- Following scan added by Sched for reference pointing ----------

19 28 38  P-RLEO       12 54 57  42.8 256.3  3.1      58.5     0    11764   Stopped 
19 29 38  ---          12 55 57  42.6 256.5  3.1      58.6    60    11764           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 30 01  OJ287        12 56 20  35.2 274.0  4.0      66.0     0    11764   19 30 01
19 37 01  ---          13 03 21  33.7 274.8  4.1      65.9   420    11872   19 30 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 37 21  OJ287        13 03 41  33.6 274.8  4.1      65.9    14    11872   19 37 21
19 40 41  ---          13 07 01  32.9 275.2  4.2      65.8   200    11923   19 37 22
Schedule for VLBA_FD   (Code Fd )                                   Page  51
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 42 28  P-RCNC       13 08 49  20.6 271.7  4.9      61.4    75    11923   Stopped 
19 43 28  ---          13 09 49  20.4 271.8  4.9      61.4    60    11923           

 ---------- Following scan added by Sched for reference pointing ----------

19 43 34  P-RCNC       13 09 55  20.3 271.8  4.9      61.4     0    11923   Stopped 
19 44 34  ---          13 10 55  20.1 271.9  4.9      61.4    60    11923           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 45 01  0827+243     13 11 22  28.6 282.6  4.7      66.9     2    11923   19 45 01
19 52 01  ---          13 18 23  27.1 283.3  4.8      66.5   420    12031   19 45 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 52 21  0827+243     13 18 43  27.0 283.4  4.8      66.5    14    12031   19 52 21
19 55 41  ---          13 22 04  26.3 283.7  4.8      66.3   200    12082   19 52 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 57 32  P-RLEO       13 23 56  36.7 261.0  3.6      60.1    82    12082   Stopped 
19 58 32  ---          13 24 56  36.5 261.2  3.6      60.1    60    12082           

 ---------- Following scan added by Sched for reference pointing ----------

19 58 38  P-RLEO       13 25 02  36.5 261.2  3.6      60.1     0    12082   Stopped 
19 59 38  ---          13 26 02  36.2 261.4  3.6      60.2    60    12082           
Schedule for VLBA_FD   (Code Fd )                                   Page  52
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 00 01  OJ287        13 26 25  28.8 277.4  4.5      65.3     0    12082   20 00 01
20 07 01  ---          13 33 26  27.3 278.2  4.6      65.0   420    12190   20 00 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 07 21  OJ287        13 33 46  27.2 278.2  4.6      65.0    14    12190   20 07 21
20 10 41  ---          13 37 06  26.5 278.6  4.7      64.9   200    12241   20 07 22

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

20 12 26  P-RLEO       13 38 52  33.5 263.3  3.8      60.6    82    12241   Stopped 
20 13 26  ---          13 39 52  33.3 263.4  3.9      60.7    60    12241           

 ---------- Following scan added by Sched for reference pointing ----------

20 13 32  P-RLEO       13 39 58  33.3 263.4  3.9      60.7     0    12241   Stopped 
20 14 32  ---          13 40 58  33.1 263.6  3.9      60.7    60    12241           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 15 01  0827+243     13 41 27  22.3 285.7  5.2      65.2     0    12241   20 15 01
20 22 01  ---          13 48 28  20.8 286.4  5.3      64.7   420    12349   20 15 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 22 21  0827+243     13 48 48  20.8 286.5  5.3      64.7    14    12349   20 22 21
20 25 41  ---          13 52 09  20.1 286.8  5.3      64.5   200    12400   20 22 22
Schedule for VLBA_FD   (Code Fd )                                   Page  53
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

20 27 32  P-RLEO       13 54 01  30.3 265.4  4.1      61.0    83    12400   Stopped 
20 28 32  ---          13 55 01  30.0 265.5  4.1      61.0    60    12400           

 ---------- Following scan added by Sched for reference pointing ----------

20 28 38  P-RLEO       13 55 07  30.0 265.5  4.1      61.0     0    12400   Stopped 
20 29 38  ---          13 56 07  29.8 265.7  4.1      61.1    60    12400           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 30 01  OJ287        13 56 30  22.4 280.8  5.0      64.1     0    12400   20 30 01
20 36 01  ---          14 02 31  21.1 281.4  5.1      63.9   360    12492   20 30 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 36 21  OJ287        14 02 51  21.1 281.5  5.1      63.8    14    12492   20 36 21
20 39 41  ---          14 06 11  20.4 281.8  5.2      63.7   200    12544   20 36 22

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 40 00  2013+370     14 06 30  16.2 416.0 -6.2     -63.6   -84    12544   20 41 24
20 43 00  ---          14 09 31  16.8 416.2 -6.1     -63.9    96    12568   20 40 01

20 44 20  CYG-A        14 10 51  21.3 414.3 -5.8     -67.3    63    12568   20 44 20
20 51 20  ---          14 17 52  22.6 414.8 -5.7     -68.3   420    12676   20 44 21
Schedule for VLBA_FD   (Code Fd )                                   Page  54
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

20 56 27  P-UHER       14 22 59  59.7 105.6 -2.1     -61.1    78    12676   Stopped 
20 57 27  ---          14 24 00  59.9 105.8 -2.0     -61.0    60    12676           

 ---------- Following scan added by Sched for reference pointing ----------

20 57 33  P-UHER       14 24 06  60.0 105.9 -2.0     -61.0     0    12676   Stopped 
20 58 33  ---          14 25 06  60.2 106.1 -2.0     -60.9    60    12676           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

21 00 00  2013+370     14 26 33  19.9  57.7 -5.8     -66.0     0    12676   21 00 00
21 03 00  ---          14 29 34  20.4  58.0 -5.8     -66.4   180    12722   21 00 01

21 04 20  CYG-A        14 30 54  24.9  55.8 -5.5     -70.0    64    12722   21 04 20
21 11 20  ---          14 37 55  26.1  56.3 -5.4     -70.9   420    12830   21 04 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

21 16 26  P-UHER       14 43 02  63.8 110.7 -1.7     -58.3   225    12830   Stopped 
21 17 26  ---          14 44 02  64.0 111.0 -1.7     -58.1    60    12830           

 ---------- Following scan added by Sched for reference pointing ----------

21 17 32  P-UHER       14 44 08  64.1 111.0 -1.7     -58.1     0    12830   Stopped 
21 18 32  ---          14 45 08  64.3 111.3 -1.7     -57.9    60    12830           
Schedule for VLBA_FD   (Code Fd )                                   Page  55
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

21 20 00  2013+370     14 46 37  23.5  59.4 -5.5     -68.5     0    12830   21 20 00
21 23 00  ---          14 49 37  24.1  59.6 -5.4     -68.8   180    12876   21 20 01

21 24 20  CYG-A        14 50 57  28.5  57.1 -5.2     -72.7    64    12876   21 24 20
21 31 20  ---          14 57 59  29.7  57.6 -5.0     -73.6   420    12984   21 24 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

21 36 52  P-VXSGR      15 03 31  20.9 134.2 -3.1     -41.8   270    12984   Stopped 
21 37 52  ---          15 04 31  21.1 134.4 -3.1     -41.6    60    12984           

 ---------- Following scan added by Sched for reference pointing ----------

21 37 58  P-VXSGR      15 04 37  21.1 134.4 -3.1     -41.6     0    12984   Stopped 
21 38 58  ---          15 05 38  21.2 134.6 -3.1     -41.5    60    12984           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

21 40 00  2013+370     15 06 40  27.3  60.9 -5.2     -70.8     2    12984   21 40 00
21 43 00  ---          15 09 41  27.9  61.2 -5.1     -71.2   180    13030   21 40 01

21 44 10  CYG-A        15 10 51  32.1  58.3 -4.8     -75.3    54    13030   21 44 10
21 51 10  ---          15 17 52  33.4  58.7 -4.7     -76.2   420    13137   21 44 11

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

21 56 50  P-VXSGR      15 23 33  23.9 138.0 -2.8     -38.5   277    13137   Stopped 
21 57 50  ---          15 24 33  24.1 138.2 -2.7     -38.3    60    13137           
Schedule for VLBA_FD   (Code Fd )                                   Page  56
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

21 57 56  P-VXSGR      15 24 39  24.1 138.2 -2.7     -38.3     0    13137   Stopped 
21 58 56  ---          15 25 39  24.2 138.4 -2.7     -38.1    60    13137           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

22 00 00  2013+370     15 26 43  31.1  62.3 -4.8     -73.2     2    13137   22 00 00
22 03 00  ---          15 29 44  31.7  62.5 -4.8     -73.5   180    13184   22 00 01

22 04 10  CYG-A        15 30 54  35.8  59.4 -4.5     -78.0    54    13184   22 04 10
22 11 10  ---          15 37 55  37.1  59.7 -4.4     -78.9   420    13291   22 04 11

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

22 17 02  P-RRAQL      15 43 48  21.4 105.8 -4.2     -55.9   311    13291   Stopped 
22 18 02  ---          15 44 48  21.6 106.0 -4.2     -55.9    60    13291           

 ---------- Following scan added by Sched for reference pointing ----------

22 18 08  P-RRAQL      15 44 54  21.7 106.0 -4.2     -55.9     0    13291   Stopped 
22 19 08  ---          15 45 54  21.9 106.1 -4.2     -55.8    60    13291           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

22 20 00  2013+370     15 46 47  34.9  63.6 -4.5     -75.5    14    13291   22 20 00
22 23 00  ---          15 49 47  35.5  63.8 -4.4     -75.9   180    13337   22 20 01

22 24 10  CYG-A        15 50 57  39.5  60.3 -4.2     -80.7    54    13337   22 24 10
22 31 10  ---          15 57 58  40.8  60.6 -4.0     -81.7   420    13445   22 24 11
Schedule for VLBA_FD   (Code Fd )                                   Page  57
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

22 37 00  P-RRAQL      16 03 50  25.5 108.9 -3.9     -54.5   309    13445   Stopped 
22 38 00  ---          16 04 50  25.7 109.1 -3.9     -54.4    60    13445           

 ---------- Following scan added by Sched for reference pointing ----------

22 38 06  P-RRAQL      16 04 56  25.8 109.1 -3.9     -54.4     0    13445   Stopped 
22 39 06  ---          16 05 56  26.0 109.3 -3.9     -54.4    60    13445           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

22 40 00  2013+370     16 06 50  38.8  64.8 -4.2     -77.9    14    13445   22 40 00
22 43 00  ---          16 09 50  39.4  64.9 -4.1     -78.2   180    13491   22 40 01

22 44 10  CYG-A        16 11 01  43.3  61.0 -3.8     -83.6    55    13491   22 44 10
22 51 10  ---          16 18 02  44.6  61.2 -3.7     -84.6   420    13599   22 44 11

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

22 56 59  P-RRAQL      16 23 51  29.6 112.3 -3.6     -52.8   305    13599   Stopped 
22 57 59  ---          16 24 51  29.8 112.4 -3.6     -52.7    60    13599           

 ---------- Following scan added by Sched for reference pointing ----------

22 58 05  P-RRAQL      16 24 57  29.8 112.5 -3.6     -52.7     0    13599   Stopped 
22 59 05  ---          16 25 58  30.0 112.6 -3.5     -52.6    60    13599           
Schedule for VLBA_FD   (Code Fd )                                   Page  58
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

23 00 00  BLLAC        16 26 53  24.1  53.6 -5.6     -69.7     6    13599   23 00 00
23 07 00  ---          16 33 54  25.3  54.1 -5.5     -70.6   420    13707   23 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

23 07 20  BLLAC        16 34 14  25.4  54.2 -5.5     -70.7    14    13707   23 07 20
23 10 40  ---          16 37 35  26.0  54.4 -5.4     -71.2   200    13758   23 07 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

23 16 57  P-RRAQL      16 43 53  33.5 115.9 -3.2     -50.7   326    13758   Stopped 
23 17 57  ---          16 44 53  33.7 116.1 -3.2     -50.6    60    13758           

 ---------- Following scan added by Sched for reference pointing ----------

23 18 03  P-RRAQL      16 44 59  33.7 116.1 -3.2     -50.6     0    13758   Stopped 
23 19 03  ---          16 45 59  33.9 116.3 -3.2     -50.5    60    13758           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

23 20 00  2013+370     16 46 56  46.7  66.6 -3.5     -82.7    14    13758   23 20 00
23 23 00  ---          16 49 57  47.3  66.7 -3.4     -83.1   180    13804   23 20 01

23 24 00  CYG-A        16 50 57  50.8  61.6 -3.2     -89.6    45    13804   23 24 00
23 31 00  ---          16 57 58  52.1  61.6 -3.0     -90.7   420    13912   23 24 01
Schedule for VLBA_FD   (Code Fd )                                   Page  59
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  26 Sep 2014   Day 269 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

23 36 55  P-RRAQL      17 03 54  37.3 119.9 -2.9     -48.3   306    13912   Stopped 
23 37 55  ---          17 04 54  37.5 120.1 -2.9     -48.1    60    13912           

 ---------- Following scan added by Sched for reference pointing ----------

23 38 01  P-RRAQL      17 05 00  37.5 120.1 -2.9     -48.1     0    13912   Stopped 
23 39 01  ---          17 06 00  37.7 120.3 -2.9     -48.0    60    13912           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

23 40 00  2013+370     17 07 00  50.6  67.2 -3.2     -85.3    14    13912   23 40 00
23 43 00  ---          17 10 00  51.2  67.3 -3.1     -85.7   180    13958   23 40 01

23 44 00  CYG-A        17 11 00  54.6  61.5 -2.8     -93.0    46    13958   23 44 00
23 51 00  ---          17 18 02  55.9  61.4 -2.7     -94.3   420    14066   23 44 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

23 56 52  P-RRAQL      17 23 55  41.0 124.3 -2.6     -45.3   301    14066   Stopped 
23 57 52  ---          17 24 55  41.1 124.5 -2.6     -45.2    60    14066           

 ---------- Following scan added by Sched for reference pointing ----------

23 57 58  P-RRAQL      17 25 01  41.2 124.6 -2.6     -45.1     0    14066   Stopped 
23 58 58  ---          17 26 01  41.3 124.8 -2.5     -45.0    60    14066           
Schedule for VLBA_FD   (Code Fd )                                   Page  60
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

00 00 01  2013+370     17 27 04  54.6  67.6 -2.8     -88.0    14    14066   00 00 01
00 03 01  ---          17 30 05  55.2  67.7 -2.8     -88.4   180    14112   00 00 02

00 04 01  CYG-A        17 31 05  58.4  60.9 -2.5     -96.8    46    14112   00 04 01
00 11 01  ---          17 38 06  59.7  60.6 -2.4     -98.2   420    14219   00 04 02

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

00 16 48  P-RRAQL      17 43 54  44.4 129.2 -2.2     -41.8   291    14219   Stopped 
00 17 48  ---          17 44 54  44.6 129.5 -2.2     -41.6    60    14219           

 ---------- Following scan added by Sched for reference pointing ----------

00 17 54  P-RRAQL      17 45 00  44.6 129.5 -2.2     -41.6     0    14219   Stopped 
00 18 54  ---          17 46 00  44.8 129.8 -2.2     -41.4    60    14219           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

00 20 00  2013+370     17 47 06  58.6  67.7 -2.5     -91.0    14    14219   00 20 00
00 23 00  ---          17 50 07  59.2  67.7 -2.4     -91.4   180    14266   00 20 01

00 24 00  CYG-A        17 51 07  62.1  59.7 -2.1    -101.1    47    14266   00 24 00
00 31 00  ---          17 58 08  63.4  59.1 -2.0    -102.7   420    14373   00 24 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

00 36 43  P-RRAQL      18 03 52  47.6 134.7 -1.9     -37.7   283    14373   Stopped 
00 37 43  ---          18 04 53  47.8 135.0 -1.9     -37.5    60    14373           
Schedule for VLBA_FD   (Code Fd )                                   Page  61
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

00 37 49  P-RRAQL      18 04 59  47.8 135.1 -1.9     -37.4     0    14373   Stopped 
00 38 49  ---          18 05 59  47.9 135.4 -1.9     -37.2    60    14373           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

00 40 00  2013+370     18 07 10  62.6  67.3 -2.1     -94.3    14    14373   00 40 00
00 43 00  ---          18 10 10  63.2  67.2 -2.1     -94.9   180    14419   00 40 01

00 44 00  CYG-A        18 11 10  65.8  57.7 -1.8    -106.2    45    14419   00 44 00
00 51 00  ---          18 18 11  67.1  56.7 -1.7    -108.2   420    14527   00 44 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

00 56 59  3C454.3      18 24 11  27.2  86.5 -4.5     -63.4   271    14527   Stopped 
00 57 59  ---          18 25 12  27.4  86.6 -4.5     -63.5    60    14527           

 ---------- Following scan added by Sched for reference pointing ----------

00 58 05  3C454.3      18 25 18  27.4  86.6 -4.5     -63.5     0    14527   Stopped 
00 59 05  ---          18 26 18  27.6  86.8 -4.5     -63.5    60    14527           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 00 00  BLLAC        18 27 13  45.8  59.1 -3.6     -87.0    11    14527   01 00 00
01 07 00  ---          18 34 14  47.1  59.1 -3.5     -88.2   420    14635   01 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

01 07 20  BLLAC        18 34 34  47.1  59.1 -3.5     -88.2    14    14635   01 07 20
01 10 40  ---          18 37 55  47.8  59.2 -3.4     -88.8   200    14686   01 07 21
Schedule for VLBA_FD   (Code Fd )                                   Page  62
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 16 32  P-RRAQL      18 43 48  53.0 147.9 -1.2     -27.2   283    14686   Stopped 
01 17 32  ---          18 44 48  53.1 148.3 -1.2     -26.9    60    14686           

 ---------- Following scan added by Sched for reference pointing ----------

01 17 38  P-RRAQL      18 44 54  53.1 148.4 -1.2     -26.9     0    14686   Stopped 
01 18 38  ---          18 45 54  53.2 148.7 -1.2     -26.5    60    14686           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 20 00  2013+370     18 47 16  70.5  64.3 -1.5    -103.2    14    14686   01 20 00
01 23 00  ---          18 50 17  71.1  63.8 -1.4    -104.1   180    14732   01 20 01

01 24 00  CYG-A        18 51 17  72.8  49.2 -1.1    -120.7    42    14732   01 24 00
01 31 00  ---          18 58 18  73.9  46.7 -1.0    -124.3   420    14840   01 24 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 36 27  P-RRAQL      19 03 46  55.0 155.7 -0.9     -20.7   243    14840   Stopped 
01 37 27  ---          19 04 46  55.1 156.1 -0.9     -20.4    60    14840           

 ---------- Following scan added by Sched for reference pointing ----------

01 37 33  P-RRAQL      19 04 52  55.1 156.2 -0.9     -20.4     0    14840   Stopped 
01 38 33  ---          19 05 52  55.2 156.6 -0.9     -20.0    60    14840           
Schedule for VLBA_FD   (Code Fd )                                   Page  63
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 40 00  2013+370     19 07 19  74.3  60.5 -1.1    -109.8    11    14840   01 40 00
01 43 00  ---          19 10 20  74.9  59.7 -1.1    -111.1   180    14886   01 40 01

01 44 00  CYG-A        19 11 20  75.9  40.8 -0.8    -132.0    39    14886   01 44 00
01 51 00  ---          19 18 21  76.8  36.9 -0.7    -137.0   420    14994   01 44 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 56 24  3C454.3      19 23 46  40.0  94.2 -3.5     -63.4   242    14994   Stopped 
01 57 24  ---          19 24 46  40.2  94.3 -3.5     -63.3    60    14994           

 ---------- Following scan added by Sched for reference pointing ----------

01 57 30  3C454.3      19 24 52  40.2  94.3 -3.5     -63.3     0    14994   Stopped 
01 58 30  ---          19 25 53  40.4  94.5 -3.5     -63.3    60    14994           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 00 00  2013+370     19 27 23  78.0  53.5 -0.8    -119.7     8    14994   02 00 00
02 03 00  ---          19 30 23  78.5  52.0 -0.8    -121.6   180    15040   02 00 01

02 04 00  CYG-A        19 31 23  78.3  27.8 -0.5    -148.1    35    15040   02 04 00
02 11 00  ---          19 38 25  79.0  21.8 -0.4    -155.0   420    15148   02 04 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 16 24  3C454.3      19 43 50  44.3  97.1 -3.2     -62.8   246    15148   Stopped 
02 17 24  ---          19 44 50  44.5  97.3 -3.2     -62.7    60    15148           
Schedule for VLBA_FD   (Code Fd )                                   Page  64
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

02 17 30  3C454.3      19 44 56  44.5  97.3 -3.2     -62.7     0    15148   Stopped 
02 18 30  ---          19 45 56  44.7  97.4 -3.1     -62.7    60    15148           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 20 00  2013+370     19 47 26  81.1  40.0 -0.5    -136.0    10    15148   02 20 00
02 23 00  ---          19 50 27  81.5  37.1 -0.4    -139.3   180    15194   02 20 01

02 24 00  CYG-A        19 51 27  79.7   9.1 -0.1    -169.6    33    15194   02 24 00
02 31 00  ---          19 58 28  79.8   1.7 -0.0    -178.1   420    15302   02 24 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 36 20  3C454.3      20 03 49  48.5 100.3 -2.8     -61.8   243    15302   Stopped 
02 37 20  ---          20 04 49  48.7 100.5 -2.8     -61.8    60    15302           

 ---------- Following scan added by Sched for reference pointing ----------

02 37 26  3C454.3      20 04 55  48.8 100.5 -2.8     -61.8     0    15302   Stopped 
02 38 26  ---          20 05 56  49.0 100.7 -2.8     -61.7    60    15302           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 40 00  2013+370     20 07 29  83.2  14.5 -0.1    -164.3    18    15302   02 40 00
02 43 00  ---          20 10 30  83.3   9.5 -0.1    -169.7   180    15348   02 40 01

02 44 00  CYG-A        20 11 30  79.6 -12.1  0.2     166.2    37    15348   02 44 00
02 51 00  ---          20 18 31  79.2 -19.0  0.3     158.3   420    15455   02 44 01
Schedule for VLBA_FD   (Code Fd )                                   Page  65
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 56 55  3C454.3      20 24 27  52.9 104.1 -2.5     -60.3   260    15455   Stopped 
02 57 55  ---          20 25 27  53.1 104.3 -2.5     -60.3    60    15455           

 ---------- Following scan added by Sched for reference pointing ----------

02 58 01  3C454.3      20 25 33  53.1 104.3 -2.5     -60.3     0    15455   Stopped 
02 59 01  ---          20 26 33  53.3 104.5 -2.5     -60.2    60    15455           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 00 00  BLLAC        20 27 33  67.6  51.9 -1.6    -113.7    14    15455   03 00 00
03 07 00  ---          20 34 34  68.8  50.4 -1.5    -116.2   420    15563   03 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

03 07 20  BLLAC        20 34 54  68.8  50.3 -1.5    -116.4    14    15563   03 07 20
03 10 40  ---          20 38 14  69.4  49.5 -1.4    -117.6   200    15614   03 07 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

03 15 44  P-GYAQL      20 43 19  49.8 200.4  0.9      17.6   190    15614   Stopped 
03 16 44  ---          20 44 20  49.7 200.7  0.9      17.9    60    15614           

 ---------- Following scan added by Sched for reference pointing ----------

03 16 50  P-GYAQL      20 44 26  49.7 200.8  0.9      17.9     0    15614   Stopped 
03 17 50  ---          20 45 26  49.6 201.1  0.9      18.2    60    15614           
Schedule for VLBA_FD   (Code Fd )                                   Page  66
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 20 00  2013+370     20 47 36  80.7 317.4  0.5     133.0    39    15614   03 20 00
03 23 00  ---          20 50 36  80.3 315.0  0.6     130.2   180    15660   03 20 01

03 24 00  CYG-A        20 51 37  75.4 317.7  0.9     130.1    43    15660   03 24 00
03 31 00  ---          20 58 38  74.4 314.6  1.0     125.9   420    15768   03 24 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

03 36 15  P-GYAQL      21 03 53  48.0 207.6  1.2      23.7   230    15768   Stopped 
03 37 15  ---          21 04 53  47.9 208.0  1.2      24.0    60    15768           

 ---------- Following scan added by Sched for reference pointing ----------

03 37 21  P-GYAQL      21 04 59  47.9 208.0  1.2      24.0     0    15768   Stopped 
03 38 21  ---          21 06 00  47.8 208.3  1.3      24.3    60    15768           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 40 00  2013+370     21 07 39  77.4 305.2  0.9     117.9    22    15768   03 40 00
03 43 00  ---          21 10 40  76.9 303.9  0.9     116.3   180    15814   03 40 01

03 44 10  CYG-A        21 11 50  72.3 309.9  1.2     119.3    53    15814   03 44 10
03 51 10  ---          21 18 51  71.1 307.9  1.3     116.3   420    15922   03 44 11

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

03 56 32  P-RRAQL      21 24 14  51.6 216.1  1.4      30.5   248    15922   Stopped 
03 57 32  ---          21 25 15  51.5 216.4  1.4      30.8    60    15922           
Schedule for VLBA_FD   (Code Fd )                                   Page  67
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

03 57 38  P-RRAQL      21 25 21  51.5 216.5  1.4      30.8     0    15922   Stopped 
03 58 38  ---          21 26 21  51.4 216.8  1.5      31.1    60    15922           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 00 00  2013+370     21 27 42  73.8 298.8  1.2     108.7    15    15922   04 00 00
04 03 00  ---          21 30 43  73.2 298.1  1.2     107.6   180    15968   04 00 01

04 03 40  CYG-A        21 31 23  68.9 305.1  1.5     111.6    24    15968   04 03 40
04 10 40  ---          21 38 24  67.7 303.8  1.6     109.3   420    16076   04 03 41

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 16 44  P-RRAQL      21 44 29  48.9 222.7  1.8      35.7   297    16076   Stopped 
04 17 44  ---          21 45 29  48.7 223.0  1.8      36.0    60    16076           

 ---------- Following scan added by Sched for reference pointing ----------

04 17 50  P-RRAQL      21 45 35  48.7 223.1  1.8      36.0     0    16076   Stopped 
04 18 50  ---          21 46 35  48.5 223.4  1.8      36.2    60    16076           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 20 00  2013+370     21 47 46  69.9 295.4  1.5     102.4    11    16076   04 20 00
04 23 00  ---          21 50 46  69.3 295.0  1.6     101.6   180    16122   04 20 01

04 23 40  CYG-A        21 51 26  65.3 302.0  1.9     105.4    24    16122   04 23 40
04 30 40  ---          21 58 28  64.1 301.2  2.0     103.6   420    16230   04 23 41
Schedule for VLBA_FD   (Code Fd )                                   Page  68
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 36 47  P-RRAQL      22 04 36  45.8 228.6  2.1      40.2   307    16230   Stopped 
04 37 47  ---          22 05 36  45.6 228.8  2.1      40.4    60    16230           

 ---------- Following scan added by Sched for reference pointing ----------

04 37 53  P-RRAQL      22 05 42  45.6 228.9  2.1      40.4     0    16230   Stopped 
04 38 53  ---          22 06 42  45.4 229.1  2.1      40.6    60    16230           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 40 00  2013+370     22 07 49  66.0 293.5  1.9      97.7    13    16230   04 40 00
04 43 00  ---          22 10 50  65.4 293.3  1.9      97.0   180    16276   04 40 01

04 43 40  CYG-A        22 11 30  61.6 300.1  2.2     100.5    25    16276   04 43 40
04 50 40  ---          22 18 31  60.3 299.6  2.3      98.9   420    16384   04 43 41

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 56 03  P-RRAQL      22 23 54  42.5 233.6  2.4      43.8   267    16384   Stopped 
04 57 03  ---          22 24 55  42.4 233.8  2.4      44.0    60    16384           

 ---------- Following scan added by Sched for reference pointing ----------

04 57 09  P-RRAQL      22 25 01  42.3 233.8  2.4      44.0     0    16384   Stopped 
04 58 09  ---          22 26 01  42.2 234.1  2.5      44.2    60    16384           
Schedule for VLBA_FD   (Code Fd )                                   Page  69
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 00 00  BLLAC        22 27 52  77.3 339.0  0.4     155.3    28    16384   05 00 00
05 07 00  ---          22 34 53  76.7 333.9  0.5     149.2   420    16491   05 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

05 07 20  BLLAC        22 35 14  76.7 333.7  0.5     148.9    14    16491   05 07 20
05 10 40  ---          22 38 34  76.3 331.4  0.6     146.2   200    16543   05 07 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 16 49  P-RRAQL      22 44 44  38.8 238.4  2.8      47.1   289    16543   Stopped 
05 17 49  ---          22 45 45  38.6 238.6  2.8      47.3    60    16543           

 ---------- Following scan added by Sched for reference pointing ----------

05 17 55  P-RRAQL      22 45 51  38.6 238.6  2.8      47.3     0    16543   Stopped 
05 18 55  ---          22 46 51  38.4 238.8  2.8      47.4    60    16543           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 20 00  2013+370     22 47 56  58.0 292.3  2.5      90.5    18    16543   05 20 00
05 23 00  ---          22 50 56  57.4 292.3  2.6      90.1   180    16589   05 20 01

05 23 40  CYG-A        22 51 36  54.1 298.5  2.9      92.5    26    16589   05 23 40
05 30 40  ---          22 58 37  52.8 298.4  3.0      91.3   420    16696   05 23 41
Schedule for VLBA_FD   (Code Fd )                                   Page  70
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 36 50  P-RRAQL      23 04 48  35.1 242.5  3.1      49.8   321    16696   Stopped 
05 37 50  ---          23 05 48  34.9 242.7  3.1      49.9    60    16696           

 ---------- Following scan added by Sched for reference pointing ----------

05 37 56  P-RRAQL      23 05 54  34.9 242.7  3.1      49.9     0    16696   Stopped 
05 38 56  ---          23 06 55  34.7 242.9  3.1      50.1    60    16696           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 40 00  2013+370     23 07 59  54.0 292.4  2.9      87.6    18    16696   05 40 00
05 43 00  ---          23 10 59  53.4 292.5  2.9      87.2   180    16743   05 40 01

05 43 40  CYG-A        23 11 40  50.3 298.4  3.2      89.2    26    16743   05 43 40
05 50 40  ---          23 18 41  49.0 298.4  3.3      88.1   420    16850   05 43 41

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 56 50  P-RRAQL      23 24 52  31.2 246.3  3.4      52.0   324    16850   Stopped 
05 57 50  ---          23 25 52  31.0 246.5  3.5      52.1    60    16850           

 ---------- Following scan added by Sched for reference pointing ----------

05 57 56  P-RRAQL      23 25 58  31.0 246.5  3.5      52.1     0    16850   Stopped 
05 58 56  ---          23 26 58  30.8 246.7  3.5      52.2    60    16850           
Schedule for VLBA_FD   (Code Fd )                                   Page  71
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 00 00  2013+370     23 28 02  50.1 292.8  3.2      84.9    18    16850   06 00 00
06 03 00  ---          23 31 03  49.5 292.9  3.2      84.5   180    16896   06 00 01

06 03 40  CYG-A        23 31 43  46.5 298.6  3.5      86.1    26    16896   06 03 40
06 10 40  ---          23 38 44  45.2 298.7  3.6      85.0   420    17004   06 03 41

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 16 38  3C454.3      23 44 43  71.6 221.2  0.8      36.2   293    17004   Stopped 
06 17 38  ---          23 45 43  71.5 221.8  0.8      36.7    60    17004           

 ---------- Following scan added by Sched for reference pointing ----------

06 17 44  3C454.3      23 45 49  71.5 221.9  0.9      36.8     0    17004   Stopped 
06 18 44  ---          23 46 49  71.3 222.5  0.9      37.3    60    17004           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 20 00  2013+370     23 48 05  46.1 293.5  3.5      82.3    18    17004   06 20 00
06 23 00  ---          23 51 06  45.5 293.6  3.6      82.0   180    17050   06 20 01

06 23 40  CYG-A        23 51 46  42.7 299.1  3.9      83.2    27    17050   06 23 40
06 30 40  ---          23 58 47  41.4 299.3  4.0      82.2   420    17158   06 23 41

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 36 48  3C454.3      00 04 57  68.4 232.0  1.2      45.0   306    17158   Stopped 
06 37 48  ---          00 05 57  68.3 232.5  1.2      45.3    60    17158           
Schedule for VLBA_FD   (Code Fd )                                   Page  72
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

06 37 54  3C454.3      00 06 03  68.3 232.5  1.2      45.3     0    17158   Stopped 
06 38 54  ---          00 07 03  68.1 233.0  1.2      45.7    60    17158           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 40 00  2013+370     00 08 09  42.2 294.4  3.9      79.9     7    17158   06 40 00
06 43 00  ---          00 11 09  41.6 294.5  3.9      79.5   180    17204   06 40 01

06 43 40  CYG-A        00 11 49  39.0 299.8  4.2      80.4    27    17204   06 43 40
06 50 40  ---          00 18 51  37.7 300.1  4.3      79.4   420    17312   06 43 41

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 56 49  3C454.3      00 25 01  64.9 240.2  1.5      51.0   306    17312   Stopped 
06 57 49  ---          00 26 01  64.7 240.5  1.5      51.3    60    17312           

 ---------- Following scan added by Sched for reference pointing ----------

06 57 55  3C454.3      00 26 07  64.7 240.6  1.5      51.3     0    17312   Stopped 
06 58 55  ---          00 27 07  64.5 240.9  1.5      51.5    60    17312           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 00 00  BLLAC        00 28 12  58.9 302.3  2.4     100.2    13    17312   07 00 00
07 07 00  ---          00 35 13  57.6 301.9  2.5      98.6   420    17419   07 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

07 07 20  BLLAC        00 35 33  57.6 301.9  2.5      98.6    14    17419   07 07 20
07 10 40  ---          00 38 54  57.0 301.7  2.6      97.9   200    17471   07 07 21
Schedule for VLBA_FD   (Code Fd )                                   Page  73
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 16 54  3C454.3      00 45 09  61.0 246.5  1.8      55.3   326    17471   Stopped 
07 17 54  ---          00 46 09  60.8 246.8  1.9      55.5    60    17471           

 ---------- Following scan added by Sched for reference pointing ----------

07 18 00  3C454.3      00 46 15  60.8 246.9  1.9      55.5     0    17471   Stopped 
07 19 00  ---          00 47 16  60.6 247.1  1.9      55.7    60    17471           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 20 00  2013+370     00 48 15  34.4 296.6  4.5      75.2     0    17471   07 20 00
07 23 00  ---          00 51 16  33.8 296.7  4.6      74.8   180    17517   07 20 01

07 23 40  CYG-A        00 51 56  31.6 301.8  4.9      74.9    28    17517   07 23 40
07 30 40  ---          00 58 57  30.3 302.2  5.0      74.0   420    17625   07 23 41

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 36 55  3C454.3      01 05 13  57.0 251.7  2.2      58.3   312    17625   Stopped 
07 37 55  ---          01 06 13  56.7 251.9  2.2      58.4    60    17625           

 ---------- Following scan added by Sched for reference pointing ----------

07 38 01  3C454.3      01 06 19  56.7 251.9  2.2      58.4     0    17625   Stopped 
07 39 01  ---          01 07 19  56.5 252.1  2.2      58.5    60    17625           
Schedule for VLBA_FD   (Code Fd )                                   Page  74
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 40 00  2013+370     01 08 19  30.5 297.9  4.9      72.8     0    17625   07 40 00
07 43 00  ---          01 11 19  30.0 298.1  4.9      72.5   180    17671   07 40 01

07 43 40  CYG-A        01 11 59  27.9 303.0  5.2      72.3    28    17671   07 43 40
07 50 40  ---          01 19 00  26.7 303.5  5.3      71.3   420    17778   07 43 41

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 56 55  3C454.3      01 25 16  52.8 255.9  2.5      60.4   313    17778   Stopped 
07 57 55  ---          01 26 17  52.6 256.1  2.5      60.5    60    17778           

 ---------- Following scan added by Sched for reference pointing ----------

07 58 01  3C454.3      01 26 23  52.6 256.1  2.5      60.5     0    17778   Stopped 
07 59 01  ---          01 27 23  52.4 256.3  2.5      60.6    60    17778           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 00 00  2013+370     01 28 22  26.7 299.3  5.2      70.5     1    17778   08 00 00
08 03 00  ---          01 31 22  26.2 299.5  5.3      70.1   180    17825   08 00 01

08 03 40  CYG-A        01 32 03  24.3 304.4  5.5      69.6    29    17825   08 03 40
08 10 40  ---          01 39 04  23.1 304.9  5.7      68.7   420    17932   08 03 41

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 12 11  3C454.3      01 40 34  49.6 258.8  2.8      61.5    30    17932   Stopped 
08 13 11  ---          01 41 35  49.4 259.0  2.8      61.6    60    17932           
Schedule for VLBA_FD   (Code Fd )                                   Page  75
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

08 13 17  3C454.3      01 41 41  49.4 259.0  2.8      61.6     0    17932   Stopped 
08 14 17  ---          01 42 41  49.2 259.1  2.8      61.7    60    17932           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 15 00  BLLAC        01 43 24  45.1 301.0  3.7      86.4     6    17932   08 15 00
08 22 00  ---          01 50 26  43.8 301.1  3.8      85.3   420    18040   08 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 22 20  BLLAC        01 50 46  43.7 301.1  3.8      85.3    14    18040   08 22 20
08 25 40  ---          01 54 06  43.1 301.2  3.8      84.8   200    18091   08 22 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 27 13  3C454.3      01 55 39  46.4 261.3  3.0      62.4    57    18091   Stopped 
08 28 13  ---          01 56 39  46.2 261.5  3.0      62.4    60    18091           

 ---------- Following scan added by Sched for reference pointing ----------

08 28 19  3C454.3      01 56 45  46.2 261.5  3.0      62.4     0    18091   Stopped 
08 29 19  ---          01 57 46  46.0 261.7  3.1      62.5    60    18091           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 30 00  BLLAC        01 58 27  42.3 301.3  3.9      84.1     5    18091   08 30 00
08 36 40  ---          02 05 08  41.1 301.5  4.0      83.1   400    18194   08 30 01
Schedule for VLBA_FD   (Code Fd )                                   Page  76
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 37 00  BLLAC        02 05 28  41.0 301.5  4.0      83.0    14    18194   08 37 00
08 40 20  ---          02 08 49  40.4 301.6  4.1      82.6   200    18245   08 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 42 15  3C454.3      02 10 44  43.2 263.7  3.3      63.0    80    18245   Stopped 
08 43 15  ---          02 11 44  43.0 263.8  3.3      63.0    60    18245           

 ---------- Following scan added by Sched for reference pointing ----------

08 43 21  3C454.3      02 11 50  43.0 263.8  3.3      63.0     0    18245   Stopped 
08 44 21  ---          02 12 50  42.7 264.0  3.3      63.0    60    18245           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 45 00  BLLAC        02 13 29  39.5 301.8  4.2      81.9     4    18245   08 45 00
08 51 40  ---          02 20 10  38.3 302.0  4.3      80.9   400    18348   08 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 52 00  BLLAC        02 20 30  38.3 302.0  4.3      80.8    14    18348   08 52 00
08 55 20  ---          02 23 51  37.6 302.1  4.3      80.4   200    18399   08 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page  77
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 57 17  3C454.3      02 25 48  40.0 265.8  3.5      63.4    83    18399   Stopped 
08 58 17  ---          02 26 48  39.7 266.0  3.5      63.4    60    18399           

 ---------- Following scan added by Sched for reference pointing ----------

08 58 23  3C454.3      02 26 54  39.7 266.0  3.5      63.4     0    18399   Stopped 
08 59 23  ---          02 27 54  39.5 266.1  3.6      63.4    60    18399           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 00 00  BLLAC        02 28 32  36.8 302.3  4.4      79.7     4    18399   09 00 00
09 06 40  ---          02 35 13  35.6 302.6  4.5      78.7   400    18502   09 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 07 00  BLLAC        02 35 33  35.5 302.6  4.5      78.7    14    18502   09 07 00
09 10 20  ---          02 38 53  34.9 302.8  4.6      78.2   200    18553   09 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 12 19  3C454.3      02 40 53  36.7 267.9  3.8      63.6    86    18553   Stopped 
09 13 19  ---          02 41 53  36.5 268.0  3.8      63.6    60    18553           

 ---------- Following scan added by Sched for reference pointing ----------

09 13 25  3C454.3      02 41 59  36.5 268.1  3.8      63.6     0    18553   Stopped 
09 14 25  ---          02 42 59  36.3 268.2  3.8      63.6    60    18553           
Schedule for VLBA_FD   (Code Fd )                                   Page  78
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 15 01  BLLAC        02 43 35  34.1 303.0  4.7      77.5     3    18553   09 15 01
09 21 41  ---          02 50 16  32.9 303.3  4.8      76.6   400    18655   09 15 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 22 01  BLLAC        02 50 36  32.8 303.4  4.8      76.5    14    18655   09 22 01
09 25 21  ---          02 53 57  32.2 303.5  4.8      76.1   200    18707   09 22 02

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 27 51  P-ORINEW2    02 56 27  37.6 126.3 -2.7     -44.1    16    18707   Stopped 
09 28 51  =ORIIRC2     02 57 27  37.7 126.6 -2.6     -43.9    60    18707           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 30 00  4C39.25      02 58 37  13.6  52.5 -6.5     -61.4     8    18707   09 30 00
09 36 40  ---          03 05 18  14.7  53.1 -6.4     -62.3   400    18809   09 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 37 00  4C39.25      03 05 38  14.8  53.2 -6.4     -62.3    14    18809   09 37 00
09 40 20  ---          03 08 58  15.4  53.5 -6.3     -62.8   200    18860   09 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page  79
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 41 43  P-ORINEW2    03 10 22  39.9 129.6 -2.4     -41.8    21    18860   Stopped 
09 42 43  =ORIIRC2     03 11 22  40.1 129.8 -2.4     -41.6    60    18860           

 ---------- Following scan added by Sched for reference pointing ----------

09 42 49  P-ORINEW2    03 11 28  40.1 129.9 -2.4     -41.6     0    18860   Stopped 
09 43 49  =ORIIRC2     03 12 28  40.3 130.1 -2.4     -41.4    60    18860           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 45 00  4C39.25      03 13 39  16.2  53.9 -6.2     -63.4     9    18860   09 45 00
09 51 40  ---          03 20 20  17.4  54.5 -6.1     -64.3   400    18963   09 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 52 00  4C39.25      03 20 40  17.4  54.5 -6.1     -64.3    14    18963   09 52 00
09 55 20  ---          03 24 01  18.0  54.8 -6.1     -64.8   200    19014   09 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 57 59  P-ORINEW2    03 26 40  42.6 133.7 -2.2     -38.6    95    19014   Stopped 
09 58 59  =ORIIRC2     03 27 41  42.7 134.0 -2.1     -38.4    60    19014           
Schedule for VLBA_FD   (Code Fd )                                   Page  80
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 00 00  OJ287        03 28 42  16.9  76.3 -5.4     -62.9     2    19014   10 00 00
10 06 40  ---          03 35 23  18.3  77.1 -5.3     -63.2   400    19117   10 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 07 00  OJ287        03 35 43  18.4  77.1 -5.3     -63.2    14    19117   10 07 00
10 10 20  ---          03 39 03  19.1  77.5 -5.3     -63.4   200    19168   10 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 12 18  P-RCNC       03 41 02  23.8  90.2 -4.6     -61.5   102    19168   Stopped 
10 13 18  ---          03 42 02  24.0  90.4 -4.6     -61.5    60    19168           

 ---------- Following scan added by Sched for reference pointing ----------

10 13 24  P-RCNC       03 42 08  24.1  90.4 -4.6     -61.5     0    19168   Stopped 
10 14 24  ---          03 43 08  24.3  90.5 -4.6     -61.5    60    19168           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 15 00  4C39.25      03 43 44  21.5  56.5 -5.7     -67.3     3    19168   10 15 00
10 21 40  ---          03 50 25  22.7  57.0 -5.6     -68.2   400    19271   10 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 22 00  4C39.25      03 50 45  22.8  57.0 -5.6     -68.2    14    19271   10 22 00
10 25 20  ---          03 54 06  23.4  57.3 -5.6     -68.6   200    19322   10 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page  81
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 27 17  P-RCNC       03 56 04  27.1  92.2 -4.4     -61.4    85    19322   Stopped 
10 28 17  ---          03 57 04  27.3  92.3 -4.3     -61.4    60    19322           

 ---------- Following scan added by Sched for reference pointing ----------

10 28 23  P-RCNC       03 57 10  27.3  92.3 -4.3     -61.4     0    19322   Stopped 
10 29 23  ---          03 58 10  27.5  92.5 -4.3     -61.4    60    19322           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 30 00  4C39.25      03 58 47  24.2  57.6 -5.5     -69.2     4    19322   10 30 00
10 36 40  ---          04 05 28  25.4  58.1 -5.4     -70.1   400    19425   10 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 37 00  4C39.25      04 05 48  25.5  58.2 -5.4     -70.1    14    19425   10 37 00
10 40 20  ---          04 09 08  26.1  58.4 -5.3     -70.5   200    19476   10 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 42 35  P-RLMI       04 11 23  21.4  61.7 -5.6     -66.8   117    19476   Stopped 
10 43 35  ---          04 12 24  21.6  61.8 -5.6     -66.9    60    19476           

 ---------- Following scan added by Sched for reference pointing ----------

10 43 41  P-RLMI       04 12 30  21.6  61.8 -5.6     -66.9     0    19476   Stopped 
10 44 41  ---          04 13 30  21.8  61.9 -5.5     -67.0    60    19476           
Schedule for VLBA_FD   (Code Fd )                                   Page  82
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 45 00  4C39.25      04 13 49  27.0  58.7 -5.2     -71.1     1    19476   10 45 00
10 51 40  ---          04 20 30  28.2  59.2 -5.1     -71.9   400    19578   10 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 52 00  4C39.25      04 20 50  28.3  59.2 -5.1     -72.0    14    19578   10 52 00
10 55 20  ---          04 24 11  28.9  59.5 -5.1     -72.4   200    19630   10 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 57 34  P-RCNC       04 26 25  33.6  96.4 -3.8     -60.8   100    19630   Stopped 
10 58 34  ---          04 27 26  33.8  96.5 -3.8     -60.8    60    19630           

 ---------- Following scan added by Sched for reference pointing ----------

10 58 40  P-RCNC       04 27 32  33.8  96.5 -3.8     -60.8     0    19630   Stopped 
10 59 40  ---          04 28 32  34.0  96.7 -3.8     -60.8    60    19630           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 00 00  OJ287        04 28 51  29.6  83.0 -4.4     -65.4     2    19630   11 00 00
11 06 40  ---          04 35 33  31.1  83.8 -4.3     -65.6   400    19732   11 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 07 00  OJ287        04 35 53  31.1  83.8 -4.3     -65.6    14    19732   11 07 00
11 10 20  ---          04 39 13  31.8  84.2 -4.3     -65.7   200    19784   11 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page  83
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 12 35  P-RLMI       04 41 28  27.2  64.2 -5.1     -70.0   113    19784   Stopped 
11 13 35  ---          04 42 29  27.4  64.3 -5.1     -70.1    60    19784           

 ---------- Following scan added by Sched for reference pointing ----------

11 13 41  P-RLMI       04 42 35  27.4  64.3 -5.1     -70.1     0    19784   Stopped 
11 14 41  ---          04 43 35  27.6  64.4 -5.0     -70.2    60    19784           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 15 00  4C39.25      04 43 54  32.6  60.7 -4.7     -74.9     1    19784   11 15 00
11 21 40  ---          04 50 35  33.8  61.1 -4.6     -75.7   400    19886   11 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 22 00  4C39.25      04 50 55  33.9  61.1 -4.6     -75.7    14    19886   11 22 00
11 25 20  ---          04 54 16  34.5  61.3 -4.6     -76.2   200    19937   11 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 27 35  P-RLMI       04 56 31  30.1  65.4 -4.8     -71.6   118    19937   Stopped 
11 28 35  ---          04 57 31  30.3  65.5 -4.8     -71.7    60    19937           

 ---------- Following scan added by Sched for reference pointing ----------

11 28 41  P-RLMI       04 57 37  30.3  65.5 -4.8     -71.7     0    19937   Stopped 
11 29 41  ---          04 58 37  30.5  65.6 -4.8     -71.8    60    19937           
Schedule for VLBA_FD   (Code Fd )                                   Page  84
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 30 00  4C39.25      04 58 56  35.4  61.6 -4.5     -76.7     1    19937   11 30 00
11 36 40  ---          05 05 38  36.7  61.9 -4.4     -77.6   400    20040   11 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 37 00  4C39.25      05 05 58  36.7  62.0 -4.4     -77.6    14    20040   11 37 00
11 40 20  ---          05 09 18  37.4  62.1 -4.3     -78.1   200    20091   11 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 42 35  P-RLMI       05 11 34  33.1  66.5 -4.6     -73.1   118    20091   Stopped 
11 43 35  ---          05 12 34  33.3  66.6 -4.6     -73.2    60    20091           

 ---------- Following scan added by Sched for reference pointing ----------

11 43 41  P-RLMI       05 12 40  33.3  66.6 -4.6     -73.2     0    20091   Stopped 
11 44 41  ---          05 13 40  33.5  66.7 -4.5     -73.3    60    20091           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 45 00  4C39.25      05 13 59  38.2  62.4 -4.2     -78.6     2    20091   11 45 00
11 51 40  ---          05 20 40  39.5  62.7 -4.1     -79.5   400    20194   11 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 52 00  4C39.25      05 21 00  39.6  62.7 -4.1     -79.5    14    20194   11 52 00
11 55 20  ---          05 24 21  40.2  62.8 -4.1     -80.0   200    20245   11 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page  85
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 57 32  P-RCNC       05 26 33  46.2 106.2 -2.8     -57.6    94    20245   Stopped 
11 58 32  ---          05 27 33  46.5 106.4 -2.8     -57.5    60    20245           

 ---------- Following scan added by Sched for reference pointing ----------

11 58 38  P-RCNC       05 27 39  46.5 106.4 -2.8     -57.5     0    20245   Stopped 
11 59 38  ---          05 28 39  46.7 106.6 -2.8     -57.4    60    20245           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 00 00  OJ287        05 29 01  42.5  90.2 -3.4     -66.3     2    20245   12 00 00
12 06 40  ---          05 35 42  44.0  91.0 -3.3     -66.3   400    20348   12 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 07 00  OJ287        05 36 02  44.1  91.1 -3.3     -66.3    14    20348   12 07 00
12 10 20  ---          05 39 23  44.8  91.5 -3.3     -66.3   200    20399   12 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 12 35  P-RLMI       05 41 39  39.1  68.5 -4.1     -76.2   111    20399   Stopped 
12 13 35  ---          05 42 39  39.3  68.6 -4.1     -76.3    60    20399           

 ---------- Following scan added by Sched for reference pointing ----------

12 13 41  P-RLMI       05 42 45  39.3  68.6 -4.1     -76.3     0    20399   Stopped 
12 14 41  ---          05 43 45  39.5  68.7 -4.0     -76.4    60    20399           
Schedule for VLBA_FD   (Code Fd )                                   Page  86
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 15 00  4C39.25      05 44 04  44.0  63.6 -3.7     -82.5     2    20399   12 15 00
12 21 40  ---          05 50 45  45.3  63.8 -3.6     -83.4   400    20501   12 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 22 00  4C39.25      05 51 05  45.4  63.9 -3.6     -83.5    14    20501   12 22 00
12 25 20  ---          05 54 26  46.0  64.0 -3.6     -83.9   200    20553   12 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 27 35  P-RLMI       05 56 41  42.1  69.5 -3.8     -77.7   119    20553   Stopped 
12 28 35  ---          05 57 41  42.3  69.5 -3.8     -77.8    60    20553           

 ---------- Following scan added by Sched for reference pointing ----------

12 28 41  P-RLMI       05 57 47  42.3  69.5 -3.8     -77.8     0    20553   Stopped 
12 29 41  ---          05 58 47  42.5  69.6 -3.8     -77.9    60    20553           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 30 00  4C39.25      05 59 06  46.9  64.1 -3.5     -84.6     2    20553   12 30 00
12 36 40  ---          06 05 47  48.2  64.3 -3.4     -85.5   400    20655   12 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 37 00  4C39.25      06 06 07  48.3  64.3 -3.4     -85.6    14    20655   12 37 00
12 40 20  ---          06 09 28  48.9  64.3 -3.3     -86.0   200    20707   12 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page  87
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 42 35  P-RLMI       06 11 44  45.1  70.3 -3.6     -79.2   119    20707   Stopped 
12 43 35  ---          06 12 44  45.3  70.4 -3.6     -79.3    60    20707           

 ---------- Following scan added by Sched for reference pointing ----------

12 43 41  P-RLMI       06 12 50  45.3  70.4 -3.6     -79.3     0    20707   Stopped 
12 44 41  ---          06 13 50  45.5  70.4 -3.5     -79.4    60    20707           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 45 00  4C39.25      06 14 09  49.8  64.4 -3.2     -86.7     2    20707   12 45 00
12 51 40  ---          06 20 50  51.1  64.5 -3.1     -87.7   400    20809   12 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 52 00  4C39.25      06 21 10  51.2  64.5 -3.1     -87.7    14    20809   12 52 00
12 55 20  ---          06 24 30  51.8  64.6 -3.1     -88.2   200    20860   12 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 57 29  P-RCNC       06 26 40  58.1 120.5 -1.8     -49.2    82    20860   Stopped 
12 58 29  ---          06 27 40  58.3 120.8 -1.8     -49.0    60    20860           

 ---------- Following scan added by Sched for reference pointing ----------

12 58 35  P-RCNC       06 27 46  58.3 120.8 -1.8     -49.0     0    20860   Stopped 
12 59 35  ---          06 28 46  58.5 121.1 -1.8     -48.8    60    20860           
Schedule for VLBA_FD   (Code Fd )                                   Page  88
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 00 00  OJ287        06 29 11  55.4  99.0 -2.4     -64.8     1    20860   13 00 00
13 06 40  ---          06 35 52  56.9 100.3 -2.3     -64.3   400    20963   13 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 07 00  OJ287        06 36 12  56.9 100.3 -2.3     -64.3    14    20963   13 07 00
13 10 20  ---          06 39 33  57.6 101.0 -2.3     -64.1   200    21014   13 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 12 35  P-RLMI       06 41 49  51.2  71.8 -3.1     -82.4   107    21014   Stopped 
13 13 35  ---          06 42 49  51.4  71.8 -3.1     -82.5    60    21014           

 ---------- Following scan added by Sched for reference pointing ----------

13 13 41  P-RLMI       06 42 55  51.5  71.9 -3.1     -82.5     0    21014   Stopped 
13 14 41  ---          06 43 55  51.7  71.9 -3.0     -82.6    60    21014           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 15 00  4C39.25      06 44 14  55.7  64.6 -2.7     -91.3     3    21014   13 15 00
13 21 40  ---          06 50 55  57.0  64.5 -2.6     -92.4   400    21117   13 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 22 00  4C39.25      06 51 15  57.0  64.5 -2.6     -92.5    14    21117   13 22 00
13 25 20  ---          06 54 35  57.7  64.5 -2.6     -93.0   200    21168   13 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page  89
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 27 35  P-RLMI       06 56 51  54.3  72.4 -2.8     -84.0   120    21168   Stopped 
13 28 35  ---          06 57 51  54.5  72.4 -2.8     -84.1    60    21168           

 ---------- Following scan added by Sched for reference pointing ----------

13 28 41  P-RLMI       06 57 57  54.5  72.5 -2.8     -84.1     0    21168   Stopped 
13 29 41  ---          06 58 57  54.7  72.5 -2.8     -84.2    60    21168           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 30 00  4C39.25      06 59 16  58.6  64.4 -2.5     -93.9     3    21168   13 30 00
13 36 40  ---          07 05 57  59.9  64.2 -2.4     -95.1   400    21271   13 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 37 00  4C39.25      07 06 17  60.0  64.1 -2.4     -95.1    14    21271   13 37 00
13 40 20  ---          07 09 38  60.6  64.0 -2.3     -95.8   200    21322   13 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 42 35  P-RLMI       07 11 53  57.4  72.9 -2.6     -85.7   120    21322   Stopped 
13 43 35  ---          07 12 54  57.6  72.9 -2.6     -85.8    60    21322           

 ---------- Following scan added by Sched for reference pointing ----------

13 43 41  P-RLMI       07 13 00  57.6  72.9 -2.6     -85.9     0    21322   Stopped 
13 44 41  ---          07 14 00  57.8  73.0 -2.5     -86.0    60    21322           
Schedule for VLBA_FD   (Code Fd )                                   Page  90
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 45 00  4C39.25      07 14 19  61.5  63.8 -2.2     -96.7     4    21322   13 45 00
13 51 40  ---          07 21 00  62.8  63.5 -2.1     -98.1   400    21425   13 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 52 00  4C39.25      07 21 20  62.9  63.4 -2.1     -98.1    14    21425   13 52 00
13 55 20  ---          07 24 40  63.5  63.2 -2.1     -98.8   200    21476   13 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 57 22  P-RCNC       07 26 43  67.7 145.5 -0.8     -29.8    56    21476   Stopped 
13 58 22  ---          07 27 43  67.8 146.1 -0.8     -29.3    60    21476           

 ---------- Following scan added by Sched for reference pointing ----------

13 58 28  P-RCNC       07 27 49  67.8 146.2 -0.8     -29.3     0    21476   Stopped 
13 59 28  ---          07 28 49  68.0 146.7 -0.8     -28.8    60    21476           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 00 00  OJ287        07 29 21  67.9 113.5 -1.4     -57.1     0    21476   14 00 00
14 06 40  ---          07 36 02  69.2 115.9 -1.3     -55.5   400    21578   14 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 07 00  OJ287        07 36 22  69.2 116.0 -1.3     -55.4    14    21578   14 07 00
14 10 20  ---          07 39 43  69.9 117.3 -1.3     -54.5   200    21630   14 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page  91
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 12 35  P-RLMI       07 41 58  63.6  73.4 -2.1     -89.5    96    21630   Stopped 
14 13 35  ---          07 42 58  63.8  73.4 -2.1     -89.7    60    21630           

 ---------- Following scan added by Sched for reference pointing ----------

14 13 41  P-RLMI       07 43 04  63.8  73.4 -2.1     -89.7     0    21630   Stopped 
14 14 41  ---          07 44 04  64.0  73.4 -2.0     -89.8    60    21630           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 15 00  4C39.25      07 44 24  67.3  61.4 -1.7    -103.6     3    21630   14 15 00
14 21 40  ---          07 51 05  68.5  60.6 -1.6    -105.4   400    21732   14 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 22 00  4C39.25      07 51 25  68.6  60.5 -1.6    -105.5    14    21732   14 22 00
14 25 20  ---          07 54 45  69.2  60.0 -1.6    -106.5   200    21784   14 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 27 34  P-RLMI       07 57 00  66.7  73.3 -1.8     -91.7   117    21784   Stopped 
14 28 34  ---          07 58 00  66.9  73.3 -1.8     -91.9    60    21784           

 ---------- Following scan added by Sched for reference pointing ----------

14 28 40  P-RLMI       07 58 06  66.9  73.3 -1.8     -91.9     0    21784   Stopped 
14 29 40  ---          07 59 06  67.1  73.3 -1.8     -92.1    60    21784           
Schedule for VLBA_FD   (Code Fd )                                   Page  92
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 30 00  4C39.25      07 59 26  70.1  59.3 -1.5    -108.0     2    21784   14 30 00
14 36 40  ---          08 06 07  71.3  58.0 -1.4    -110.2   400    21886   14 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 37 00  4C39.25      08 06 27  71.4  57.9 -1.4    -110.4    14    21886   14 37 00
14 40 20  ---          08 09 48  72.0  57.2 -1.3    -111.6   200    21937   14 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 42 34  P-RLMI       08 12 02  69.8  72.9 -1.6     -94.3   115    21937   Stopped 
14 43 34  ---          08 13 02  70.0  72.9 -1.6     -94.5    60    21937           

 ---------- Following scan added by Sched for reference pointing ----------

14 43 40  P-RLMI       08 13 08  70.0  72.9 -1.6     -94.5     0    21937   Stopped 
14 44 40  ---          08 14 08  70.2  72.8 -1.5     -94.7    60    21937           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 45 00  4C39.25      08 14 28  72.8  56.0 -1.2    -113.4     0    21937   14 45 00
14 51 40  ---          08 21 10  74.0  54.1 -1.1    -116.3   400    22040   14 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 52 00  4C39.25      08 21 30  74.1  54.0 -1.1    -116.5    14    22040   14 52 00
14 55 20  ---          08 24 50  74.6  52.9 -1.1    -118.0   200    22091   14 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page  93
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 57 19  P-RCNC       08 26 50  70.9 187.1  0.2       6.2    16    22091   Stopped 
14 58 19  ---          08 27 50  70.9 187.8  0.2       6.9    60    22091           

 ---------- Following scan added by Sched for reference pointing ----------

14 58 25  P-RCNC       08 27 56  70.9 187.9  0.2       7.0     0    22091   Stopped 
14 59 25  ---          08 28 56  70.9 188.7  0.2       7.6    60    22091           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 00 01  OJ287        08 29 32  77.9 149.4 -0.4     -27.8     0    22091   15 00 01
15 06 41  ---          08 36 13  78.5 156.4 -0.3     -21.5   400    22194   15 00 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 07 01  OJ287        08 36 33  78.6 156.8 -0.3     -21.2    14    22194   15 07 01
15 10 21  ---          08 39 54  78.8 160.5 -0.3     -17.8   200    22245   15 07 02

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 12 14  P-RLMI       08 41 47  75.9  70.1 -1.1    -101.1    41    22245   Stopped 
15 13 14  ---          08 42 48  76.1  70.0 -1.1    -101.4    60    22245           

 ---------- Following scan added by Sched for reference pointing ----------

15 13 20  P-RLMI       08 42 54  76.1  69.9 -1.1    -101.5     0    22245   Stopped 
15 14 20  ---          08 43 54  76.3  69.8 -1.0    -101.8    60    22245           
Schedule for VLBA_FD   (Code Fd )                                   Page  94
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 15 00  4C39.25      08 44 33  77.8  43.9 -0.7    -129.9    13    22245   15 15 00
15 21 40  ---          08 51 14  78.8  39.6 -0.6    -135.2   400    22348   15 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 22 00  4C39.25      08 51 35  78.8  39.3 -0.6    -135.5    14    22348   15 22 00
15 25 20  ---          08 54 55  79.3  36.8 -0.6    -138.4   200    22399   15 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 27 07  P-RLMI       08 56 43  78.9  66.8 -0.8    -106.5    78    22399   Stopped 
15 28 07  ---          08 57 43  79.1  66.4 -0.8    -107.0    60    22399           

 ---------- Following scan added by Sched for reference pointing ----------

15 28 13  P-RLMI       08 57 49  79.1  66.4 -0.8    -107.0     0    22399   Stopped 
15 29 13  ---          08 58 49  79.3  66.1 -0.8    -107.5    60    22399           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 30 00  4C39.25      08 59 36  79.8  32.9 -0.5    -143.0    16    22399   15 30 00
15 36 40  ---          09 06 17  80.6  26.6 -0.4    -150.3   400    22501   15 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 37 00  4C39.25      09 06 37  80.6  26.2 -0.4    -150.7    14    22501   15 37 00
15 40 20  ---          09 09 58  80.9  22.6 -0.3    -154.8   200    22553   15 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page  95
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 42 14  P-RLMI       09 11 52  81.8  60.1 -0.6    -115.2    79    22553   Stopped 
15 43 14  ---          09 12 52  82.0  59.5 -0.6    -116.0    60    22553           

 ---------- Following scan added by Sched for reference pointing ----------

15 43 20  P-RLMI       09 12 58  82.0  59.4 -0.6    -116.1     0    22553   Stopped 
15 44 20  ---          09 13 58  82.2  58.8 -0.5    -116.9    60    22553           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 45 00  4C39.25      09 14 38  81.2  17.2 -0.2    -160.9     3    22553   15 45 00
15 51 40  ---          09 21 19  81.6   8.8 -0.1    -170.2   400    22655   15 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 52 00  4C39.25      09 21 39  81.6   8.4 -0.1    -170.7    14    22655   15 52 00
15 55 20  ---          09 25 00  81.6   3.9 -0.0    -175.6   200    22707   15 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 56 48  P-RLMI       09 26 28  84.3  46.5 -0.3    -130.8    49    22707   Stopped 
15 57 48  ---          09 27 28  84.5  45.1 -0.3    -132.3    60    22707           

 ---------- Following scan added by Sched for reference pointing ----------

15 57 54  P-RLMI       09 27 34  84.5  45.0 -0.3    -132.5     0    22707   Stopped 
15 58 54  ---          09 28 35  84.6  43.5 -0.3    -134.1    60    22707           
Schedule for VLBA_FD   (Code Fd )                                   Page  96
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 00 00  4C39.25      09 29 41  81.7  -2.3  0.0     177.4    26    22707   16 00 00
16 06 40  ---          09 36 22  81.5 -11.1  0.1     167.7   400    22809   16 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 07 00  4C39.25      09 36 42  81.5 -11.5  0.1     167.2    14    22809   16 07 00
16 10 20  ---          09 40 02  81.3 -15.7  0.2     162.5   200    22860   16 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 12 19  P-TXCAM      09 42 02  36.0 -40.2  4.7      87.3    22    22860   Stopped 
16 13 19  ---          09 43 02  35.8 -40.2  4.7      87.1    60    22860           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 15 00  4C39.25      09 44 43  81.0 -21.3  0.3     156.3     4    22860   16 15 00
16 21 40  ---          09 51 24  80.4 -28.4  0.4     148.3   400    22963   16 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 22 00  4C39.25      09 51 44  80.3 -28.7  0.4     147.9    14    22963   16 22 00
16 25 20  ---          09 55 05  80.0 -31.9  0.5     144.3   200    23014   16 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page  97
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 27 19  P-TXCAM      09 57 04  33.9 -40.0  4.9      84.2    20    23014   Stopped 
16 28 19  ---          09 58 04  33.7 -40.0  4.9      84.0    60    23014           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 30 00  4C39.25      09 59 46  79.4 -35.9  0.5     139.6     4    23014   16 30 00
16 36 40  ---          10 06 27  78.5 -40.8  0.6     133.7   400    23117   16 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 37 00  4C39.25      10 06 47  78.5 -41.0  0.6     133.4    14    23117   16 37 00
16 40 20  ---          10 10 07  78.0 -43.2  0.7     130.8   200    23168   16 37 01

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 45 00  OJ287        10 14 48  69.3 244.0  1.3      55.4    68    23168   16 45 00
16 51 40  ---          10 21 29  68.0 246.4  1.4      57.0   400    23271   16 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 52 00  OJ287        10 21 49  67.9 246.5  1.4      57.1    14    23271   16 52 00
16 55 20  ---          10 25 10  67.2 247.6  1.5      57.8   200    23322   16 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page  98
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 57 25  P-RLMI       10 27 15  80.6 296.6  0.7     111.1    81    23322   Stopped 
16 58 25  ---          10 28 15  80.4 296.1  0.7     110.5    60    23322           

 ---------- Following scan added by Sched for reference pointing ----------

16 58 31  P-RLMI       10 28 21  80.4 296.1  0.7     110.4     0    23322   Stopped 
16 59 31  ---          10 29 21  80.2 295.7  0.7     109.9    60    23322           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 00 00  4C39.25      10 29 51  74.8 307.5  1.0     118.6    11    23322   17 00 00
17 06 40  ---          10 36 32  73.7 305.4  1.1     115.5   400    23425   17 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 07 00  4C39.25      10 36 52  73.6 305.3  1.1     115.3    14    23425   17 07 00
17 10 20  ---          10 40 12  73.0 304.3  1.2     113.9   200    23476   17 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 12 20  P-RCNC       10 42 13  51.5 248.5  2.4      54.8    70    23476   Stopped 
17 13 20  ---          10 43 13  51.3 248.7  2.4      54.9    60    23476           

 ---------- Following scan added by Sched for reference pointing ----------

17 13 26  P-RCNC       10 43 19  51.3 248.7  2.4      54.9     0    23476   Stopped 
17 14 26  ---          10 44 19  51.1 248.9  2.4      55.1    60    23476           
Schedule for VLBA_FD   (Code Fd )                                   Page  99
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 15 00  OJ287        10 44 53  63.2 253.2  1.8      61.3     2    23476   17 15 00
17 21 40  ---          10 51 34  61.9 254.8  1.9      62.1   400    23578   17 15 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 27 33  P-RLMI       10 57 28  74.6 289.0  1.2      99.3   318    23578   Stopped 
17 28 33  ---          10 58 28  74.4 288.8  1.2      99.1    60    23578           

 ---------- Following scan added by Sched for reference pointing ----------

17 28 39  P-RLMI       10 58 34  74.4 288.8  1.2      99.1     0    23578   Stopped 
17 29 39  ---          10 59 34  74.1 288.7  1.2      98.8    60    23578           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 30 00  4C39.25      10 59 56  69.4 300.2  1.5     106.9     4    23578   17 30 00
17 36 40  ---          11 06 37  68.2 299.2  1.6     104.9   400    23681   17 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 37 00  4C39.25      11 06 57  68.1 299.1  1.6     104.8    14    23681   17 37 00
17 40 20  ---          11 10 17  67.5 298.7  1.7     103.9   200    23732   17 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 100
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 42 51  P-RHYA       11 12 48  23.7 139.7 -2.7     -37.3    30    23732   Stopped 
17 43 51  ---          11 13 49  23.8 139.9 -2.7     -37.1    60    23732           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 45 01  3C345        11 14 59  24.6  56.9 -5.5     -69.7     3    23732   17 45 01
17 51 41  ---          11 21 40  25.8  57.3 -5.4     -70.5   400    23835   17 45 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 52 01  3C345        11 22 00  25.9  57.4 -5.4     -70.6    14    23835   17 52 01
17 55 21  ---          11 25 21  26.5  57.6 -5.3     -71.0   200    23886   17 52 02

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 57 28  P-UHER       11 27 28  22.3  80.6 -5.0     -63.8   103    23886   Stopped 
17 58 28  ---          11 28 28  22.5  80.7 -5.0     -63.8    60    23886           

 ---------- Following scan added by Sched for reference pointing ----------

17 58 34  P-UHER       11 28 34  22.5  80.7 -5.0     -63.8     0    23886   Stopped 
17 59 34  ---          11 29 34  22.7  80.8 -4.9     -63.9    60    23886           
Schedule for VLBA_FD   (Code Fd )                                   Page 101
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 00 00  1633+38      11 30 00  28.2  60.3 -5.1     -71.7     3    23886   18 00 00
18 06 40  ---          11 36 42  29.5  60.7 -5.0     -72.5   400    23989   18 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 07 00  1633+38      11 37 02  29.6  60.7 -5.0     -72.6    14    23989   18 07 00
18 10 20  ---          11 40 22  30.2  61.0 -4.9     -73.0   200    24040   18 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 12 27  P-UHER       11 42 30  25.5  82.3 -4.7     -64.3   104    24040   Stopped 
18 13 27  ---          11 43 30  25.7  82.4 -4.7     -64.3    60    24040           

 ---------- Following scan added by Sched for reference pointing ----------

18 13 33  P-UHER       11 43 36  25.7  82.4 -4.7     -64.3     0    24040   Stopped 
18 14 33  ---          11 44 36  25.9  82.5 -4.7     -64.4    60    24040           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 15 00  3C345        11 45 03  30.1  58.9 -5.0     -73.5     2    24040   18 15 00
18 21 40  ---          11 51 44  31.3  59.3 -4.9     -74.4   400    24143   18 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 22 00  3C345        11 52 04  31.4  59.3 -4.9     -74.4    14    24143   18 22 00
18 25 20  ---          11 55 25  32.0  59.5 -4.8     -74.9   200    24194   18 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 102
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 27 28  P-UHER       11 57 33  28.7  84.0 -4.5     -64.7   103    24194   Stopped 
18 28 28  ---          11 58 34  28.9  84.1 -4.5     -64.8    60    24194           

 ---------- Following scan added by Sched for reference pointing ----------

18 28 34  P-UHER       11 58 40  28.9  84.1 -4.5     -64.8     0    24194   Stopped 
18 29 34  ---          11 59 40  29.1  84.3 -4.4     -64.8    60    24194           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 30 00  1633+38      12 00 05  33.9  62.2 -4.6     -75.3     2    24194   18 30 00
18 36 40  ---          12 06 47  35.2  62.6 -4.5     -76.2   400    24296   18 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 37 00  1633+38      12 07 07  35.3  62.6 -4.5     -76.2    14    24296   18 37 00
18 40 20  ---          12 10 27  35.9  62.8 -4.4     -76.6   200    24348   18 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 42 25  P-UHER       12 12 33  31.9  85.8 -4.2     -65.1   101    24348   Stopped 
18 43 25  ---          12 13 33  32.1  85.9 -4.2     -65.1    60    24348           

 ---------- Following scan added by Sched for reference pointing ----------

18 43 31  P-UHER       12 13 39  32.1  85.9 -4.2     -65.1     0    24348   Stopped 
18 44 31  ---          12 14 39  32.4  86.0 -4.2     -65.1    60    24348           
Schedule for VLBA_FD   (Code Fd )                                   Page 103
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 45 00  3C345        12 15 08  35.7  60.6 -4.5     -77.4     3    24348   18 45 00
18 51 40  ---          12 21 49  37.0  61.0 -4.4     -78.3   400    24450   18 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 52 00  3C345        12 22 09  37.0  61.0 -4.4     -78.3    14    24450   18 52 00
18 55 20  ---          12 25 30  37.6  61.1 -4.3     -78.8   200    24501   18 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 57 27  P-UHER       12 27 37  35.1  87.5 -4.0     -65.3   100    24501   Stopped 
18 58 27  ---          12 28 37  35.3  87.7 -4.0     -65.3    60    24501           

 ---------- Following scan added by Sched for reference pointing ----------

18 58 33  P-UHER       12 28 43  35.4  87.7 -4.0     -65.3     0    24501   Stopped 
18 59 33  ---          12 29 43  35.6  87.8 -3.9     -65.3    60    24501           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 00 00  1633+38      12 30 10  39.7  63.9 -4.1     -79.0     2    24501   19 00 00
19 06 40  ---          12 36 51  41.0  64.2 -4.0     -79.8   400    24604   19 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 07 00  1633+38      12 37 11  41.0  64.2 -4.0     -79.9    14    24604   19 07 00
19 10 20  ---          12 40 32  41.7  64.3 -3.9     -80.3   200    24655   19 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page 104
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 12 23  P-UHER       12 42 35  38.4  89.4 -3.7     -65.4    98    24655   Stopped 
19 13 23  ---          12 43 36  38.6  89.5 -3.7     -65.4    60    24655           

 ---------- Following scan added by Sched for reference pointing ----------

19 13 29  P-UHER       12 43 42  38.6  89.5 -3.7     -65.4     0    24655   Stopped 
19 14 29  ---          12 44 42  38.8  89.7 -3.7     -65.4    60    24655           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 15 00  3C345        12 45 13  41.4  62.0 -4.0     -81.4     3    24655   19 15 00
19 21 40  ---          12 51 54  42.7  62.2 -3.9     -82.3   400    24758   19 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 22 00  3C345        12 52 14  42.7  62.3 -3.9     -82.3    14    24758   19 22 00
19 25 20  ---          12 55 34  43.4  62.4 -3.8     -82.8   200    24809   19 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 27 24  P-UHER       12 57 39  41.6  91.3 -3.5     -65.4    96    24809   Stopped 
19 28 24  ---          12 58 39  41.8  91.5 -3.5     -65.4    60    24809           

 ---------- Following scan added by Sched for reference pointing ----------

19 28 30  P-UHER       12 58 46  41.8  91.5 -3.5     -65.4     0    24809   Stopped 
19 29 30  ---          12 59 46  42.0  91.6 -3.4     -65.4    60    24809           
Schedule for VLBA_FD   (Code Fd )                                   Page 105
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 30 00  1633+38      13 00 15  45.5  65.1 -3.6     -82.8     3    24809   19 30 00
19 36 40  ---          13 06 56  46.8  65.3 -3.5     -83.7   400    24912   19 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 37 00  1633+38      13 07 16  46.9  65.4 -3.5     -83.7    14    24912   19 37 00
19 40 20  ---          13 10 37  47.6  65.5 -3.4     -84.1   200    24963   19 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 42 20  P-UHER       13 12 37  44.8  93.4 -3.2     -65.2    92    24963   Stopped 
19 43 20  ---          13 13 37  45.0  93.5 -3.2     -65.2    60    24963           

 ---------- Following scan added by Sched for reference pointing ----------

19 43 26  P-UHER       13 13 43  45.0  93.5 -3.2     -65.2     0    24963   Stopped 
19 44 26  ---          13 14 44  45.3  93.7 -3.2     -65.2    60    24963           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 45 00  3C345        13 15 18  47.1  62.9 -3.5     -85.5     4    24963   19 45 00
19 51 40  ---          13 21 59  48.4  63.0 -3.4     -86.5   400    25066   19 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 52 00  3C345        13 22 19  48.5  63.1 -3.4     -86.6    14    25066   19 52 00
19 55 20  ---          13 25 39  49.1  63.1 -3.3     -87.1   200    25117   19 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 106
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 57 21  P-UHER       13 27 41  48.0  95.5 -3.0     -64.8    91    25117   Stopped 
19 58 21  ---          13 28 41  48.3  95.7 -3.0     -64.8    60    25117           

 ---------- Following scan added by Sched for reference pointing ----------

19 58 27  P-UHER       13 28 47  48.3  95.7 -3.0     -64.8     0    25117   Stopped 
19 59 27  ---          13 29 48  48.5  95.9 -2.9     -64.8    60    25117           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 00 00  1633+38      13 30 20  51.4  65.9 -3.1     -86.8     3    25117   20 00 00
20 06 40  ---          13 37 01  52.7  66.0 -3.0     -87.8   400    25219   20 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 07 00  1633+38      13 37 21  52.8  66.0 -3.0     -87.8    14    25219   20 07 00
20 10 20  ---          13 40 42  53.5  66.1 -2.9     -88.3   200    25271   20 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

20 12 16  P-UHER       13 42 38  51.2  97.9 -2.7     -64.2    86    25271   Stopped 
20 13 16  ---          13 43 38  51.4  98.1 -2.7     -64.2    60    25271           

 ---------- Following scan added by Sched for reference pointing ----------

20 13 22  P-UHER       13 43 44  51.5  98.1 -2.7     -64.2     0    25271   Stopped 
20 14 22  ---          13 44 45  51.7  98.2 -2.7     -64.1    60    25271           
Schedule for VLBA_FD   (Code Fd )                                   Page 107
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 15 00  3C345        13 45 23  52.9  63.3 -3.0     -90.1     5    25271   20 15 00
20 21 40  ---          13 52 04  54.2  63.2 -2.9     -91.2   400    25373   20 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 22 00  3C345        13 52 24  54.2  63.2 -2.9     -91.2    14    25373   20 22 00
20 25 20  ---          13 55 44  54.9  63.2 -2.8     -91.8   200    25425   20 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

20 27 18  P-UHER       13 57 42  54.4 100.5 -2.5     -63.4    83    25425   Stopped 
20 28 18  ---          13 58 42  54.6 100.7 -2.5     -63.3    60    25425           

 ---------- Following scan added by Sched for reference pointing ----------

20 28 24  P-UHER       13 58 49  54.7 100.7 -2.5     -63.3     0    25425   Stopped 
20 29 24  ---          13 59 49  54.9 100.9 -2.4     -63.2    60    25425           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 30 00  1633+38      14 00 25  57.3  66.1 -2.6     -91.4     4    25425   20 30 00
20 36 40  ---          14 07 06  58.6  66.0 -2.5     -92.5   400    25527   20 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 37 00  1633+38      14 07 26  58.7  66.0 -2.5     -92.5    14    25527   20 37 00
20 40 20  ---          14 10 47  59.4  65.9 -2.4     -93.1   200    25578   20 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 108
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

20 42 11  P-UHER       14 12 38  57.6 103.4 -2.2     -62.2    76    25578   Stopped 
20 43 11  ---          14 13 38  57.8 103.6 -2.2     -62.1    60    25578           

 ---------- Following scan added by Sched for reference pointing ----------

20 43 17  P-UHER       14 13 44  57.8 103.6 -2.2     -62.1     0    25578   Stopped 
20 44 17  ---          14 14 44  58.0 103.8 -2.2     -62.0    60    25578           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 45 00  3C345        14 15 28  58.7  62.8 -2.5     -95.3     6    25578   20 45 00
20 51 40  ---          14 22 09  59.9  62.5 -2.4     -96.6   400    25681   20 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 52 00  3C345        14 22 29  60.0  62.5 -2.3     -96.7    14    25681   20 52 00
20 55 20  ---          14 25 49  60.6  62.3 -2.3     -97.4   200    25732   20 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

20 57 13  P-UHER       14 27 43  60.7 106.7 -2.0     -60.6    74    25732   Stopped 
20 58 13  ---          14 28 43  60.9 107.0 -2.0     -60.4    60    25732           

 ---------- Following scan added by Sched for reference pointing ----------

20 58 19  P-UHER       14 28 49  60.9 107.0 -2.0     -60.4     0    25732   Stopped 
20 59 19  ---          14 29 49  61.1 107.2 -1.9     -60.3    60    25732           
Schedule for VLBA_FD   (Code Fd )                                   Page 109
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

21 00 00  1633+38      14 30 30  63.2  65.2 -2.1     -96.7     3    25732   21 00 00
21 06 40  ---          14 37 11  64.5  64.9 -2.0     -98.1   400    25835   21 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

21 07 00  1633+38      14 37 31  64.6  64.8 -2.0     -98.2    14    25835   21 07 00
21 10 20  ---          14 40 52  65.3  64.6 -1.9     -98.9   200    25886   21 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

21 12 04  P-UHER       14 42 37  63.7 110.6 -1.7     -58.4    64    25886   Stopped 
21 13 04  ---          14 43 37  63.9 110.8 -1.7     -58.2    60    25886           

 ---------- Following scan added by Sched for reference pointing ----------

21 13 10  P-UHER       14 43 43  64.0 110.9 -1.7     -58.2     0    25886   Stopped 
21 14 10  ---          14 44 43  64.2 111.2 -1.7     -58.0    60    25886           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

21 15 00  3C345        14 45 33  64.4  61.0 -2.0    -101.7     6    25886   21 15 00
21 21 40  ---          14 52 14  65.6  60.3 -1.9    -103.4   400    25989   21 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

21 22 00  3C345        14 52 34  65.7  60.3 -1.8    -103.5    14    25989   21 22 00
21 25 20  ---          14 55 54  66.3  59.9 -1.8    -104.4   200    26040   21 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 110
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

21 27 08  P-UHER       14 57 43  66.7 115.2 -1.5     -55.3    61    26040   Stopped 
21 28 08  ---          14 58 43  66.9 115.6 -1.5     -55.1    60    26040           

 ---------- Following scan added by Sched for reference pointing ----------

21 28 14  P-UHER       14 58 49  67.0 115.6 -1.5     -55.1     0    26040   Stopped 
21 29 14  ---          14 59 49  67.1 116.0 -1.4     -54.8    60    26040           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

21 30 00  1633+38      15 00 35  69.1  62.6 -1.6    -103.8     0    26040   21 30 00
21 36 40  ---          15 07 16  70.3  61.7 -1.5    -105.7   400    26143   21 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

21 37 00  1633+38      15 07 36  70.4  61.6 -1.5    -105.8    14    26143   21 37 00
21 40 20  ---          15 10 57  71.0  61.1 -1.4    -106.8   200    26194   21 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

21 41 59  P-UHER       15 12 36  69.6 120.9 -1.2     -51.3    49    26194   Stopped 
21 42 59  ---          15 13 36  69.8 121.3 -1.2     -51.0    60    26194           

 ---------- Following scan added by Sched for reference pointing ----------

21 43 05  P-UHER       15 13 42  69.8 121.4 -1.2     -50.9     0    26194   Stopped 
21 44 05  ---          15 14 42  70.0 121.8 -1.2     -50.6    60    26194           
Schedule for VLBA_FD   (Code Fd )                                   Page 111
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

21 45 00  3C345        15 15 37  69.9  56.9 -1.5    -110.3     1    26194   21 45 00
21 51 40  ---          15 22 19  71.1  55.5 -1.4    -112.7   400    26296   21 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

21 52 00  3C345        15 22 39  71.2  55.4 -1.3    -112.8    14    26296   21 52 00
21 55 20  ---          15 25 59  71.8  54.6 -1.3    -114.1   200    26348   21 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

21 57 24  P-UHER       15 28 03  72.3 128.3 -1.0     -45.5    64    26348   Stopped 
21 58 24  ---          15 29 03  72.5 128.9 -1.0     -45.1    60    26348           

 ---------- Following scan added by Sched for reference pointing ----------

21 58 30  P-UHER       15 29 09  72.5 128.9 -1.0     -45.0     0    26348   Stopped 
21 59 30  ---          15 30 09  72.7 129.5 -0.9     -44.6    60    26348           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

22 00 30  1633+38      15 31 10  74.7  56.3 -1.1    -114.5     0    26348   22 00 30
22 07 10  ---          15 37 51  75.9  54.0 -1.0    -117.8   400    26450   22 00 31

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

22 07 30  1633+38      15 38 11  76.0  53.9 -1.0    -117.9    14    26450   22 07 30
22 10 50  ---          15 41 32  76.6  52.5 -0.9    -119.8   200    26501   22 07 31
Schedule for VLBA_FD   (Code Fd )                                   Page 112
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

22 12 47  P-UHER       15 43 29  74.7 138.0 -0.7     -37.5    49    26501   Stopped 
22 13 47  ---          15 44 29  74.9 138.7 -0.7     -36.9    60    26501           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

22 15 00  3C345        15 45 42  75.1  48.2 -1.0    -123.4     1    26501   22 15 00
22 21 40  ---          15 52 23  76.1  45.2 -0.9    -127.4   400    26604   22 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

22 22 00  3C345        15 52 44  76.2  45.0 -0.8    -127.6    14    26604   22 22 00
22 25 20  ---          15 56 04  76.7  43.3 -0.8    -129.8   200    26655   22 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

22 27 33  P-UHER       15 58 18  76.6 149.9 -0.5     -27.1    50    26655   Stopped 
22 28 33  ---          15 59 18  76.7 150.9 -0.5     -26.3    60    26655           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

22 30 00  1633+38      16 00 45  79.6  41.6 -0.6    -133.4     1    26655   22 30 00
22 36 40  ---          16 07 26  80.5  36.1 -0.5    -139.9   400    26758   22 30 01
Schedule for VLBA_FD   (Code Fd )                                   Page 113
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

22 37 00  1633+38      16 07 46  80.6  35.8 -0.5    -140.3    14    26758   22 37 00
22 40 20  ---          16 11 07  81.0  32.5 -0.4    -144.0   200    26809   22 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

22 42 13  P-UHER       16 13 00  77.8 164.7 -0.2     -13.9    12    26809   Stopped 
22 43 13  ---          16 14 00  77.9 165.8 -0.2     -12.9    60    26809           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

22 45 00  3C345        16 15 47  79.2  29.8 -0.5    -146.2     2    26809   22 45 00
22 51 40  ---          16 22 28  79.9  23.6 -0.3    -153.3   400    26912   22 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

22 52 00  3C345        16 22 48  79.9  23.3 -0.3    -153.7    14    26912   22 52 00
22 55 20  ---          16 26 09  80.2  19.9 -0.3    -157.6   200    26963   22 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

22 58 15  3C279        16 29 04  27.6 243.7  3.5      50.8     8    26963   Stopped 
22 59 15  ---          16 30 05  27.4 243.9  3.6      51.0    60    26963           
Schedule for VLBA_FD   (Code Fd )                                   Page 114
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

23 00 00  1510-089     16 30 50  46.1 208.1  1.3      24.2     0    26963   23 00 00
23 06 40  ---          16 37 31  45.4 210.2  1.4      26.0   400    27066   23 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

23 07 00  1510-089     16 37 51  45.4 210.3  1.4      26.1    14    27066   23 07 00
23 10 20  ---          16 41 11  45.0 211.4  1.5      27.0   200    27117   23 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

23 12 06  3C279        16 42 58  24.8 246.1  3.8      52.3    59    27117   Stopped 
23 13 06  ---          16 43 58  24.7 246.3  3.8      52.4    60    27117           

 ---------- Following scan added by Sched for reference pointing ----------

23 13 12  3C279        16 44 04  24.6 246.3  3.8      52.4     0    27117   Stopped 
23 14 12  ---          16 45 05  24.4 246.4  3.8      52.5    60    27117           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

23 15 00  1510-089     16 45 52  44.5 212.8  1.5      28.2     0    27117   23 15 00
23 21 40  ---          16 52 33  43.7 214.8  1.6      29.8   400    27219   23 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

23 22 00  1510-089     16 52 53  43.6 214.9  1.7      29.9    14    27219   23 22 00
23 25 20  ---          16 56 14  43.2 215.9  1.7      30.7   200    27271   23 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 115
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

23 27 06  P-VXSGR      16 58 00  34.5 160.0 -1.2     -18.5    58    27271   Stopped 
23 28 06  ---          16 59 00  34.5 160.3 -1.2     -18.3    60    27271           

 ---------- Following scan added by Sched for reference pointing ----------

23 28 12  P-VXSGR      16 59 06  34.6 160.3 -1.2     -18.3     0    27271   Stopped 
23 29 12  ---          17 00 06  34.6 160.6 -1.1     -18.0    60    27271           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

23 30 00  1510-089     17 00 55  42.6 217.2  1.8      31.8     0    27271   23 30 00
23 36 40  ---          17 07 36  41.7 219.1  1.9      33.4   400    27373   23 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

23 37 00  1510-089     17 07 56  41.7 219.2  1.9      33.4    14    27373   23 37 00
23 40 20  ---          17 11 16  41.2 220.1  2.0      34.2   200    27425   23 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

23 42 05  P-VXSGR      17 13 02  35.5 164.1 -0.9     -14.8    57    27425   Stopped 
23 43 05  ---          17 14 02  35.5 164.3 -0.9     -14.5    60    27425           

 ---------- Following scan added by Sched for reference pointing ----------

23 43 11  P-VXSGR      17 14 08  35.5 164.4 -0.9     -14.5     0    27425   Stopped 
23 44 11  ---          17 15 08  35.6 164.6 -0.9     -14.3    60    27425           
Schedule for VLBA_FD   (Code Fd )                                   Page 116
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  27 Sep 2014   Day 270 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

23 45 00  1510-089     17 15 57  40.6 221.4  2.0      35.2     1    27425   23 45 00
23 51 40  ---          17 22 38  39.6 223.1  2.2      36.6   400    27527   23 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

23 52 00  1510-089     17 22 58  39.5 223.2  2.2      36.6    14    27527   23 52 00
23 55 20  ---          17 26 19  39.1 224.1  2.2      37.3   200    27578   23 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

23 57 06  P-VXSGR      17 28 05  36.2 168.2 -0.7     -10.9    58    27578   Stopped 
23 58 06  ---          17 29 05  36.3 168.5 -0.7     -10.6    60    27578           

 ---------- Following scan added by Sched for reference pointing ----------

23 58 12  P-VXSGR      17 29 11  36.3 168.6 -0.7     -10.6     0    27578   Stopped 
23 59 12  ---          17 30 11  36.3 168.8 -0.6     -10.4    60    27578           

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

00 00 01  1510-089     17 31 01  38.3 225.2  2.3      38.2     1    27578   00 00 01
00 06 41  ---          17 37 42  37.3 226.9  2.4      39.5   400    27681   00 00 02
Schedule for VLBA_FD   (Code Fd )                                   Page 117
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

00 07 01  1510-089     17 38 02  37.3 227.0  2.4      39.6    14    27681   00 07 01
00 10 21  ---          17 41 22  36.7 227.7  2.5      40.2   200    27732   00 07 02

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

00 12 05  P-VXSGR      17 43 06  36.8 172.5 -0.4      -6.9    56    27732   Stopped 
00 13 05  ---          17 44 07  36.8 172.8 -0.4      -6.7    60    27732           

 ---------- Following scan added by Sched for reference pointing ----------

00 13 11  P-VXSGR      17 44 13  36.8 172.8 -0.4      -6.7     0    27732   Stopped 
00 14 11  ---          17 45 13  36.8 173.1 -0.4      -6.4    60    27732           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

00 15 00  1510-089     17 46 02  36.0 228.8  2.5      41.0     2    27732   00 15 00
00 21 40  ---          17 52 43  34.9 230.3  2.7      42.1   400    27835   00 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

00 22 00  1510-089     17 53 03  34.8 230.4  2.7      42.2    14    27835   00 22 00
00 25 20  ---          17 56 24  34.3 231.2  2.7      42.8   200    27886   00 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 118
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

00 27 05  P-VXSGR      17 58 09  37.1 176.9 -0.2      -2.9    58    27886   Stopped 
00 28 05  ---          17 59 09  37.1 177.2 -0.2      -2.6    60    27886           

 ---------- Following scan added by Sched for reference pointing ----------

00 28 11  P-VXSGR      17 59 15  37.1 177.2 -0.2      -2.6     0    27886   Stopped 
00 29 11  ---          18 00 15  37.1 177.5 -0.1      -2.3    60    27886           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

00 30 00  1510-089     18 01 05  33.5 232.2  2.8      43.5     2    27886   00 30 00
00 36 40  ---          18 07 46  32.3 233.6  2.9      44.5   400    27989   00 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

00 37 00  1510-089     18 08 06  32.3 233.7  2.9      44.6    14    27989   00 37 00
00 40 20  ---          18 11 26  31.7 234.3  3.0      45.1   200    28040   00 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

00 42 05  P-VXSGR      18 13 12  37.1 181.2  0.1       1.1    60    28040   Stopped 
00 43 05  ---          18 14 12  37.1 181.5  0.1       1.4    60    28040           

 ---------- Following scan added by Sched for reference pointing ----------

00 43 11  P-VXSGR      18 14 18  37.1 181.6  0.1       1.4     0    28040   Stopped 
00 44 11  ---          18 15 18  37.1 181.8  0.1       1.7    60    28040           
Schedule for VLBA_FD   (Code Fd )                                   Page 119
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

00 45 00  1510-089     18 16 07  30.9 235.3  3.0      45.8     3    28040   00 45 00
00 51 40  ---          18 22 48  29.7 236.6  3.2      46.7   400    28142   00 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

00 52 00  1510-089     18 23 08  29.6 236.7  3.2      46.7    14    28142   00 52 00
00 55 20  ---          18 26 29  29.0 237.3  3.2      47.2   200    28194   00 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

00 57 48  3C454.3      18 28 57  28.2  87.1 -4.4     -63.5    33    28194   Stopped 
00 58 48  ---          18 29 57  28.4  87.2 -4.4     -63.5    60    28194           

 ---------- Following scan added by Sched for reference pointing ----------

00 58 54  3C454.3      18 30 03  28.4  87.2 -4.4     -63.5     0    28194   Stopped 
00 59 54  ---          18 31 03  28.7  87.3 -4.4     -63.5    60    28194           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 00 00  3C454.3      18 31 09  28.7  87.3 -4.4     -63.5     0    28194   01 00 00
01 06 40  ---          18 37 51  30.1  88.2 -4.3     -63.6   400    28296   01 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

01 07 00  3C454.3      18 38 11  30.2  88.2 -4.3     -63.6    14    28296   01 07 00
01 10 20  ---          18 41 31  30.9  88.6 -4.2     -63.6   200    28348   01 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page 120
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 12 40  3C454.3      18 43 51  31.4  88.9 -4.2     -63.6   133    28348   Stopped 
01 13 40  ---          18 44 51  31.6  89.0 -4.2     -63.6    60    28348           

 ---------- Following scan added by Sched for reference pointing ----------

01 13 46  3C454.3      18 44 57  31.6  89.0 -4.2     -63.6     0    28348   Stopped 
01 14 46  ---          18 45 58  31.9  89.2 -4.1     -63.6    60    28348           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 15 00  CTA102       18 46 12  34.4  96.8 -3.8     -60.8     1    28348   01 15 00
01 21 40  ---          18 52 53  35.9  97.7 -3.7     -60.6   400    28450   01 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

01 22 00  CTA102       18 53 13  35.9  97.8 -3.7     -60.6    14    28450   01 22 00
01 25 20  ---          18 56 34  36.7  98.3 -3.6     -60.4   200    28501   01 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 27 48  3C454.3      18 59 02  34.7  90.8 -3.9     -63.6   134    28501   Stopped 
01 28 48  ---          19 00 02  34.9  91.0 -3.9     -63.6    60    28501           

 ---------- Following scan added by Sched for reference pointing ----------

01 28 54  3C454.3      19 00 08  34.9  91.0 -3.9     -63.6     0    28501   Stopped 
01 29 54  ---          19 01 08  35.1  91.1 -3.9     -63.6    60    28501           
Schedule for VLBA_FD   (Code Fd )                                   Page 121
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 30 00  3C454.3      19 01 14  35.1  91.1 -3.9     -63.6     0    28501   01 30 00
01 36 40  ---          19 07 55  36.6  92.0 -3.8     -63.6   400    28604   01 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

01 37 00  3C454.3      19 08 16  36.7  92.1 -3.8     -63.6    14    28604   01 37 00
01 40 20  ---          19 11 36  37.4  92.5 -3.7     -63.5   200    28655   01 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 42 54  3C454.3      19 14 11  37.9  92.8 -3.7     -63.5   148    28655   Stopped 
01 43 54  ---          19 15 11  38.1  93.0 -3.7     -63.5    60    28655           

 ---------- Following scan added by Sched for reference pointing ----------

01 44 00  3C454.3      19 15 17  38.2  93.0 -3.7     -63.5     0    28655   Stopped 
01 45 00  ---          19 16 17  38.4  93.1 -3.6     -63.5    60    28655           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 45 15  CTA102       19 16 32  40.9 101.4 -3.3     -59.5     1    28655   01 45 15
01 51 55  ---          19 23 13  42.3 102.5 -3.2     -59.1   400    28758   01 45 16

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

01 52 15  CTA102       19 23 33  42.4 102.6 -3.2     -59.1    14    28758   01 52 15
01 55 35  ---          19 26 54  43.1 103.2 -3.1     -58.9   200    28809   01 52 16
Schedule for VLBA_FD   (Code Fd )                                   Page 122
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 57 48  3C454.3      19 29 07  41.1  94.9 -3.4     -63.2   119    28809   Stopped 
01 58 48  ---          19 30 07  41.3  95.1 -3.4     -63.2    60    28809           

 ---------- Following scan added by Sched for reference pointing ----------

01 58 54  3C454.3      19 30 13  41.4  95.1 -3.4     -63.2     0    28809   Stopped 
01 59 54  ---          19 31 13  41.6  95.2 -3.4     -63.2    60    28809           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 00 00  3C454.3      19 31 19  41.6  95.2 -3.4     -63.2     0    28809   02 00 00
02 06 40  ---          19 38 00  43.0  96.2 -3.3     -63.0   400    28912   02 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

02 07 00  3C454.3      19 38 20  43.1  96.3 -3.3     -63.0    14    28912   02 07 00
02 10 20  ---          19 41 41  43.8  96.8 -3.2     -62.9   200    28963   02 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 12 38  3C454.3      19 44 00  44.3  97.1 -3.2     -62.8   132    28963   Stopped 
02 13 38  ---          19 45 00  44.5  97.3 -3.2     -62.7    60    28963           

 ---------- Following scan added by Sched for reference pointing ----------

02 13 44  3C454.3      19 45 06  44.6  97.3 -3.2     -62.7     0    28963   Stopped 
02 14 44  ---          19 46 06  44.8  97.5 -3.1     -62.7    60    28963           
Schedule for VLBA_FD   (Code Fd )                                   Page 123
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 15 00  CTA102       19 46 22  47.1 106.7 -2.8     -57.3     1    28963   02 15 00
02 21 40  ---          19 53 03  48.5 108.1 -2.7     -56.7   400    29066   02 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

02 22 00  CTA102       19 53 23  48.5 108.1 -2.7     -56.7    14    29066   02 22 00
02 25 20  ---          19 56 43  49.2 108.8 -2.6     -56.3   200    29117   02 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 27 48  3C454.3      19 59 12  47.6  99.6 -2.9     -62.1   133    29117   Stopped 
02 28 48  ---          20 00 12  47.8  99.7 -2.9     -62.0    60    29117           

 ---------- Following scan added by Sched for reference pointing ----------

02 28 54  3C454.3      20 00 18  47.8  99.7 -2.9     -62.0     0    29117   Stopped 
02 29 54  ---          20 01 18  48.0  99.9 -2.9     -62.0    60    29117           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 30 00  3C454.3      20 01 24  48.0  99.9 -2.9     -62.0     0    29117   02 30 00
02 36 40  ---          20 08 05  49.4 101.1 -2.8     -61.6   400    29219   02 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

02 37 00  3C454.3      20 08 25  49.5 101.1 -2.8     -61.6    14    29219   02 37 00
02 40 20  ---          20 11 46  50.2 101.7 -2.7     -61.3   200    29271   02 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 124
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 42 38  3C454.3      20 14 04  50.7 102.2 -2.7     -61.2   131    29271   Stopped 
02 43 38  ---          20 15 04  50.9 102.3 -2.7     -61.1    60    29271           

 ---------- Following scan added by Sched for reference pointing ----------

02 43 44  3C454.3      20 15 10  50.9 102.4 -2.7     -61.1     0    29271   Stopped 
02 44 44  ---          20 16 10  51.1 102.5 -2.6     -61.0    60    29271           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 45 00  CTA102       20 16 27  53.2 113.2 -2.3     -53.9     1    29271   02 45 00
02 51 40  ---          20 23 08  54.5 114.9 -2.2     -52.9   400    29373   02 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

02 52 00  CTA102       20 23 28  54.6 115.0 -2.2     -52.8    14    29373   02 52 00
02 55 20  ---          20 26 48  55.2 115.8 -2.1     -52.3   200    29425   02 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 57 48  3C454.3      20 29 17  53.9 105.1 -2.4     -59.9   132    29425   Stopped 
02 58 48  ---          20 30 17  54.1 105.3 -2.4     -59.8    60    29425           

 ---------- Following scan added by Sched for reference pointing ----------

02 58 54  3C454.3      20 30 23  54.1 105.3 -2.4     -59.8     0    29425   Stopped 
02 59 54  ---          20 31 23  54.3 105.5 -2.4     -59.7    60    29425           
Schedule for VLBA_FD   (Code Fd )                                   Page 125
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 00 00  3C454.3      20 31 29  54.3 105.5 -2.4     -59.7     0    29425   03 00 00
03 06 40  ---          20 38 10  55.7 107.0 -2.3     -59.0   400    29527   03 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

03 07 00  3C454.3      20 38 30  55.8 107.0 -2.3     -59.0    14    29527   03 07 00
03 10 20  ---          20 41 51  56.5 107.8 -2.2     -58.6   200    29578   03 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

03 12 48  3C454.3      20 44 19  57.0 108.4 -2.2     -58.3   141    29578   Stopped 
03 13 48  ---          20 45 19  57.2 108.6 -2.2     -58.1    60    29578           

 ---------- Following scan added by Sched for reference pointing ----------

03 13 54  3C454.3      20 45 25  57.2 108.6 -2.2     -58.1     0    29578   Stopped 
03 14 54  ---          20 46 25  57.4 108.9 -2.1     -58.0    60    29578           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 15 00  3C454.3      20 46 32  57.4 108.9 -2.1     -58.0     0    29578   03 15 00
03 21 40  ---          20 53 13  58.8 110.5 -2.0     -57.1   400    29681   03 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

03 22 00  3C454.3      20 53 33  58.8 110.6 -2.0     -57.0    14    29681   03 22 00
03 25 20  ---          20 56 53  59.5 111.4 -2.0     -56.5   200    29732   03 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 126
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

03 27 48  3C454.3      20 59 22  60.0 112.1 -1.9     -56.1   141    29732   Stopped 
03 28 48  ---          21 00 22  60.2 112.4 -1.9     -56.0    60    29732           

 ---------- Following scan added by Sched for reference pointing ----------

03 28 54  3C454.3      21 00 28  60.2 112.4 -1.9     -55.9     0    29732   Stopped 
03 29 54  ---          21 01 28  60.4 112.7 -1.9     -55.8    60    29732           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 30 00  3C454.3      21 01 34  60.4 112.7 -1.9     -55.8     0    29732   03 30 00
03 36 40  ---          21 08 15  61.8 114.6 -1.8     -54.6   400    29835   03 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

03 37 00  3C454.3      21 08 35  61.8 114.7 -1.8     -54.5    14    29835   03 37 00
03 40 20  ---          21 11 56  62.5 115.7 -1.7     -53.9   200    29886   03 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

03 42 48  3C454.3      21 14 24  63.0 116.5 -1.7     -53.3   141    29886   Stopped 
03 43 48  ---          21 15 24  63.2 116.8 -1.7     -53.1    60    29886           

 ---------- Following scan added by Sched for reference pointing ----------

03 43 54  3C454.3      21 15 30  63.2 116.8 -1.7     -53.1     0    29886   Stopped 
03 44 54  ---          21 16 30  63.4 117.1 -1.6     -52.9    60    29886           
Schedule for VLBA_FD   (Code Fd )                                   Page 127
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 45 00  3C454.3      21 16 37  63.4 117.2 -1.6     -52.9     0    29886   03 45 00
03 51 40  ---          21 23 18  64.6 119.4 -1.5     -51.3   400    29989   03 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

03 52 00  3C454.3      21 23 38  64.7 119.5 -1.5     -51.2    14    29989   03 52 00
03 55 20  ---          21 26 58  65.3 120.7 -1.5     -50.4   200    30040   03 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

03 57 48  3C454.3      21 29 26  65.8 121.7 -1.4     -49.7   141    30040   Stopped 
03 58 48  ---          21 30 27  66.0 122.0 -1.4     -49.4    60    30040           

 ---------- Following scan added by Sched for reference pointing ----------

03 58 54  3C454.3      21 30 33  66.0 122.1 -1.4     -49.4     0    30040   Stopped 
03 59 54  ---          21 31 33  66.2 122.5 -1.4     -49.1    60    30040           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 00 00  3C454.3      21 31 39  66.2 122.5 -1.4     -49.1     0    30040   04 00 00
04 06 40  ---          21 38 20  67.4 125.2 -1.3     -47.1   400    30142   04 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

04 07 00  3C454.3      21 38 40  67.4 125.4 -1.3     -46.9    14    30142   04 07 00
04 10 20  ---          21 42 01  68.0 126.8 -1.2     -45.8   200    30194   04 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page 128
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 12 33  3C454.3      21 44 14  68.4 127.8 -1.2     -45.0   126    30194   Stopped 
04 13 33  ---          21 45 14  68.6 128.3 -1.2     -44.7    60    30194           

 ---------- Following scan added by Sched for reference pointing ----------

04 13 39  3C454.3      21 45 20  68.6 128.4 -1.2     -44.6     0    30194   Stopped 
04 14 39  ---          21 46 20  68.8 128.8 -1.1     -44.3    60    30194           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 15 00  CTA102       21 46 42  68.3 147.6 -0.8     -28.1     0    30194   04 15 00
04 21 40  ---          21 53 23  69.0 151.7 -0.7     -24.7   400    30296   04 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

04 22 00  CTA102       21 53 43  69.1 151.9 -0.7     -24.5    14    30296   04 22 00
04 25 20  ---          21 57 03  69.4 154.0 -0.6     -22.7   200    30348   04 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 27 48  3C454.3      21 59 31  70.9 135.7 -0.9     -38.8   126    30348   Stopped 
04 28 48  ---          22 00 32  71.0 136.3 -0.9     -38.3    60    30348           

 ---------- Following scan added by Sched for reference pointing ----------

04 28 54  3C454.3      22 00 38  71.0 136.3 -0.9     -38.2     0    30348   Stopped 
04 29 54  ---          22 01 38  71.2 136.9 -0.9     -37.7    60    30348           
Schedule for VLBA_FD   (Code Fd )                                   Page 129
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 30 00  3C454.3      22 01 44  71.2 137.0 -0.9     -37.7     0    30348   04 30 00
04 36 40  ---          22 08 25  72.1 141.1 -0.8     -34.2   400    30450   04 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

04 37 00  3C454.3      22 08 45  72.2 141.3 -0.8     -34.1    14    30450   04 37 00
04 40 20  ---          22 12 06  72.6 143.5 -0.7     -32.2   200    30501   04 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 42 31  3C454.3      22 14 17  72.9 145.1 -0.7     -30.9   125    30501   Stopped 
04 43 31  ---          22 15 17  73.0 145.8 -0.7     -30.3    60    30501           

 ---------- Following scan added by Sched for reference pointing ----------

04 43 37  3C454.3      22 15 23  73.0 145.8 -0.7     -30.2     0    30501   Stopped 
04 44 37  ---          22 16 24  73.1 146.6 -0.6     -29.6    60    30501           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 45 00  CTA102       22 16 46  70.8 167.6 -0.3     -10.9     0    30501   04 45 00
04 51 40  ---          22 23 28  71.0 172.5 -0.2      -6.6   400    30604   04 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

04 52 00  CTA102       22 23 48  71.0 172.8 -0.2      -6.3    14    30604   04 52 00
04 55 20  ---          22 27 08  71.1 175.3 -0.1      -4.1   200    30655   04 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 130
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 57 48  3C454.3      22 29 36  74.5 156.9 -0.4     -20.6   125    30655   Stopped 
04 58 48  ---          22 30 36  74.6 157.7 -0.4     -19.9    60    30655           

 ---------- Following scan added by Sched for reference pointing ----------

04 58 54  3C454.3      22 30 42  74.6 157.8 -0.4     -19.8     0    30655   Stopped 
04 59 54  ---          22 31 43  74.7 158.7 -0.4     -19.0    60    30655           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 00 00  3C454.3      22 31 49  74.7 158.7 -0.4     -19.0     0    30655   05 00 00
05 06 40  ---          22 38 30  75.1 164.7 -0.3     -13.7   400    30758   05 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

05 07 00  3C454.3      22 38 50  75.1 165.0 -0.3     -13.4    14    30758   05 07 00
05 10 20  ---          22 42 11  75.3 168.0 -0.2     -10.7   200    30809   05 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 12 32  3C454.3      22 44 23  75.4 170.1 -0.2      -8.9   125    30809   Stopped 
05 13 32  ---          22 45 23  75.4 171.1 -0.2      -8.0    60    30809           

 ---------- Following scan added by Sched for reference pointing ----------

05 13 38  3C454.3      22 45 29  75.4 171.1 -0.2      -7.9     0    30809   Stopped 
05 14 38  ---          22 46 29  75.5 172.1 -0.1      -7.1    60    30809           
Schedule for VLBA_FD   (Code Fd )                                   Page 131
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 15 00  CTA102       22 46 51  70.9 190.1  0.2       8.9     2    30809   05 15 00
05 21 40  ---          22 53 32  70.6 195.0  0.3      13.2   400    30912   05 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

05 22 00  CTA102       22 53 53  70.6 195.3  0.3      13.4    14    30912   05 22 00
05 25 20  ---          22 57 13  70.4 197.6  0.4      15.4   200    30963   05 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 27 48  3C454.3      22 59 41  75.6 184.8  0.1       4.3   129    30963   Stopped 
05 28 48  ---          23 00 41  75.5 185.7  0.1       5.1    60    30963           

 ---------- Following scan added by Sched for reference pointing ----------

05 28 54  3C454.3      23 00 47  75.5 185.8  0.1       5.2     0    30963   Stopped 
05 29 54  ---          23 01 47  75.5 186.8  0.1       6.1    60    30963           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 30 00  3C454.3      23 01 54  75.5 186.9  0.1       6.2     0    30963   05 30 00
05 36 40  ---          23 08 35  75.3 193.2  0.2      11.8   400    31066   05 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

05 37 00  3C454.3      23 08 55  75.2 193.5  0.2      12.1    14    31066   05 37 00
05 40 20  ---          23 12 16  75.0 196.5  0.3      14.8   200    31117   05 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 132
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 42 34  3C454.3      23 14 30  74.9 198.5  0.3      16.5   127    31117   Stopped 
05 43 34  ---          23 15 30  74.8 199.4  0.3      17.3    60    31117           

 ---------- Following scan added by Sched for reference pointing ----------

05 43 40  3C454.3      23 15 36  74.8 199.5  0.3      17.4     0    31117   Stopped 
05 44 40  ---          23 16 36  74.8 200.4  0.4      18.2    60    31117           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 45 00  CTA102       23 16 56  68.6 210.5  0.7      26.5     0    31117   05 45 00
05 51 40  ---          23 23 37  67.9 214.4  0.8      29.8   400    31219   05 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

05 52 00  CTA102       23 23 57  67.8 214.6  0.8      30.0    14    31219   05 52 00
05 55 20  ---          23 27 18  67.4 216.5  0.9      31.5   200    31271   05 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 57 17  P-IKTAU      23 29 15  26.1  91.9 -4.4     -61.3    20    31271   Stopped 
05 58 17  ---          23 30 15  26.4  92.1 -4.4     -61.3    60    31271           

 ---------- Following scan added by Sched for reference pointing ----------

05 58 23  P-IKTAU      23 30 21  26.4  92.1 -4.4     -61.3     0    31271   Stopped 
05 59 23  ---          23 31 21  26.6  92.2 -4.4     -61.3    60    31271           
Schedule for VLBA_FD   (Code Fd )                                   Page 133
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 00 00  0420-014     23 31 59  13.9 100.0 -4.9     -58.0     4    31271   06 00 00
06 06 40  ---          23 38 40  15.3 100.9 -4.8     -57.7   400    31373   06 00 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 12 23  P-IKTAU      23 44 23  29.4  93.9 -4.2     -61.1   309    31373   Stopped 
06 13 23  ---          23 45 24  29.6  94.1 -4.1     -61.1    60    31373           

 ---------- Following scan added by Sched for reference pointing ----------

06 13 29  P-IKTAU      23 45 30  29.6  94.1 -4.1     -61.1     0    31373   Stopped 
06 14 29  ---          23 46 30  29.8  94.2 -4.1     -61.1    60    31373           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 15 00  3C120        23 47 01  18.4  94.7 -4.8     -59.5     1    31373   06 15 00
06 21 40  ---          23 53 42  19.9  95.6 -4.7     -59.3   400    31476   06 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

06 22 00  3C120        23 54 02  19.9  95.7 -4.7     -59.3    14    31476   06 22 00
06 25 20  ---          23 57 23  20.7  96.1 -4.6     -59.2   200    31527   06 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 134
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 27 23  P-IKTAU      23 59 26  32.6  96.0 -3.9     -60.8    92    31527   Stopped 
06 28 23  ---          00 00 26  32.8  96.2 -3.9     -60.8    60    31527           

 ---------- Following scan added by Sched for reference pointing ----------

06 28 29  P-IKTAU      00 00 32  32.9  96.2 -3.9     -60.8     0    31527   Stopped 
06 29 29  ---          00 01 32  33.1  96.3 -3.9     -60.8    60    31527           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 30 00  3C120        00 02 04  21.7  96.8 -4.5     -59.1     1    31527   06 30 00
06 36 40  ---          00 08 45  23.1  97.7 -4.4     -58.9   400    31630   06 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

06 37 00  3C120        00 09 05  23.2  97.7 -4.4     -58.9    14    31630   06 37 00
06 40 20  ---          00 12 25  23.9  98.2 -4.4     -58.8   200    31681   06 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 42 23  P-IKTAU      00 14 28  35.8  98.2 -3.7     -60.3    92    31681   Stopped 
06 43 23  ---          00 15 29  36.0  98.4 -3.6     -60.3    60    31681           

 ---------- Following scan added by Sched for reference pointing ----------

06 43 29  P-IKTAU      00 15 35  36.1  98.4 -3.6     -60.3     0    31681   Stopped 
06 44 29  ---          00 16 35  36.3  98.5 -3.6     -60.2    60    31681           
Schedule for VLBA_FD   (Code Fd )                                   Page 135
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 45 00  3C120        00 17 06  24.9  98.9 -4.3     -58.6     1    31681   06 45 00
06 51 40  ---          00 23 47  26.3  99.8 -4.2     -58.4   400    31784   06 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

06 52 00  3C120        00 24 07  26.3  99.9 -4.2     -58.4    14    31784   06 52 00
06 55 20  ---          00 27 28  27.1 100.4 -4.1     -58.2   200    31835   06 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 57 16  P-IKTAU      00 29 24  39.0 100.5 -3.4     -59.7    85    31835   Stopped 
06 58 16  ---          00 30 24  39.2 100.7 -3.4     -59.6    60    31835           

 ---------- Following scan added by Sched for reference pointing ----------

06 58 22  P-IKTAU      00 30 30  39.2 100.7 -3.4     -59.6     0    31835   Stopped 
06 59 22  ---          00 31 30  39.4 100.9 -3.4     -59.6    60    31835           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 00 00  0420-014     00 32 09  26.4 108.9 -3.9     -54.5     4    31835   07 00 00
07 06 40  ---          00 38 50  27.8 110.0 -3.8     -54.0   400    31937   07 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

07 07 00  0420-014     00 39 10  27.8 110.0 -3.7     -54.0    14    31937   07 07 00
07 10 20  ---          00 42 30  28.5 110.6 -3.7     -53.7   200    31989   07 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page 136
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 12 23  P-IKTAU      00 44 33  42.2 103.0 -3.2     -58.8    88    31989   Stopped 
07 13 23  ---          00 45 33  42.4 103.2 -3.1     -58.7    60    31989           

 ---------- Following scan added by Sched for reference pointing ----------

07 13 29  P-IKTAU      00 45 39  42.4 103.2 -3.1     -58.7     0    31989   Stopped 
07 14 29  ---          00 46 40  42.6 103.4 -3.1     -58.7    60    31989           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 15 00  3C120        00 47 11  31.2 103.4 -3.8     -57.2     1    31989   07 15 00
07 21 40  ---          00 53 52  32.6 104.4 -3.7     -56.8   400    32091   07 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

07 22 00  3C120        00 54 12  32.7 104.5 -3.7     -56.8    14    32091   07 22 00
07 25 20  ---          00 57 33  33.4 105.0 -3.6     -56.6   200    32142   07 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 27 23  P-IKTAU      00 59 36  45.3 105.7 -2.9     -57.7    92    32142   Stopped 
07 28 23  ---          01 00 36  45.5 105.9 -2.9     -57.6    60    32142           

 ---------- Following scan added by Sched for reference pointing ----------

07 28 29  P-IKTAU      01 00 42  45.5 105.9 -2.9     -57.6     0    32142   Stopped 
07 29 29  ---          01 01 42  45.8 106.1 -2.9     -57.5    60    32142           
Schedule for VLBA_FD   (Code Fd )                                   Page 137
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 30 00  3C120        01 02 14  34.3 105.8 -3.5     -56.3     1    32142   07 30 00
07 36 40  ---          01 08 55  35.7 106.9 -3.4     -55.8   400    32245   07 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

07 37 00  3C120        01 09 15  35.8 107.0 -3.4     -55.7    14    32245   07 37 00
07 40 20  ---          01 12 35  36.5 107.6 -3.4     -55.5   200    32296   07 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 42 23  P-IKTAU      01 14 38  48.4 108.6 -2.7     -56.3    92    32296   Stopped 
07 43 23  ---          01 15 38  48.6 108.9 -2.6     -56.2    60    32296           

 ---------- Following scan added by Sched for reference pointing ----------

07 43 29  P-IKTAU      01 15 44  48.6 108.9 -2.6     -56.2     0    32296   Stopped 
07 44 29  ---          01 16 45  48.8 109.1 -2.6     -56.1    60    32296           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 45 00  3C120        01 17 16  37.4 108.4 -3.3     -55.1     1    32296   07 45 00
07 51 40  ---          01 23 57  38.8 109.6 -3.2     -54.5   400    32399   07 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

07 52 00  3C120        01 24 17  38.9 109.7 -3.2     -54.5    14    32399   07 52 00
07 55 20  ---          01 27 38  39.5 110.3 -3.1     -54.1   200    32450   07 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 138
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 57 15  P-IKTAU      01 29 33  51.4 111.9 -2.4     -54.6    85    32450   Stopped 
07 58 15  ---          01 30 34  51.6 112.1 -2.4     -54.4    60    32450           

 ---------- Following scan added by Sched for reference pointing ----------

07 58 21  P-IKTAU      01 30 40  51.6 112.1 -2.4     -54.4     0    32450   Stopped 
07 59 21  ---          01 31 40  51.8 112.4 -2.4     -54.3    60    32450           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 00 00  0420-014     01 32 18  38.2 120.0 -2.9     -48.2     4    32450   08 00 00
08 06 40  ---          01 39 00  39.4 121.4 -2.8     -47.3   400    32553   08 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 07 00  0420-014     01 39 20  39.5 121.5 -2.7     -47.2    14    32553   08 07 00
08 10 20  ---          01 42 40  40.1 122.2 -2.7     -46.7   200    32604   08 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 12 23  P-IKTAU      01 44 43  54.4 115.5 -2.2     -52.4    87    32604   Stopped 
08 13 23  ---          01 45 43  54.6 115.8 -2.1     -52.2    60    32604           

 ---------- Following scan added by Sched for reference pointing ----------

08 13 29  P-IKTAU      01 45 49  54.6 115.8 -2.1     -52.2     0    32604   Stopped 
08 14 29  ---          01 46 50  54.8 116.1 -2.1     -52.0    60    32604           
Schedule for VLBA_FD   (Code Fd )                                   Page 139
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 15 00  3C120        01 47 21  43.5 114.3 -2.8     -52.0     1    32604   08 15 00
08 21 40  ---          01 54 02  44.8 115.7 -2.7     -51.1   400    32707   08 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 22 00  3C120        01 54 22  44.8 115.8 -2.7     -51.1    14    32707   08 22 00
08 25 20  ---          01 57 43  45.5 116.5 -2.6     -50.7   200    32758   08 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 27 23  P-IKTAU      01 59 46  57.3 119.7 -1.9     -49.7    92    32758   Stopped 
08 28 23  ---          02 00 46  57.5 120.0 -1.9     -49.5    60    32758           

 ---------- Following scan added by Sched for reference pointing ----------

08 28 29  P-IKTAU      02 00 52  57.5 120.0 -1.9     -49.5     0    32758   Stopped 
08 29 29  ---          02 01 52  57.7 120.3 -1.9     -49.3    60    32758           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 30 00  3C120        02 02 23  46.4 117.6 -2.5     -50.0     1    32758   08 30 00
08 36 40  ---          02 09 04  47.6 119.2 -2.4     -49.0   400    32860   08 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 37 00  3C120        02 09 25  47.7 119.3 -2.4     -48.9    14    32860   08 37 00
08 40 20  ---          02 12 45  48.3 120.1 -2.4     -48.4   200    32912   08 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 140
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 42 23  P-IKTAU      02 14 48  60.0 124.4 -1.7     -46.4    92    32912   Stopped 
08 43 23  ---          02 15 48  60.2 124.7 -1.6     -46.2    60    32912           

 ---------- Following scan added by Sched for reference pointing ----------

08 43 29  P-IKTAU      02 15 55  60.2 124.8 -1.6     -46.1     0    32912   Stopped 
08 44 29  ---          02 16 55  60.4 125.1 -1.6     -45.9    60    32912           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 45 00  3C120        02 17 26  49.2 121.3 -2.3     -47.6     1    32912   08 45 00
08 51 40  ---          02 24 07  50.4 123.0 -2.2     -46.4   400    33014   08 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 52 00  3C120        02 24 27  50.5 123.1 -2.2     -46.4    14    33014   08 52 00
08 55 20  ---          02 27 48  51.1 124.0 -2.1     -45.8   200    33066   08 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 57 16  P-IKTAU      02 29 44  62.6 129.8 -1.4     -42.4    86    33066   Stopped 
08 58 16  ---          02 30 44  62.7 130.2 -1.4     -42.1    60    33066           

 ---------- Following scan added by Sched for reference pointing ----------

08 58 22  P-IKTAU      02 30 50  62.8 130.3 -1.4     -42.0     0    33066   Stopped 
08 59 22  ---          02 31 51  62.9 130.7 -1.4     -41.7    60    33066           
Schedule for VLBA_FD   (Code Fd )                                   Page 141
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 00 00  0420-014     02 32 28  48.5 135.1 -1.9     -37.4     1    33066   09 00 00
09 06 40  ---          02 39 09  49.5 137.2 -1.7     -35.8   400    33168   09 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 07 00  0420-014     02 39 29  49.5 137.3 -1.7     -35.7    14    33168   09 07 00
09 10 20  ---          02 42 50  50.0 138.3 -1.7     -34.9   200    33219   09 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 12 23  P-IKTAU      02 44 54  65.0 136.3 -1.2     -37.3    86    33219   Stopped 
09 13 23  ---          02 45 54  65.1 136.8 -1.1     -37.0    60    33219           

 ---------- Following scan added by Sched for reference pointing ----------

09 13 29  P-IKTAU      02 46 00  65.1 136.8 -1.1     -36.9     0    33219   Stopped 
09 14 29  ---          02 47 00  65.3 137.3 -1.1     -36.6    60    33219           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 15 00  3C120        02 47 31  54.5 129.9 -1.8     -41.5     1    33219   09 15 00
09 21 40  ---          02 54 12  55.5 132.1 -1.7     -39.9   400    33322   09 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 22 00  3C120        02 54 32  55.6 132.2 -1.7     -39.8    14    33322   09 22 00
09 25 20  ---          02 57 52  56.1 133.3 -1.6     -38.9   200    33373   09 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 142
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 27 16  P-IKTAU      02 59 49  67.0 143.7 -0.9     -31.3    87    33373   Stopped 
09 28 16  ---          03 00 49  67.2 144.3 -0.9     -30.8    60    33373           

 ---------- Following scan added by Sched for reference pointing ----------

09 28 22  P-IKTAU      03 00 55  67.2 144.3 -0.9     -30.8     0    33373   Stopped 
09 29 22  ---          03 01 55  67.3 144.9 -0.9     -30.3    60    33373           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 30 00  0420-014     03 02 33  52.6 145.0 -1.4     -29.6     1    33373   09 30 00
09 36 40  ---          03 09 14  53.4 147.5 -1.2     -27.6   400    33476   09 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 37 00  0420-014     03 09 34  53.5 147.6 -1.2     -27.5    14    33476   09 37 00
09 40 20  ---          03 12 55  53.9 148.8 -1.2     -26.4   200    33527   09 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 42 24  P-IKTAU      03 14 59  68.8 152.5 -0.7     -23.9    87    33527   Stopped 
09 43 24  ---          03 16 00  68.9 153.1 -0.6     -23.4    60    33527           

 ---------- Following scan added by Sched for reference pointing ----------

09 43 30  P-IKTAU      03 16 06  68.9 153.2 -0.6     -23.3     0    33527   Stopped 
09 44 30  ---          03 17 06  69.0 153.8 -0.6     -22.8    60    33527           
Schedule for VLBA_FD   (Code Fd )                                   Page 143
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 45 00  3C120        03 17 36  59.0 140.7 -1.3     -33.1     2    33527   09 45 00
09 51 40  ---          03 24 17  59.9 143.5 -1.2     -30.9   400    33630   09 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 52 00  3C120        03 24 37  59.9 143.7 -1.2     -30.8    14    33630   09 52 00
09 55 20  ---          03 27 57  60.4 145.1 -1.1     -29.6   200    33681   09 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 57 18  P-ORINEW2    03 29 56  43.1 134.6 -2.1     -38.0    75    33681   Stopped 
09 58 18  =ORIIRC2     03 30 56  43.2 134.9 -2.1     -37.8    60    33681           

 ---------- Following scan added by Sched for reference pointing ----------

09 58 24  P-ORINEW2    03 31 02  43.2 134.9 -2.1     -37.8     0    33681   Stopped 
09 59 24  =ORIIRC2     03 32 02  43.4 135.2 -2.1     -37.5    60    33681           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 00 00  0420-014     03 32 38  55.8 156.7 -0.9     -19.9     4    33681   10 00 00
10 06 40  ---          03 39 19  56.3 159.5 -0.7     -17.5   400    33783   10 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 07 00  0420-014     03 39 39  56.4 159.7 -0.7     -17.4    14    33783   10 07 00
10 10 20  ---          03 43 00  56.6 161.1 -0.7     -16.2   200    33835   10 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page 144
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 12 26  P-IKTAU      03 45 06  70.7 173.2 -0.2      -6.0    90    33835   Stopped 
10 13 26  ---          03 46 06  70.7 173.9 -0.1      -5.4    60    33835           

 ---------- Following scan added by Sched for reference pointing ----------

10 13 32  P-IKTAU      03 46 12  70.7 174.0 -0.1      -5.3     0    33835   Stopped 
10 14 32  ---          03 47 13  70.7 174.7 -0.1      -4.6    60    33835           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 15 00  3C120        03 47 41  62.5 154.4 -0.8     -22.0     4    33835   10 15 00
10 21 40  ---          03 54 22  63.1 157.8 -0.7     -19.1   400    33937   10 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 22 00  3C120        03 54 42  63.1 157.9 -0.7     -18.9    14    33937   10 22 00
10 25 20  ---          03 58 02  63.4 159.7 -0.6     -17.4   200    33989   10 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 29 35  P-RCNC       04 02 18  28.4  93.0 -4.3     -61.3   177    33989   Stopped 
10 30 35  ---          04 03 18  28.6  93.2 -4.2     -61.3    60    33989           

 ---------- Following scan added by Sched for reference pointing ----------

10 30 41  P-RCNC       04 03 24  28.6  93.2 -4.2     -61.3     0    33989   Stopped 
10 31 41  ---          04 04 25  28.9  93.3 -4.2     -61.3    60    33989           
Schedule for VLBA_FD   (Code Fd )                                   Page 145
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 32 00  OJ287        04 04 43  24.5  80.3 -4.8     -64.5     2    33989   10 32 00
10 38 40  ---          04 11 25  25.9  81.1 -4.7     -64.8   400    34091   10 32 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 39 00  OJ287        04 11 45  26.0  81.1 -4.7     -64.8    14    34091   10 39 00
10 42 20  ---          04 15 05  26.7  81.5 -4.7     -64.9   200    34142   10 39 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 43 41  P-RCNC       04 16 26  31.4  94.9 -4.0     -61.1    63    34142   Stopped 
10 44 41  ---          04 17 26  31.6  95.1 -4.0     -61.1    60    34142           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 45 00  OJ287        04 17 46  27.3  81.8 -4.6     -65.0     2    34142   10 45 00
10 51 40  ---          04 24 27  28.7  82.5 -4.5     -65.3   400    34245   10 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 52 00  OJ287        04 24 47  28.8  82.6 -4.5     -65.3    14    34245   10 52 00
10 55 20  ---          04 28 07  29.5  82.9 -4.5     -65.4   200    34296   10 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 146
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 57 34  P-RCNC       04 30 22  34.4  96.9 -3.8     -60.7   117    34296   Stopped 
10 58 34  ---          04 31 22  34.6  97.1 -3.8     -60.7    60    34296           

 ---------- Following scan added by Sched for reference pointing ----------

10 58 40  P-RCNC       04 31 28  34.6  97.1 -3.8     -60.7     0    34296   Stopped 
10 59 40  ---          04 32 28  34.9  97.2 -3.7     -60.6    60    34296           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 00 00  OJ287        04 32 48  30.5  83.5 -4.4     -65.5     2    34296   11 00 00
11 06 40  ---          04 39 29  31.9  84.2 -4.3     -65.7   400    34399   11 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 07 00  OJ287        04 39 49  32.0  84.3 -4.3     -65.7    14    34399   11 07 00
11 10 20  ---          04 43 10  32.7  84.6 -4.2     -65.8   200    34450   11 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 12 34  P-RCNC       04 45 24  37.6  99.2 -3.5     -60.2   116    34450   Stopped 
11 13 34  ---          04 46 24  37.8  99.3 -3.5     -60.1    60    34450           

 ---------- Following scan added by Sched for reference pointing ----------

11 13 40  P-RCNC       04 46 30  37.8  99.3 -3.5     -60.1     0    34450   Stopped 
11 14 40  ---          04 47 30  38.1  99.5 -3.5     -60.1    60    34450           
Schedule for VLBA_FD   (Code Fd )                                   Page 147
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 15 00  OJ287        04 47 51  33.7  85.2 -4.1     -65.9     2    34450   11 15 00
11 21 40  ---          04 54 32  35.1  86.0 -4.0     -66.0   400    34553   11 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 22 00  OJ287        04 54 52  35.2  86.0 -4.0     -66.0    14    34553   11 22 00
11 25 20  ---          04 58 12  35.9  86.4 -4.0     -66.1   200    34604   11 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 27 33  P-RCNC       05 00 26  40.8 101.6 -3.3     -59.4   115    34604   Stopped 
11 28 33  ---          05 01 26  41.0 101.7 -3.3     -59.4    60    34604           

 ---------- Following scan added by Sched for reference pointing ----------

11 28 39  P-RCNC       05 01 32  41.0 101.7 -3.3     -59.3     0    34604   Stopped 
11 29 39  ---          05 02 32  41.2 101.9 -3.2     -59.3    60    34604           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 30 00  OJ287        05 02 53  36.9  86.9 -3.9     -66.2     2    34604   11 30 00
11 36 40  ---          05 09 34  38.4  87.7 -3.8     -66.2   400    34707   11 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 37 00  OJ287        05 09 54  38.4  87.8 -3.8     -66.2    14    34707   11 37 00
11 40 20  ---          05 13 15  39.1  88.2 -3.7     -66.3   200    34758   11 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 148
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 42 33  P-RCNC       05 15 28  43.9 104.1 -3.0     -58.4   114    34758   Stopped 
11 43 33  ---          05 16 28  44.2 104.3 -3.0     -58.4    60    34758           

 ---------- Following scan added by Sched for reference pointing ----------

11 43 39  P-RCNC       05 16 34  44.2 104.3 -3.0     -58.4     0    34758   Stopped 
11 44 39  ---          05 17 34  44.4 104.5 -3.0     -58.3    60    34758           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 45 00  OJ287        05 17 55  40.2  88.8 -3.6     -66.3     2    34758   11 45 00
11 51 40  ---          05 24 37  41.6  89.6 -3.5     -66.3   400    34860   11 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 52 00  OJ287        05 24 57  41.7  89.6 -3.5     -66.3    14    34860   11 52 00
11 55 20  ---          05 28 17  42.4  90.1 -3.5     -66.3   200    34912   11 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 57 32  P-RCNC       05 30 29  47.1 106.9 -2.8     -57.2   112    34912   Stopped 
11 58 32  ---          05 31 29  47.3 107.1 -2.8     -57.1    60    34912           

 ---------- Following scan added by Sched for reference pointing ----------

11 58 38  P-RCNC       05 31 36  47.3 107.1 -2.8     -57.1     0    34912   Stopped 
11 59 38  ---          05 32 36  47.5 107.3 -2.7     -57.0    60    34912           
Schedule for VLBA_FD   (Code Fd )                                   Page 149
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 00 00  OJ287        05 32 58  43.4  90.7 -3.4     -66.3     2    34912   12 00 00
12 06 40  ---          05 39 39  44.8  91.5 -3.3     -66.3   400    35014   12 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 07 00  OJ287        05 39 59  44.9  91.6 -3.3     -66.3    14    35014   12 07 00
12 10 20  ---          05 43 20  45.6  92.0 -3.2     -66.3   200    35066   12 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 12 31  P-RCNC       05 45 31  50.1 110.0 -2.5     -55.7   111    35066   Stopped 
12 13 31  ---          05 46 31  50.3 110.2 -2.5     -55.5    60    35066           

 ---------- Following scan added by Sched for reference pointing ----------

12 13 37  P-RCNC       05 46 37  50.4 110.2 -2.5     -55.5     0    35066   Stopped 
12 14 37  ---          05 47 37  50.6 110.5 -2.5     -55.4    60    35066           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 15 00  OJ287        05 48 00  46.6  92.7 -3.1     -66.2     2    35066   12 15 00
12 21 40  ---          05 54 41  48.1  93.6 -3.0     -66.1   400    35168   12 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 22 00  OJ287        05 55 02  48.1  93.7 -3.0     -66.1    14    35168   12 22 00
12 25 20  ---          05 58 22  48.9  94.1 -3.0     -66.0   200    35219   12 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 150
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 27 30  P-RCNC       06 00 33  53.1 113.4 -2.3     -53.7   109    35219   Stopped 
12 28 30  ---          06 01 33  53.3 113.7 -2.3     -53.6    60    35219           

 ---------- Following scan added by Sched for reference pointing ----------

12 28 36  P-RCNC       06 01 39  53.3 113.7 -2.3     -53.6     0    35219   Stopped 
12 29 36  ---          06 02 39  53.5 113.9 -2.2     -53.4    60    35219           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 30 00  OJ287        06 03 03  49.9  94.8 -2.9     -65.9     2    35219   12 30 00
12 36 40  ---          06 09 44  51.3  95.8 -2.8     -65.7   400    35322   12 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 37 00  OJ287        06 10 04  51.4  95.9 -2.8     -65.7    14    35322   12 37 00
12 40 20  ---          06 13 25  52.1  96.4 -2.7     -65.5   200    35373   12 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 42 30  P-RCNC       06 15 35  56.1 117.3 -2.0     -51.3   107    35373   Stopped 
12 43 30  ---          06 16 35  56.2 117.6 -2.0     -51.2    60    35373           

 ---------- Following scan added by Sched for reference pointing ----------

12 43 36  P-RCNC       06 16 41  56.3 117.6 -2.0     -51.1     0    35373   Stopped 
12 44 36  ---          06 17 41  56.5 117.9 -2.0     -51.0    60    35373           
Schedule for VLBA_FD   (Code Fd )                                   Page 151
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 45 00  OJ287        06 18 05  53.1  97.2 -2.6     -65.3     2    35373   12 45 00
12 51 40  ---          06 24 46  54.5  98.3 -2.5     -65.0   400    35476   12 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 52 00  OJ287        06 25 06  54.6  98.3 -2.5     -65.0    14    35476   12 52 00
12 55 20  ---          06 28 27  55.3  98.9 -2.5     -64.8   200    35527   12 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 57 29  P-RCNC       06 30 36  58.9 121.7 -1.8     -48.4   105    35527   Stopped 
12 58 29  ---          06 31 37  59.1 122.0 -1.8     -48.2    60    35527           

 ---------- Following scan added by Sched for reference pointing ----------

12 58 35  P-RCNC       06 31 43  59.1 122.0 -1.8     -48.1     0    35527   Stopped 
12 59 35  ---          06 32 43  59.3 122.4 -1.7     -47.9    60    35527           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 00 00  OJ287        06 33 08  56.3  99.8 -2.4     -64.5     1    35527   13 00 00
13 06 40  ---          06 39 49  57.7 101.0 -2.3     -64.0   400    35630   13 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 07 00  OJ287        06 40 09  57.8 101.1 -2.3     -64.0    14    35630   13 07 00
13 10 20  ---          06 43 29  58.5 101.7 -2.2     -63.7   200    35681   13 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page 152
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 12 28  P-RCNC       06 45 38  61.5 126.8 -1.5     -44.7   103    35681   Stopped 
13 13 28  ---          06 46 38  61.7 127.2 -1.5     -44.4    60    35681           

 ---------- Following scan added by Sched for reference pointing ----------

13 13 34  P-RCNC       06 46 44  61.7 127.2 -1.5     -44.4     0    35681   Stopped 
13 14 34  ---          06 47 45  61.9 127.6 -1.5     -44.1    60    35681           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 15 00  OJ287        06 48 10  59.4 102.7 -2.1     -63.3     0    35681   13 15 00
13 21 00  ---          06 54 11  60.7 104.0 -2.0     -62.7   360    35773   13 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 21 20  OJ287        06 54 31  60.8 104.0 -2.0     -62.7    14    35773   13 21 20
13 24 40  ---          06 57 52  61.5 104.8 -2.0     -62.3   200    35824   13 21 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 27 15  P-TXCAM      07 00 27  57.1 -30.4  2.0     128.5    51    35824   Stopped 
13 28 15  ---          07 01 28  57.0 -30.5  2.0     128.2    60    35824           

 ---------- Following scan added by Sched for reference pointing ----------

13 28 21  P-TXCAM      07 01 34  57.0 -30.6  2.0     128.2     0    35824   Stopped 
13 29 21  ---          07 02 34  56.9 -30.7  2.0     127.8    60    35824           
Schedule for VLBA_FD   (Code Fd )                                   Page 153
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 30 00  0716+714     07 03 13  49.2   2.5 -0.3    -173.3     7    35824   13 30 00
13 36 40  ---          07 09 54  49.3   1.7 -0.2    -175.5   400    35927   13 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 37 00  0716+714     07 10 14  49.3   1.6 -0.2    -175.6    14    35927   13 37 00
13 40 20  ---          07 13 34  49.3   1.2 -0.2    -176.7   200    35978   13 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 42 16  P-TXCAM      07 15 31  55.4 -32.6  2.2     123.6    85    35978   Stopped 
13 43 16  ---          07 16 31  55.3 -32.7  2.2     123.2    60    35978           

 ---------- Following scan added by Sched for reference pointing ----------

13 43 22  P-TXCAM      07 16 37  55.3 -32.8  2.2     123.2     0    35978   Stopped 
13 44 22  ---          07 17 38  55.2 -32.9  2.3     122.9    60    35978           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 45 00  0716+714     07 18 15  49.3   0.6 -0.1    -178.3     6    35978   13 45 00
13 51 40  ---          07 24 56  49.3  -0.2  0.0     179.5   400    36081   13 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 52 00  0716+714     07 25 16  49.3  -0.2  0.0     179.4    14    36081   13 52 00
13 55 20  ---          07 28 37  49.3  -0.6  0.1     178.3   200    36132   13 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 154
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 57 09  P-TXCAM      07 30 26  53.6 -34.5  2.5     118.9    77    36132   Stopped 
13 58 09  ---          07 31 26  53.5 -34.6  2.5     118.6    60    36132           

 ---------- Following scan added by Sched for reference pointing ----------

13 58 15  P-TXCAM      07 31 32  53.5 -34.6  2.5     118.6     0    36132   Stopped 
13 59 15  ---          07 32 32  53.4 -34.7  2.5     118.3    60    36132           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 00 00  0836+710     07 33 18  48.7   8.5 -1.2    -157.1     7    36132   14 00 00
14 06 40  ---          07 39 59  48.9   7.8 -1.0    -159.2   400    36235   14 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 07 00  0836+710     07 40 19  48.9   7.7 -1.0    -159.4    14    36235   14 07 00
14 10 20  ---          07 43 39  49.0   7.3 -1.0    -160.4   200    36286   14 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 12 19  P-TXCAM      07 45 38  51.8 -36.0  2.7     114.5    80    36286   Stopped 
14 13 19  ---          07 46 38  51.6 -36.1  2.7     114.3    60    36286           

 ---------- Following scan added by Sched for reference pointing ----------

14 13 25  P-TXCAM      07 46 44  51.6 -36.1  2.7     114.2     0    36286   Stopped 
14 14 25  ---          07 47 45  51.5 -36.2  2.8     113.9    60    36286           
Schedule for VLBA_FD   (Code Fd )                                   Page 155
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 15 00  0716+714     07 48 20  49.2  -3.0  0.4     171.8     4    36286   14 15 00
14 21 40  ---          07 55 01  49.1  -3.8  0.5     169.6   400    36389   14 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 22 00  0716+714     07 55 21  49.1  -3.9  0.5     169.5    14    36389   14 22 00
14 25 20  ---          07 58 42  49.0  -4.3  0.6     168.4   200    36440   14 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 27 19  P-TXCAM      08 00 41  49.8 -37.3  3.0     110.4    88    36440   Stopped 
14 28 19  ---          08 01 42  49.7 -37.4  3.0     110.2    60    36440           

 ---------- Following scan added by Sched for reference pointing ----------

14 28 25  P-TXCAM      08 01 48  49.7 -37.4  3.0     110.1     0    36440   Stopped 
14 29 25  ---          08 02 48  49.5 -37.5  3.0     109.9    60    36440           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 30 00  0716+714     08 03 23  49.0  -4.8  0.7     166.9     4    36440   14 30 00
14 36 40  ---          08 10 04  48.8  -5.6  0.8     164.7   400    36542   14 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 37 00  0716+714     08 10 24  48.8  -5.7  0.8     164.6    14    36542   14 37 00
14 40 20  ---          08 13 44  48.8  -6.1  0.8     163.5   200    36594   14 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 156
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 42 20  P-TXCAM      08 15 45  47.8 -38.3  3.2     106.5    89    36594   Stopped 
14 43 20  ---          08 16 45  47.7 -38.4  3.2     106.3    60    36594           

 ---------- Following scan added by Sched for reference pointing ----------

14 43 26  P-TXCAM      08 16 51  47.7 -38.4  3.2     106.3     0    36594   Stopped 
14 44 26  ---          08 17 51  47.6 -38.4  3.3     106.0    60    36594           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 45 00  0716+714     08 18 25  48.6  -6.6  0.9     162.0     3    36594   14 45 00
14 51 40  ---          08 25 06  48.5  -7.4  1.0     159.9   400    36696   14 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 52 00  0716+714     08 25 26  48.5  -7.4  1.0     159.7    14    36696   14 52 00
14 55 20  ---          08 28 47  48.4  -7.8  1.1     158.7   200    36748   14 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 57 13  P-TXCAM      08 30 40  45.8 -39.1  3.5     102.9    83    36748   Stopped 
14 58 13  ---          08 31 40  45.7 -39.1  3.5     102.6    60    36748           

 ---------- Following scan added by Sched for reference pointing ----------

14 58 19  P-TXCAM      08 31 46  45.7 -39.1  3.5     102.6     0    36748   Stopped 
14 59 19  ---          08 32 46  45.5 -39.2  3.5     102.4    60    36748           
Schedule for VLBA_FD   (Code Fd )                                   Page 157
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 00 00  0836+710     08 33 27  49.8   1.2 -0.2    -176.9     4    36748   15 00 00
15 06 40  ---          08 40 09  49.8   0.3 -0.0    -179.1   400    36850   15 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 07 00  0836+710     08 40 29  49.8   0.3 -0.0    -179.2    14    36850   15 07 00
15 10 20  ---          08 43 49  49.8  -0.1  0.0     179.7   200    36901   15 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 12 22  P-TXCAM      08 45 51  43.8 -39.6  3.7      99.3    86    36901   Stopped 
15 13 22  ---          08 46 52  43.6 -39.7  3.7      99.1    60    36901           

 ---------- Following scan added by Sched for reference pointing ----------

15 13 28  P-TXCAM      08 46 58  43.6 -39.7  3.7      99.1     0    36901   Stopped 
15 14 28  ---          08 47 58  43.5 -39.7  3.8      98.8    60    36901           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 15 00  0716+714     08 48 30  47.7  -9.9  1.4     152.4     3    36901   15 15 00
15 21 40  ---          08 55 11  47.4 -10.6  1.5     150.3   400    37004   15 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 22 00  0716+714     08 55 31  47.4 -10.7  1.5     150.2    14    37004   15 22 00
15 25 20  ---          08 58 52  47.3 -11.0  1.6     149.2   200    37055   15 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 158
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 27 20  P-TXCAM      09 00 52  41.7 -40.0  4.0      95.9    91    37055   Stopped 
15 28 20  ---          09 01 52  41.5 -40.0  4.0      95.7    60    37055           

 ---------- Following scan added by Sched for reference pointing ----------

15 28 26  P-TXCAM      09 01 58  41.5 -40.0  4.0      95.7     0    37055   Stopped 
15 29 26  ---          09 02 58  41.4 -40.1  4.0      95.5    60    37055           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 30 00  0716+714     09 03 32  47.1 -11.5  1.7     147.7     6    37055   15 30 00
15 36 40  ---          09 10 13  46.8 -12.1  1.8     145.6   400    37158   15 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 37 00  0716+714     09 10 34  46.8 -12.2  1.8     145.5    14    37158   15 37 00
15 40 20  ---          09 13 54  46.6 -12.5  1.8     144.5   200    37209   15 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 42 18  P-TXCAM      09 15 52  39.6 -40.2  4.2      92.7    90    37209   Stopped 
15 43 18  ---          09 16 52  39.5 -40.2  4.2      92.5    60    37209           

 ---------- Following scan added by Sched for reference pointing ----------

15 43 24  P-TXCAM      09 16 58  39.4 -40.2  4.2      92.5     0    37209   Stopped 
15 44 24  ---          09 17 58  39.3 -40.2  4.3      92.2    60    37209           
Schedule for VLBA_FD   (Code Fd )                                   Page 159
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 45 00  0716+714     09 18 35  46.4 -12.9  1.9     143.1     9    37209   15 45 00
15 51 40  ---          09 25 16  46.1 -13.5  2.0     141.1   400    37312   15 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 52 00  0716+714     09 25 36  46.1 -13.6  2.0     141.0    14    37312   15 52 00
15 55 20  ---          09 28 57  45.9 -13.9  2.1     140.0   200    37363   15 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 57 05  P-TXCAM      09 30 42  37.5 -40.3  4.5      89.6    78    37363   Stopped 
15 58 05  ---          09 31 42  37.4 -40.3  4.5      89.4    60    37363           

 ---------- Following scan added by Sched for reference pointing ----------

15 58 11  P-TXCAM      09 31 48  37.4 -40.3  4.5      89.4     0    37363   Stopped 
15 59 11  ---          09 32 48  37.2 -40.3  4.5      89.1    60    37363           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 00 00  0836+710     09 33 37  49.2  -6.3  0.8     163.2    17    37363   16 00 00
16 06 40  ---          09 40 18  49.0  -7.1  1.0     161.0   400    37465   16 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 07 00  0836+710     09 40 38  49.0  -7.2  1.0     160.9    14    37465   16 07 00
16 10 20  ---          09 43 59  48.9  -7.6  1.0     159.8   200    37517   16 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page 160
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 12 14  P-TXCAM      09 45 53  35.4 -40.2  4.7      86.5    80    37517   Stopped 
16 13 14  ---          09 46 53  35.3 -40.2  4.7      86.3    60    37517           

 ---------- Following scan added by Sched for reference pointing ----------

16 13 20  P-TXCAM      09 46 59  35.3 -40.2  4.7      86.3     0    37517   Stopped 
16 14 20  ---          09 48 00  35.1 -40.2  4.8      86.1    60    37517           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 15 00  0716+714     09 48 40  44.8 -15.5  2.4     134.1    13    37517   16 15 00
16 21 40  ---          09 55 21  44.4 -16.0  2.5     132.2   400    37619   16 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 22 00  0716+714     09 55 41  44.4 -16.0  2.5     132.1    14    37619   16 22 00
16 25 20  ---          09 59 01  44.2 -16.3  2.6     131.1   200    37671   16 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 27 12  P-TXCAM      10 00 54  33.3 -40.0  5.0      83.5    83    37671   Stopped 
16 28 12  ---          10 01 54  33.2 -40.0  5.0      83.3    60    37671           

 ---------- Following scan added by Sched for reference pointing ----------

16 28 18  P-TXCAM      10 02 00  33.2 -39.9  5.0      83.3     0    37671   Stopped 
16 29 18  ---          10 03 00  33.1 -39.9  5.0      83.1    60    37671           
Schedule for VLBA_FD   (Code Fd )                                   Page 161
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 30 00  0716+714     10 03 42  43.9 -16.6  2.7     129.8    12    37671   16 30 00
16 36 40  ---          10 10 23  43.5 -17.1  2.8     127.9   400    37773   16 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 37 00  0716+714     10 10 43  43.5 -17.1  2.8     127.8    14    37773   16 37 00
16 40 20  ---          10 14 04  43.3 -17.3  2.8     126.8   200    37824   16 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 42 11  P-TXCAM      10 15 55  31.3 -39.6  5.2      80.5    79    37824   Stopped 
16 43 11  ---          10 16 55  31.1 -39.6  5.2      80.4    60    37824           

 ---------- Following scan added by Sched for reference pointing ----------

16 43 17  P-TXCAM      10 17 01  31.1 -39.6  5.2      80.3     0    37824   Stopped 
16 44 17  ---          10 18 01  31.0 -39.6  5.3      80.1    60    37824           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 45 00  0716+714     10 18 45  43.0 -17.6  2.9     125.5    12    37824   16 45 00
16 51 40  ---          10 25 26  42.5 -18.1  3.0     123.6   400    37927   16 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 52 00  0716+714     10 25 46  42.5 -18.1  3.0     123.6    14    37927   16 52 00
16 55 20  ---          10 29 06  42.3 -18.3  3.1     122.6   200    37978   16 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 162
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 56 57  P-TXCAM      10 30 43  29.3 -39.2  5.5      77.7    63    37978   Stopped 
16 57 57  ---          10 31 43  29.1 -39.1  5.5      77.5    60    37978           

 ---------- Following scan added by Sched for reference pointing ----------

16 58 03  P-TXCAM      10 31 50  29.1 -39.1  5.5      77.5     0    37978   Stopped 
16 59 03  ---          10 32 50  29.0 -39.1  5.5      77.3    60    37978           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 00 00  0836+710     10 33 47  47.0 -12.9  1.8     144.0    14    37978   17 00 00
17 06 40  ---          10 40 28  46.7 -13.6  2.0     142.0   400    38081   17 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 07 00  0836+710     10 40 48  46.7 -13.6  2.0     141.9    14    38081   17 07 00
17 10 20  ---          10 44 09  46.5 -13.9  2.0     140.9   200    38132   17 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 12 08  P-TXCAM      10 45 57  27.2 -38.6  5.7      74.8    62    38132   Stopped 
17 13 08  ---          10 46 57  27.1 -38.6  5.7      74.6    60    38132           

 ---------- Following scan added by Sched for reference pointing ----------

17 13 14  P-TXCAM      10 47 03  27.1 -38.6  5.7      74.6     0    38132   Stopped 
17 14 14  ---          10 48 04  26.9 -38.5  5.8      74.4    60    38132           
Schedule for VLBA_FD   (Code Fd )                                   Page 163
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 15 00  0716+714     10 48 50  40.9 -19.3  3.4     117.3    10    38132   17 15 00
17 21 40  ---          10 55 31  40.4 -19.6  3.5     115.5   400    38235   17 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 22 00  0716+714     10 55 51  40.4 -19.7  3.5     115.4    14    38235   17 22 00
17 25 20  ---          10 59 11  40.2 -19.8  3.6     114.5   200    38286   17 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 27 07  P-TXCAM      11 00 59  25.2 -37.9  6.0      72.0    70    38286   Stopped 
17 28 07  ---          11 01 59  25.1 -37.9  6.0      71.8    60    38286           

 ---------- Following scan added by Sched for reference pointing ----------

17 28 13  P-TXCAM      11 02 05  25.1 -37.9  6.0      71.8     0    38286   Stopped 
17 29 13  ---          11 03 05  24.9 -37.8  6.0      71.6    60    38286           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 30 00  0716+714     11 03 52  39.8 -20.0  3.7     113.3    10    38286   17 30 00
17 36 40  ---          11 10 33  39.3 -20.3  3.8     111.5   400    38389   17 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 37 00  0716+714     11 10 53  39.3 -20.3  3.8     111.4    14    38389   17 37 00
17 40 20  ---          11 14 14  39.1 -20.4  3.8     110.5   200    38440   17 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 164
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 42 06  P-TXCAM      11 16 00  23.2 -37.2  6.2      69.2    67    38440   Stopped 
17 43 06  ---          11 17 00  23.1 -37.1  6.2      69.0    60    38440           

 ---------- Following scan added by Sched for reference pointing ----------

17 43 12  P-TXCAM      11 17 06  23.1 -37.1  6.2      69.0     0    38440   Stopped 
17 44 12  ---          11 18 06  23.0 -37.1  6.3      68.8    60    38440           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 45 00  0716+714     11 18 55  38.7 -20.6  3.9     109.3     9    38440   17 45 00
17 51 00  ---          11 24 56  38.3 -20.8  4.0     107.8   360    38532   17 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 51 20  0716+714     11 25 16  38.2 -20.8  4.0     107.7    14    38532   17 51 20
17 54 40  ---          11 28 36  38.0 -20.9  4.1     106.9   200    38583   17 51 21

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 01 27  P-RHYA       11 35 25  26.7 144.4 -2.3     -33.1   283    38583   Stopped 
18 02 27  ---          11 36 25  26.8 144.6 -2.3     -32.9    60    38583           

 ---------- Following scan added by Sched for reference pointing ----------

18 02 33  P-RHYA       11 36 31  26.8 144.6 -2.3     -32.9     0    38583   Stopped 
18 03 33  ---          11 37 31  26.9 144.8 -2.3     -32.7    60    38583           
Schedule for VLBA_FD   (Code Fd )                                   Page 165
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 04 00  1510-089     11 37 58  24.8 118.5 -3.6     -50.0     0    38583   18 04 00
18 10 40  ---          11 44 39  26.0 119.7 -3.5     -49.2   400    38686   18 04 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 11 00  1510-089     11 44 59  26.1 119.7 -3.5     -49.2    14    38686   18 11 00
18 14 20  ---          11 48 19  26.7 120.3 -3.4     -48.8   200    38737   18 11 01

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 15 00  1510-089     11 48 59  26.9 120.5 -3.4     -48.7    34    38737   18 15 00
18 21 40  ---          11 55 41  28.1 121.7 -3.3     -47.9   400    38840   18 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 22 00  1510-089     11 56 01  28.1 121.8 -3.3     -47.8    14    38840   18 22 00
18 25 20  ---          11 59 21  28.8 122.4 -3.2     -47.4   200    38891   18 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 27 27  P-RHYA       12 01 28  29.7 150.2 -1.9     -27.7    99    38891   Stopped 
18 28 27  ---          12 02 28  29.8 150.5 -1.9     -27.5    60    38891           

 ---------- Following scan added by Sched for reference pointing ----------

18 28 33  P-RHYA       12 02 34  29.8 150.5 -1.8     -27.5     0    38891   Stopped 
18 29 33  ---          12 03 34  29.9 150.7 -1.8     -27.3    60    38891           
Schedule for VLBA_FD   (Code Fd )                                   Page 166
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 30 00  1510-089     12 04 02  29.6 123.3 -3.2     -46.8     0    38891   18 30 00
18 36 40  ---          12 10 43  30.8 124.6 -3.0     -45.8   400    38994   18 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 37 00  1510-089     12 11 03  30.9 124.7 -3.0     -45.8    14    38994   18 37 00
18 40 20  ---          12 14 24  31.4 125.4 -3.0     -45.3   200    39045   18 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 42 26  P-RHYA       12 16 30  31.2 153.8 -1.6     -24.4    98    39045   Stopped 
18 43 26  ---          12 17 30  31.3 154.1 -1.6     -24.2    60    39045           

 ---------- Following scan added by Sched for reference pointing ----------

18 43 32  P-RHYA       12 17 36  31.3 154.1 -1.6     -24.2     0    39045   Stopped 
18 44 32  ---          12 18 37  31.4 154.3 -1.6     -23.9    60    39045           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 45 00  1510-089     12 19 04  32.3 126.3 -2.9     -44.6     0    39045   18 45 00
18 51 40  ---          12 25 46  33.4 127.7 -2.8     -43.6   400    39148   18 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 52 00  1510-089     12 26 06  33.5 127.8 -2.8     -43.5    14    39148   18 52 00
18 55 20  ---          12 29 26  34.0 128.5 -2.7     -43.0   200    39199   18 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 167
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 57 26  P-RHYA       12 31 32  32.6 157.6 -1.4     -21.0    98    39199   Stopped 
18 58 26  ---          12 32 32  32.6 157.8 -1.4     -20.7    60    39199           

 ---------- Following scan added by Sched for reference pointing ----------

18 58 32  P-RHYA       12 32 38  32.6 157.8 -1.3     -20.7     0    39199   Stopped 
18 59 32  ---          12 33 39  32.7 158.1 -1.3     -20.5    60    39199           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 00 00  1510-089     12 34 07  34.8 129.6 -2.7     -42.2     0    39199   19 00 00
19 06 40  ---          12 40 48  35.9 131.1 -2.5     -41.1   400    39301   19 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 07 00  1510-089     12 41 08  36.0 131.1 -2.5     -41.0    14    39301   19 07 00
19 10 20  ---          12 44 29  36.5 131.9 -2.5     -40.4   200    39353   19 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 12 25  P-RHYA       12 46 34  33.7 161.5 -1.1     -17.3    97    39353   Stopped 
19 13 25  ---          12 47 35  33.8 161.7 -1.1     -17.1    60    39353           

 ---------- Following scan added by Sched for reference pointing ----------

19 13 31  P-RHYA       12 47 41  33.8 161.7 -1.1     -17.1     0    39353   Stopped 
19 14 31  ---          12 48 41  33.8 162.0 -1.1     -16.8    60    39353           
Schedule for VLBA_FD   (Code Fd )                                   Page 168
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 15 00  1510-089     12 49 09  37.2 133.0 -2.4     -39.6     0    39353   19 15 00
19 21 40  ---          12 55 50  38.3 134.7 -2.3     -38.3   400    39455   19 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 22 00  1510-089     12 56 11  38.3 134.7 -2.3     -38.3    14    39455   19 22 00
19 25 20  ---          12 59 31  38.8 135.6 -2.2     -37.6   200    39506   19 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 27 23  P-RHYA       13 01 34  34.6 165.5 -0.9     -13.6    94    39506   Stopped 
19 28 23  ---          13 02 35  34.7 165.7 -0.8     -13.3    60    39506           

 ---------- Following scan added by Sched for reference pointing ----------

19 28 29  P-RHYA       13 02 41  34.7 165.8 -0.8     -13.3     0    39506   Stopped 
19 29 29  ---          13 03 41  34.7 166.0 -0.8     -13.1    60    39506           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 30 00  1510-089     13 04 12  39.5 136.8 -2.2     -36.7     2    39506   19 30 00
19 36 40  ---          13 10 53  40.5 138.5 -2.0     -35.3   400    39609   19 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 37 00  1510-089     13 11 13  40.6 138.6 -2.0     -35.2    14    39609   19 37 00
19 40 20  ---          13 14 34  41.0 139.5 -2.0     -34.5   200    39660   19 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 169
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 42 21  P-RHYA       13 16 35  35.3 169.6 -0.6      -9.8    92    39660   Stopped 
19 43 21  ---          13 17 35  35.3 169.9 -0.6      -9.5    60    39660           

 ---------- Following scan added by Sched for reference pointing ----------

19 43 27  P-RHYA       13 17 41  35.3 169.9 -0.6      -9.5     0    39660   Stopped 
19 44 27  ---          13 18 41  35.4 170.2 -0.6      -9.2    60    39660           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 45 00  1510-089     13 19 14  41.7 140.8 -1.9     -33.5     4    39660   19 45 00
19 51 40  ---          13 25 55  42.6 142.6 -1.8     -31.9   400    39763   19 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 52 00  1510-089     13 26 15  42.6 142.7 -1.8     -31.9    14    39763   19 52 00
19 55 20  ---          13 29 36  43.0 143.7 -1.7     -31.1   200    39814   19 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 57 18  P-RHYA       13 31 35  35.8 173.8 -0.4      -5.8    89    39814   Stopped 
19 58 18  ---          13 32 35  35.8 174.1 -0.3      -5.6    60    39814           

 ---------- Following scan added by Sched for reference pointing ----------

19 58 24  P-RHYA       13 32 41  35.8 174.1 -0.3      -5.5     0    39814   Stopped 
19 59 24  ---          13 33 41  35.8 174.4 -0.3      -5.3    60    39814           
Schedule for VLBA_FD   (Code Fd )                                   Page 170
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 00 00  1510-089     13 34 17  43.6 145.1 -1.7     -29.9     7    39814   20 00 00
20 06 40  ---          13 40 58  44.4 147.1 -1.5     -28.3   400    39917   20 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 07 00  1510-089     13 41 18  44.5 147.2 -1.5     -28.2    14    39917   20 07 00
20 10 20  ---          13 44 38  44.8 148.2 -1.5     -27.4   200    39968   20 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

20 12 16  P-RHYA       13 46 35  36.0 178.0 -0.1      -1.9    87    39968   Stopped 
20 13 16  ---          13 47 35  36.0 178.3 -0.1      -1.6    60    39968           

 ---------- Following scan added by Sched for reference pointing ----------

20 13 22  P-RHYA       13 47 41  36.0 178.3 -0.1      -1.6     0    39968   Stopped 
20 14 22  ---          13 48 41  36.0 178.6 -0.1      -1.3    60    39968           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 15 00  1510-089     13 49 19  45.4 149.6 -1.4     -26.1     9    39968   20 15 00
20 21 40  ---          13 56 00  46.1 151.8 -1.3     -24.3   400    40071   20 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 22 00  1510-089     13 56 20  46.1 151.9 -1.3     -24.2    14    40071   20 22 00
20 25 20  ---          13 59 41  46.4 153.0 -1.2     -23.3   200    40122   20 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 171
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

20 27 14  P-RHYA       14 01 35  36.0 182.3  0.1       2.1    85    40122   Stopped 
20 28 14  ---          14 02 35  36.0 182.6  0.2       2.4    60    40122           

 ---------- Following scan added by Sched for reference pointing ----------

20 28 20  P-RHYA       14 02 41  36.0 182.6  0.2       2.4     0    40122   Stopped 
20 29 20  ---          14 03 41  36.0 182.9  0.2       2.7    60    40122           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 30 00  1510-089     14 04 22  46.9 154.5 -1.2     -22.0    11    40122   20 30 00
20 36 40  ---          14 11 03  47.5 156.8 -1.0     -20.1   400    40224   20 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 37 00  1510-089     14 11 23  47.5 156.9 -1.0     -20.0    14    40224   20 37 00
20 40 20  ---          14 14 43  47.8 158.1 -1.0     -19.0   200    40276   20 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

20 42 12  P-RHYA       14 16 35  35.7 186.5  0.4       6.1    80    40276   Stopped 
20 43 12  ---          14 17 36  35.7 186.8  0.4       6.4    60    40276           

 ---------- Following scan added by Sched for reference pointing ----------

20 43 18  P-RHYA       14 17 42  35.7 186.8  0.4       6.4     0    40276   Stopped 
20 44 18  ---          14 18 42  35.7 187.1  0.4       6.7    60    40276           
Schedule for VLBA_FD   (Code Fd )                                   Page 172
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 45 00  1510-089     14 19 24  48.1 159.7 -0.9     -17.6    10    40276   20 45 00
20 51 40  ---          14 26 05  48.6 162.1 -0.8     -15.5   400    40378   20 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 52 00  1510-089     14 26 25  48.6 162.2 -0.8     -15.4    14    40378   20 52 00
20 55 20  ---          14 29 46  48.8 163.4 -0.7     -14.4   200    40430   20 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

20 57 10  P-RHYA       14 31 36  35.3 190.7  0.6      10.0    75    40430   Stopped 
20 58 10  ---          14 32 36  35.2 191.0  0.7      10.3    60    40430           

 ---------- Following scan added by Sched for reference pointing ----------

20 58 16  P-RHYA       14 32 42  35.2 191.0  0.7      10.3     0    40430   Stopped 
20 59 16  ---          14 33 42  35.2 191.3  0.7      10.6    60    40430           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

21 00 00  1510-089     14 34 27  49.1 165.1 -0.7     -12.9     9    40430   21 00 00
21 06 40  ---          14 41 08  49.5 167.6 -0.5     -10.8   400    40532   21 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

21 07 00  1510-089     14 41 28  49.5 167.7 -0.5     -10.7    14    40532   21 07 00
21 10 20  ---          14 44 48  49.6 169.0 -0.5      -9.6   200    40583   21 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page 173
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

21 12 09  3C279        14 46 37  45.0 220.4  1.8      34.1    64    40583   Stopped 
21 13 09  ---          14 47 37  44.9 220.7  1.8      34.3    60    40583           

 ---------- Following scan added by Sched for reference pointing ----------

21 13 15  3C279        14 47 43  44.9 220.7  1.8      34.4     0    40583   Stopped 
21 14 15  ---          14 48 43  44.8 221.0  1.9      34.6    60    40583           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

21 15 00  1510-089     14 49 29  49.8 170.7 -0.4      -8.1     2    40583   21 15 00
21 21 40  ---          14 56 10  50.0 173.3 -0.3      -5.8   400    40686   21 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

21 22 00  1510-089     14 56 30  50.0 173.4 -0.3      -5.7    14    40686   21 22 00
21 25 20  ---          14 59 51  50.1 174.7 -0.2      -4.6   200    40737   21 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

21 27 09  3C279        15 01 40  42.9 224.6  2.1      37.4    66    40737   Stopped 
21 28 09  ---          15 02 40  42.7 224.9  2.1      37.6    60    40737           

 ---------- Following scan added by Sched for reference pointing ----------

21 28 15  3C279        15 02 46  42.7 224.9  2.1      37.7     0    40737   Stopped 
21 29 15  ---          15 03 46  42.5 225.2  2.1      37.9    60    40737           
Schedule for VLBA_FD   (Code Fd )                                   Page 174
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

21 30 00  1510-089     15 04 32  50.2 176.5 -0.2      -3.1     3    40737   21 30 00
21 36 40  ---          15 11 13  50.2 179.1 -0.0      -0.8   400    40840   21 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

21 37 00  1510-089     15 11 33  50.2 179.2 -0.0      -0.7    14    40840   21 37 00
21 40 20  ---          15 14 53  50.2 180.5  0.0       0.4   200    40891   21 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

21 42 10  3C279        15 16 43  40.5 228.5  2.3      40.4    68    40891   Stopped 
21 43 10  ---          15 17 43  40.3 228.8  2.3      40.6    60    40891           

 ---------- Following scan added by Sched for reference pointing ----------

21 43 16  3C279        15 17 49  40.3 228.8  2.3      40.6     0    40891   Stopped 
21 44 16  ---          15 18 49  40.2 229.1  2.4      40.8    60    40891           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

21 45 00  1510-089     15 19 34  50.2 182.3  0.1       2.0     3    40891   21 45 00
21 51 40  ---          15 26 15  50.1 184.9  0.2       4.2   400    40994   21 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

21 52 00  1510-089     15 26 35  50.1 185.0  0.2       4.3    14    40994   21 52 00
21 55 20  ---          15 29 56  50.0 186.3  0.3       5.5   200    41045   21 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 175
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

21 57 11  3C279        15 31 47  38.0 232.1  2.6      43.1    70    41045   Stopped 
21 58 11  ---          15 32 47  37.8 232.4  2.6      43.2    60    41045           

 ---------- Following scan added by Sched for reference pointing ----------

21 58 17  3C279        15 32 53  37.8 232.4  2.6      43.3     0    41045   Stopped 
21 59 17  ---          15 33 53  37.7 232.6  2.6      43.4    60    41045           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

22 00 00  1510-089     15 34 36  49.9 188.1  0.3       7.0     4    41045   22 00 00
22 06 40  ---          15 41 18  49.7 190.6  0.5       9.2   400    41147   22 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

22 07 00  1510-089     15 41 38  49.6 190.7  0.5       9.3    14    41147   22 07 00
22 10 20  ---          15 44 58  49.5 192.0  0.5      10.4   200    41199   22 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

22 12 12  3C279        15 46 50  35.4 235.5  2.8      45.5    73    41199   Stopped 
22 13 12  ---          15 47 51  35.2 235.7  2.8      45.6    60    41199           

 ---------- Following scan added by Sched for reference pointing ----------

22 13 18  3C279        15 47 57  35.2 235.7  2.9      45.6     0    41199   Stopped 
22 14 18  ---          15 48 57  35.0 235.9  2.9      45.8    60    41199           
Schedule for VLBA_FD   (Code Fd )                                   Page 176
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

22 15 00  1510-089     15 49 39  49.3 193.7  0.6      11.9     4    41199   22 15 00
22 21 40  ---          15 56 20  48.9 196.2  0.7      14.0   400    41301   22 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

22 22 00  1510-089     15 56 40  48.9 196.3  0.7      14.1    14    41301   22 22 00
22 25 20  ---          16 00 01  48.7 197.5  0.8      15.2   200    41353   22 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

22 27 01  P-RRAQL      16 01 42  25.1 108.6 -3.9     -54.7    29    41353   Stopped 
22 28 01  ---          16 02 42  25.3 108.7 -3.9     -54.6    60    41353           

 ---------- Following scan added by Sched for reference pointing ----------

22 28 07  P-RRAQL      16 02 48  25.3 108.8 -3.9     -54.6     0    41353   Stopped 
22 29 07  ---          16 03 48  25.5 108.9 -3.9     -54.5    60    41353           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

22 30 00  BLLAC        16 04 41  20.3  52.0 -6.0     -66.6     5    41353   22 30 00
22 36 40  ---          16 11 22  21.4  52.5 -5.9     -67.5   400    41455   22 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

22 37 00  BLLAC        16 11 43  21.5  52.5 -5.9     -67.5    14    41455   22 37 00
22 40 20  ---          16 15 03  22.1  52.8 -5.8     -68.0   200    41506   22 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 177
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

22 41 59  P-RRAQL      16 16 43  28.1 111.1 -3.7     -53.5    50    41506   Stopped 
22 42 59  ---          16 17 43  28.3 111.2 -3.7     -53.4    60    41506           

 ---------- Following scan added by Sched for reference pointing ----------

22 43 05  P-RRAQL      16 17 49  28.4 111.2 -3.7     -53.4     0    41506   Stopped 
22 44 05  ---          16 18 49  28.6 111.4 -3.7     -53.3    60    41506           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

22 45 00  BLLAC        16 19 44  22.9  53.1 -5.7     -68.7     5    41506   22 45 00
22 51 40  ---          16 26 25  24.0  53.6 -5.6     -69.6   400    41609   22 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

22 52 00  BLLAC        16 26 45  24.1  53.6 -5.6     -69.6    14    41609   22 52 00
22 55 20  ---          16 30 06  24.7  53.9 -5.6     -70.1   200    41660   22 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

22 56 58  P-RRAQL      16 31 44  31.1 113.7 -3.4     -52.0    47    41660   Stopped 
22 57 58  ---          16 32 44  31.3 113.8 -3.4     -51.9    60    41660           

 ---------- Following scan added by Sched for reference pointing ----------

22 58 04  P-RRAQL      16 32 50  31.4 113.9 -3.4     -51.9     0    41660   Stopped 
22 59 04  ---          16 33 50  31.5 114.0 -3.4     -51.8    60    41660           
Schedule for VLBA_FD   (Code Fd )                                   Page 178
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

23 00 00  BLLAC        16 34 46  25.5  54.2 -5.5     -70.8     6    41660   23 00 00
23 06 40  ---          16 41 27  26.6  54.6 -5.4     -71.7   400    41763   23 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

23 07 00  BLLAC        16 41 47  26.7  54.7 -5.4     -71.7    14    41763   23 07 00
23 10 20  ---          16 45 08  27.3  54.9 -5.3     -72.2   200    41814   23 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

23 11 56  P-RRAQL      16 46 44  34.1 116.5 -3.2     -50.4    44    41814   Stopped 
23 12 56  ---          16 47 44  34.3 116.6 -3.2     -50.3    60    41814           

 ---------- Following scan added by Sched for reference pointing ----------

23 13 02  P-RRAQL      16 47 50  34.3 116.7 -3.2     -50.3     0    41814   Stopped 
23 14 02  ---          16 48 51  34.5 116.9 -3.2     -50.2    60    41814           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

23 15 00  BLLAC        16 49 49  28.1  55.2 -5.2     -72.9     6    41814   23 15 00
23 21 40  ---          16 56 30  29.3  55.6 -5.1     -73.8   400    41917   23 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

23 22 00  BLLAC        16 56 50  29.4  55.6 -5.1     -73.8    14    41917   23 22 00
23 25 20  ---          17 00 10  30.0  55.8 -5.1     -74.3   200    41968   23 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 179
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

23 26 54  P-RRAQL      17 01 45  36.9 119.4 -2.9     -48.6    41    41968   Stopped 
23 27 54  ---          17 02 45  37.1 119.7 -2.9     -48.4    60    41968           

 ---------- Following scan added by Sched for reference pointing ----------

23 28 00  P-RRAQL      17 02 51  37.1 119.7 -2.9     -48.4     0    41968   Stopped 
23 29 00  ---          17 03 51  37.3 119.9 -2.9     -48.3    60    41968           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

23 30 00  BLLAC        17 04 51  30.8  56.0 -5.0     -75.0     7    41968   23 30 00
23 36 40  ---          17 11 32  32.0  56.4 -4.9     -75.9   400    42071   23 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

23 37 00  BLLAC        17 11 52  32.0  56.4 -4.9     -75.9    14    42071   23 37 00
23 40 20  ---          17 15 13  32.6  56.6 -4.8     -76.4   200    42122   23 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

23 41 52  P-RRAQL      17 16 45  39.7 122.7 -2.7     -46.4    37    42122   Stopped 
23 42 52  ---          17 17 45  39.9 122.9 -2.7     -46.3    60    42122           

 ---------- Following scan added by Sched for reference pointing ----------

23 42 58  P-RRAQL      17 17 51  39.9 122.9 -2.7     -46.3     0    42122   Stopped 
23 43 58  ---          17 18 52  40.1 123.1 -2.7     -46.1    60    42122           
Schedule for VLBA_FD   (Code Fd )                                   Page 180
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  28 Sep 2014   Day 271 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

23 45 00  BLLAC        17 19 54  33.5  56.8 -4.7     -77.1     7    42122   23 45 00
23 51 40  ---          17 26 35  34.7  57.2 -4.6     -78.0   400    42224   23 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

23 52 00  BLLAC        17 26 55  34.8  57.2 -4.6     -78.1    14    42224   23 52 00
23 55 20  ---          17 30 15  35.4  57.3 -4.6     -78.5   200    42276   23 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

23 56 51  P-RRAQL      17 31 46  42.3 126.2 -2.4     -44.0    34    42276   Stopped 
23 57 51  ---          17 32 47  42.5 126.4 -2.4     -43.8    60    42276           

 ---------- Following scan added by Sched for reference pointing ----------

23 57 57  P-RRAQL      17 32 53  42.5 126.4 -2.4     -43.8     0    42276   Stopped 
23 58 57  ---          17 33 53  42.7 126.7 -2.4     -43.7    60    42276           

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

00 00 01  BLLAC        17 34 57  36.2  57.5 -4.5     -79.2     7    42276   00 00 01
00 06 41  ---          17 41 38  37.4  57.8 -4.4     -80.2   400    42378   00 00 02
Schedule for VLBA_FD   (Code Fd )                                   Page 181
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

00 07 01  BLLAC        17 41 58  37.5  57.8 -4.4     -80.2    14    42378   00 07 01
00 10 21  ---          17 45 19  38.1  57.9 -4.3     -80.7   200    42430   00 07 02

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

00 11 47  P-RRAQL      17 46 45  44.9 130.0 -2.2     -41.3    27    42430   Stopped 
00 12 47  ---          17 47 46  45.0 130.2 -2.2     -41.1    60    42430           

 ---------- Following scan added by Sched for reference pointing ----------

00 12 53  P-RRAQL      17 47 52  45.1 130.3 -2.2     -41.1     0    42430   Stopped 
00 13 53  ---          17 48 52  45.2 130.5 -2.2     -40.9    60    42430           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

00 15 00  BLLAC        17 49 59  38.9  58.1 -4.2     -81.4     7    42430   00 15 00
00 21 40  ---          17 56 40  40.2  58.3 -4.1     -82.4   400    42532   00 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

00 22 00  BLLAC        17 57 00  40.2  58.4 -4.1     -82.4    14    42532   00 22 00
00 25 20  ---          18 00 20  40.8  58.5 -4.1     -82.9   200    42583   00 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 182
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

00 26 59  3C454.3      18 01 59  22.4  83.9 -4.9     -63.0    54    42583   Stopped 
00 27 59  ---          18 03 00  22.6  84.0 -4.9     -63.0    60    42583           

 ---------- Following scan added by Sched for reference pointing ----------

00 28 05  3C454.3      18 03 06  22.7  84.0 -4.9     -63.0     0    42583   Stopped 
00 29 05  ---          18 04 06  22.9  84.1 -4.8     -63.1    60    42583           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

00 30 00  BLLAC        18 05 01  41.7  58.6 -4.0     -83.6    10    42583   00 30 00
00 36 40  ---          18 11 42  42.9  58.8 -3.9     -84.6   400    42686   00 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

00 37 00  BLLAC        18 12 02  43.0  58.8 -3.9     -84.7    14    42686   00 37 00
00 40 20  ---          18 15 23  43.6  58.9 -3.8     -85.2   200    42737   00 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

00 41 59  3C454.3      18 17 02  25.6  85.6 -4.6     -63.3    55    42737   Stopped 
00 42 59  ---          18 18 02  25.9  85.8 -4.6     -63.3    60    42737           

 ---------- Following scan added by Sched for reference pointing ----------

00 43 05  3C454.3      18 18 08  25.9  85.8 -4.6     -63.3     0    42737   Stopped 
00 44 05  ---          18 19 08  26.1  85.9 -4.6     -63.4    60    42737           
Schedule for VLBA_FD   (Code Fd )                                   Page 183
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

00 45 00  BLLAC        18 20 04  44.5  58.9 -3.7     -85.9    11    42737   00 45 00
00 51 40  ---          18 26 45  45.7  59.1 -3.6     -87.0   400    42840   00 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

00 52 00  BLLAC        18 27 05  45.8  59.1 -3.6     -87.0    14    42840   00 52 00
00 55 20  ---          18 30 25  46.4  59.1 -3.5     -87.5   200    42891   00 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

00 56 59  3C454.3      18 32 05  28.9  87.5 -4.4     -63.5    56    42891   Stopped 
00 57 59  ---          18 33 05  29.1  87.6 -4.4     -63.6    60    42891           

 ---------- Following scan added by Sched for reference pointing ----------

00 58 05  3C454.3      18 33 11  29.1  87.6 -4.4     -63.6     0    42891   Stopped 
00 59 05  ---          18 34 11  29.3  87.7 -4.3     -63.6    60    42891           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 00 00  BLLAC        18 35 06  47.2  59.1 -3.5     -88.3    12    42891   01 00 00
01 06 40  ---          18 41 47  48.5  59.2 -3.4     -89.4   400    42994   01 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

01 07 00  BLLAC        18 42 07  48.5  59.2 -3.4     -89.4    14    42994   01 07 00
01 10 20  ---          18 45 28  49.2  59.2 -3.3     -90.0   200    43045   01 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page 184
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 11 59  3C454.3      18 47 07  32.1  89.3 -4.1     -63.6    57    43045   Stopped 
01 12 59  ---          18 48 07  32.3  89.4 -4.1     -63.7    60    43045           

 ---------- Following scan added by Sched for reference pointing ----------

01 13 05  3C454.3      18 48 13  32.3  89.5 -4.1     -63.7     0    43045   Stopped 
01 14 05  ---          18 49 13  32.6  89.6 -4.1     -63.7    60    43045           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 15 00  BLLAC        18 50 08  50.0  59.2 -3.2     -90.8    13    43045   01 15 00
01 21 40  ---          18 56 50  51.3  59.1 -3.1     -92.0   400    43147   01 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

01 22 00  BLLAC        18 57 10  51.3  59.1 -3.1     -92.0    14    43147   01 22 00
01 25 20  ---          19 00 30  51.9  59.1 -3.0     -92.6   200    43199   01 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 26 59  3C454.3      19 02 09  35.3  91.2 -3.9     -63.6    58    43199   Stopped 
01 27 59  ---          19 03 10  35.6  91.4 -3.9     -63.6    60    43199           

 ---------- Following scan added by Sched for reference pointing ----------

01 28 05  3C454.3      19 03 16  35.6  91.4 -3.9     -63.6     0    43199   Stopped 
01 29 05  ---          19 04 16  35.8  91.5 -3.8     -63.6    60    43199           
Schedule for VLBA_FD   (Code Fd )                                   Page 185
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 30 00  BLLAC        19 05 11  52.8  59.0 -3.0     -93.5    14    43199   01 30 00
01 36 40  ---          19 11 52  54.0  58.9 -2.9     -94.7   400    43301   01 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

01 37 00  BLLAC        19 12 12  54.1  58.9 -2.9     -94.8    14    43301   01 37 00
01 40 20  ---          19 15 33  54.7  58.8 -2.8     -95.4   200    43353   01 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 41 59  3C454.3      19 17 12  38.6  93.3 -3.6     -63.5    58    43353   Stopped 
01 42 59  ---          19 18 12  38.8  93.4 -3.6     -63.5    60    43353           

 ---------- Following scan added by Sched for reference pointing ----------

01 43 05  3C454.3      19 18 18  38.8  93.4 -3.6     -63.5     0    43353   Stopped 
01 44 05  ---          19 19 18  39.0  93.5 -3.6     -63.4    60    43353           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

01 45 00  BLLAC        19 20 13  55.6  58.6 -2.7     -96.3    15    43353   01 45 00
01 51 40  ---          19 26 55  56.8  58.3 -2.6     -97.7   400    43455   01 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

01 52 00  BLLAC        19 27 15  56.8  58.3 -2.6     -97.7    14    43455   01 52 00
01 55 20  ---          19 30 35  57.5  58.2 -2.5     -98.4   200    43506   01 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 186
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

01 56 58  3C454.3      19 32 14  41.8  95.4 -3.4     -63.2    59    43506   Stopped 
01 57 58  ---          19 33 14  42.0  95.5 -3.4     -63.1    60    43506           

 ---------- Following scan added by Sched for reference pointing ----------

01 58 04  3C454.3      19 33 20  42.0  95.5 -3.4     -63.1     0    43506   Stopped 
01 59 04  ---          19 34 20  42.3  95.7 -3.3     -63.1    60    43506           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 00 00  BLLAC        19 35 16  58.3  57.9 -2.5     -99.4    16    43506   02 00 00
02 06 40  ---          19 41 57  59.5  57.5 -2.4    -100.9   400    43609   02 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

02 07 00  BLLAC        19 42 17  59.6  57.5 -2.4    -101.0    14    43609   02 07 00
02 10 20  ---          19 45 38  60.2  57.2 -2.3    -101.8   200    43660   02 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 11 57  3C454.3      19 47 15  45.0  97.6 -3.1     -62.6    59    43660   Stopped 
02 12 57  ---          19 48 16  45.2  97.8 -3.1     -62.6    60    43660           

 ---------- Following scan added by Sched for reference pointing ----------

02 13 03  3C454.3      19 48 22  45.2  97.8 -3.1     -62.6     0    43660   Stopped 
02 14 03  ---          19 49 22  45.5  98.0 -3.1     -62.6    60    43660           
Schedule for VLBA_FD   (Code Fd )                                   Page 187
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 15 00  BLLAC        19 50 18  61.0  56.8 -2.2    -102.9    18    43660   02 15 00
02 21 40  ---          19 56 59  62.2  56.2 -2.1    -104.6   400    43763   02 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

02 22 00  BLLAC        19 57 19  62.3  56.2 -2.1    -104.7    14    43763   02 22 00
02 25 20  ---          20 00 40  62.9  55.8 -2.0    -105.5   200    43814   02 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 26 57  3C454.3      20 02 17  48.2 100.1 -2.9     -61.9    57    43814   Stopped 
02 27 57  ---          20 03 17  48.4 100.3 -2.9     -61.9    60    43814           

 ---------- Following scan added by Sched for reference pointing ----------

02 28 03  3C454.3      20 03 23  48.4 100.3 -2.9     -61.9     0    43814   Stopped 
02 29 03  ---          20 04 23  48.7 100.4 -2.8     -61.8    60    43814           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 30 00  BLLAC        20 05 21  63.7  55.3 -2.0    -106.8    17    43814   02 30 00
02 36 40  ---          20 12 02  64.9  54.4 -1.9    -108.7   400    43917   02 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

02 37 00  BLLAC        20 12 22  65.0  54.4 -1.9    -108.8    14    43917   02 37 00
02 40 20  ---          20 15 43  65.5  53.9 -1.8    -109.8   200    43968   02 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 188
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 41 55  3C454.3      20 17 18  51.4 102.8 -2.6     -60.9    53    43968   Stopped 
02 42 55  ---          20 18 18  51.6 102.9 -2.6     -60.9    60    43968           

 ---------- Following scan added by Sched for reference pointing ----------

02 43 01  3C454.3      20 18 24  51.6 103.0 -2.6     -60.8     0    43968   Stopped 
02 44 01  ---          20 19 25  51.8 103.2 -2.6     -60.8    60    43968           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

02 45 00  BLLAC        20 20 23  66.4  53.2 -1.7    -111.3    15    43968   02 45 00
02 51 40  ---          20 27 04  67.5  52.0 -1.6    -113.5   400    44071   02 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

02 52 00  BLLAC        20 27 24  67.6  51.9 -1.6    -113.6    14    44071   02 52 00
02 55 20  ---          20 30 45  68.1  51.2 -1.5    -114.8   200    44122   02 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

02 56 54  3C454.3      20 32 19  54.5 105.7 -2.4     -59.6    47    44122   Stopped 
02 57 54  ---          20 33 19  54.7 105.9 -2.4     -59.5    60    44122           

 ---------- Following scan added by Sched for reference pointing ----------

02 58 00  3C454.3      20 33 25  54.7 106.0 -2.4     -59.5     0    44122   Stopped 
02 59 00  ---          20 34 25  54.9 106.2 -2.3     -59.4    60    44122           
Schedule for VLBA_FD   (Code Fd )                                   Page 189
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 00 00  BLLAC        20 35 26  68.9  50.2 -1.5    -116.6    13    44122   03 00 00
03 06 40  ---          20 42 07  70.0  48.6 -1.4    -119.2   400    44224   03 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

03 07 00  BLLAC        20 42 27  70.0  48.5 -1.3    -119.4    14    44224   03 07 00
03 10 20  ---          20 45 47  70.6  47.5 -1.3    -120.8   200    44276   03 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

03 11 52  3C454.3      20 47 20  57.6 109.1 -2.1     -57.9    40    44276   Stopped 
03 12 52  ---          20 48 20  57.8 109.3 -2.1     -57.8    60    44276           

 ---------- Following scan added by Sched for reference pointing ----------

03 12 58  3C454.3      20 48 26  57.8 109.3 -2.1     -57.7     0    44276   Stopped 
03 13 58  ---          20 49 26  58.0 109.6 -2.1     -57.6    60    44276           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 15 00  BLLAC        20 50 28  71.3  46.2 -1.2    -122.9     9    44276   03 15 00
03 21 40  ---          20 57 09  72.3  43.9 -1.1    -126.2   400    44378   03 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

03 22 00  BLLAC        20 57 29  72.4  43.8 -1.1    -126.3    14    44378   03 22 00
03 25 20  ---          21 00 50  72.9  42.5 -1.0    -128.1   200    44429   03 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 190
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

03 26 47  3C454.3      21 02 17  60.6 112.9 -1.9     -55.6    29    44429   Stopped 
03 27 47  ---          21 03 17  60.8 113.2 -1.9     -55.5    60    44429           

 ---------- Following scan added by Sched for reference pointing ----------

03 27 53  3C454.3      21 03 23  60.8 113.2 -1.9     -55.5     0    44429   Stopped 
03 28 53  ---          21 04 23  61.0 113.5 -1.8     -55.3    60    44429           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 30 00  BLLAC        21 05 31  73.5  40.6 -1.0    -130.7     7    44429   03 30 00
03 36 40  ---          21 12 12  74.4  37.6 -0.9    -134.7   400    44532   03 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

03 37 00  BLLAC        21 12 32  74.5  37.4 -0.8    -134.9    14    44532   03 37 00
03 40 20  ---          21 15 52  74.9  35.8 -0.8    -137.1   200    44583   03 37 01

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

03 45 00  BLLAC        21 20 33  75.5  33.2 -0.7    -140.4   274    44583   03 45 00
03 51 40  ---          21 27 14  76.2  29.2 -0.6    -145.4   400    44686   03 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

03 52 00  BLLAC        21 27 34  76.3  29.0 -0.6    -145.7    14    44686   03 52 00
03 55 20  ---          21 30 55  76.6  26.8 -0.5    -148.4   200    44737   03 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 191
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

03 57 24  3C84         21 32 59  21.9  53.6 -5.8     -67.8     8    44737   Stopped 
03 58 24  ---          21 33 59  22.0  53.7 -5.8     -67.9    60    44737           

 ---------- Following scan added by Sched for reference pointing ----------

03 58 30  3C84         21 34 05  22.0  53.7 -5.8     -67.9     0    44737   Stopped 
03 59 30  ---          21 35 05  22.2  53.8 -5.8     -68.1    60    44737           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 00 00  0235+164     21 35 36  20.2  82.1 -5.1     -62.8     2    44737   04 00 00
04 06 40  ---          21 42 17  21.7  82.9 -5.0     -63.0   400    44840   04 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

04 07 00  0235+164     21 42 37  21.7  82.9 -4.9     -63.1    14    44840   04 07 00
04 10 20  ---          21 45 57  22.5  83.3 -4.9     -63.1   200    44891   04 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 12 23  3C84         21 48 00  24.5  54.7 -5.5     -69.8    94    44891   Stopped 
04 13 23  ---          21 49 01  24.6  54.8 -5.5     -70.0    60    44891           

 ---------- Following scan added by Sched for reference pointing ----------

04 13 29  3C84         21 49 07  24.7  54.8 -5.5     -70.0     0    44891   Stopped 
04 14 29  ---          21 50 07  24.8  54.9 -5.5     -70.1    60    44891           
Schedule for VLBA_FD   (Code Fd )                                   Page 192
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 15 00  0235+164     21 50 38  23.5  83.9 -4.8     -63.3     3    44891   04 15 00
04 21 40  ---          21 57 19  24.9  84.7 -4.7     -63.4   400    44994   04 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

04 22 00  0235+164     21 57 39  25.0  84.7 -4.7     -63.4    14    44994   04 22 00
04 25 20  ---          22 01 00  25.7  85.1 -4.6     -63.5   200    45045   04 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 27 22  3C84         22 03 02  27.1  55.7 -5.3     -71.9    93    45045   Stopped 
04 28 22  ---          22 04 02  27.3  55.8 -5.3     -72.0    60    45045           

 ---------- Following scan added by Sched for reference pointing ----------

04 28 28  3C84         22 04 08  27.3  55.8 -5.3     -72.0     0    45045   Stopped 
04 29 28  ---          22 05 08  27.5  55.9 -5.3     -72.2    60    45045           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 30 00  0235+164     22 05 41  26.7  85.7 -4.6     -63.6     3    45045   04 30 00
04 36 40  ---          22 12 22  28.1  86.5 -4.5     -63.7   400    45147   04 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

04 37 00  0235+164     22 12 42  28.2  86.5 -4.4     -63.7    14    45147   04 37 00
04 40 20  ---          22 16 02  28.9  86.9 -4.4     -63.8   200    45199   04 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 193
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 42 21  3C84         22 18 03  29.8  56.7 -5.0     -73.9    91    45199   Stopped 
04 43 21  ---          22 19 03  30.0  56.7 -5.0     -74.1    60    45199           

 ---------- Following scan added by Sched for reference pointing ----------

04 43 27  3C84         22 19 10  30.0  56.7 -5.0     -74.1     0    45199   Stopped 
04 44 27  ---          22 20 10  30.2  56.8 -5.0     -74.2    60    45199           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

04 45 00  0235+164     22 20 43  29.9  87.5 -4.3     -63.8     4    45199   04 45 00
04 51 40  ---          22 27 24  31.3  88.3 -4.2     -63.9   400    45301   04 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

04 52 00  0235+164     22 27 44  31.4  88.3 -4.2     -63.9    14    45301   04 52 00
04 55 20  ---          22 31 05  32.1  88.7 -4.1     -63.9   200    45353   04 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

04 57 20  3C84         22 33 05  32.5  57.5 -4.8     -76.0    89    45353   Stopped 
04 58 20  ---          22 34 05  32.7  57.6 -4.8     -76.1    60    45353           

 ---------- Following scan added by Sched for reference pointing ----------

04 58 26  3C84         22 34 11  32.7  57.6 -4.8     -76.1     0    45353   Stopped 
04 59 26  ---          22 35 11  32.9  57.6 -4.8     -76.3    60    45353           
Schedule for VLBA_FD   (Code Fd )                                   Page 194
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 00 00  0235+164     22 35 45  33.1  89.3 -4.1     -63.9     4    45353   05 00 00
05 06 40  ---          22 42 27  34.6  90.2 -4.0     -63.9   400    45455   05 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

05 07 00  0235+164     22 42 47  34.6  90.2 -3.9     -63.9    14    45455   05 07 00
05 10 20  ---          22 46 07  35.4  90.6 -3.9     -63.9   200    45506   05 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 12 18  3C84         22 48 06  35.3  58.3 -4.5     -78.0    87    45506   Stopped 
05 13 18  ---          22 49 06  35.4  58.3 -4.5     -78.2    60    45506           

 ---------- Following scan added by Sched for reference pointing ----------

05 13 24  3C84         22 49 12  35.5  58.3 -4.5     -78.2     0    45506   Stopped 
05 14 24  ---          22 50 12  35.7  58.4 -4.5     -78.3    60    45506           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 15 00  0235+164     22 50 48  36.4  91.3 -3.8     -63.9     5    45506   05 15 00
05 21 40  ---          22 57 29  37.8  92.1 -3.7     -63.8   400    45609   05 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

05 22 00  0235+164     22 57 49  37.9  92.2 -3.7     -63.8    14    45609   05 22 00
05 25 20  ---          23 01 10  38.6  92.6 -3.6     -63.8   200    45660   05 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 195
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 27 17  3C84         23 03 07  38.0  59.0 -4.3     -80.1    85    45660   Stopped 
05 28 17  ---          23 04 07  38.2  59.0 -4.3     -80.3    60    45660           

 ---------- Following scan added by Sched for reference pointing ----------

05 28 23  3C84         23 04 13  38.2  59.0 -4.3     -80.3     0    45660   Stopped 
05 29 23  ---          23 05 13  38.4  59.0 -4.3     -80.4    60    45660           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 30 00  0235+164     23 05 50  39.6  93.3 -3.6     -63.7     5    45660   05 30 00
05 36 40  ---          23 12 31  41.0  94.2 -3.4     -63.6   400    45763   05 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

05 37 00  0235+164     23 12 52  41.1  94.3 -3.4     -63.6    14    45763   05 37 00
05 40 20  ---          23 16 12  41.8  94.7 -3.4     -63.5   200    45814   05 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 42 15  3C84         23 18 07  40.8  59.5 -4.0     -82.3    82    45814   Stopped 
05 43 15  ---          23 19 07  41.0  59.5 -4.0     -82.4    60    45814           

 ---------- Following scan added by Sched for reference pointing ----------

05 43 21  3C84         23 19 13  41.0  59.5 -4.0     -82.4     0    45814   Stopped 
05 44 21  ---          23 20 14  41.2  59.6 -4.0     -82.6    60    45814           
Schedule for VLBA_FD   (Code Fd )                                   Page 196
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

05 45 00  0235+164     23 20 53  42.8  95.4 -3.3     -63.4     6    45814   05 45 00
05 51 40  ---          23 27 34  44.3  96.4 -3.2     -63.2   400    45917   05 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

05 52 00  0235+164     23 27 54  44.3  96.4 -3.2     -63.2    14    45917   05 52 00
05 55 20  ---          23 31 15  45.0  97.0 -3.1     -63.1   200    45968   05 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

05 57 13  3C84         23 33 08  43.6  59.9 -3.8     -84.5    79    45968   Stopped 
05 58 13  ---          23 34 08  43.8  60.0 -3.8     -84.6    60    45968           

 ---------- Following scan added by Sched for reference pointing ----------

05 58 19  3C84         23 34 14  43.8  60.0 -3.8     -84.6     0    45968   Stopped 
05 59 19  ---          23 35 14  44.0  60.0 -3.8     -84.8    60    45968           

 ---------- PICO must now resume to VLBI on day 272-0600 UT, if it was stopped before ----------

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 00 00  0235+164     23 35 55  46.0  97.7 -3.1     -62.9     6    45968   06 00 00
06 06 40  ---          23 42 36  47.5  98.8 -2.9     -62.6   400    46070   06 00 01
Schedule for VLBA_FD   (Code Fd )                                   Page 197
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

06 07 00  0235+164     23 42 56  47.5  98.8 -2.9     -62.6    14    46070   06 07 00
06 10 20  ---          23 46 17  48.3  99.4 -2.9     -62.4   200    46122   06 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 12 13  P-WXPSC      23 48 10  64.4 130.2 -1.3     -42.3    74    46122   Stopped 
06 13 13  ---          23 49 11  64.6 130.6 -1.3     -42.0    60    46122           

 ---------- Following scan added by Sched for reference pointing ----------

06 13 19  P-WXPSC      23 49 17  64.6 130.7 -1.3     -42.0     0    46122   Stopped 
06 14 19  ---          23 50 17  64.7 131.1 -1.3     -41.6    60    46122           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 15 00  0235+164     23 50 58  49.2 100.1 -2.8     -62.1     2    46122   06 15 00
06 21 40  ---          23 57 39  50.7 101.3 -2.7     -61.7   400    46224   06 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

06 22 00  0235+164     23 57 59  50.7 101.4 -2.7     -61.7    14    46224   06 22 00
06 25 20  ---          00 01 19  51.4 102.0 -2.6     -61.5   200    46276   06 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 198
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 27 14  P-WXPSC      00 03 14  66.7 137.1 -1.1     -36.9    76    46276   Stopped 
06 28 14  ---          00 04 14  66.9 137.6 -1.1     -36.5    60    46276           

 ---------- Following scan added by Sched for reference pointing ----------

06 28 20  P-WXPSC      00 04 20  66.9 137.6 -1.0     -36.5     0    46276   Stopped 
06 29 20  ---          00 05 20  67.1 138.1 -1.0     -36.1    60    46276           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 30 00  0235+164     00 06 00  52.4 102.9 -2.6     -61.1     3    46276   06 30 00
06 36 40  ---          00 12 41  53.8 104.2 -2.4     -60.6   400    46378   06 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

06 37 00  0235+164     00 13 01  53.9 104.2 -2.4     -60.5    14    46378   06 37 00
06 40 20  ---          00 16 22  54.6 104.9 -2.4     -60.2   200    46429   06 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 42 13  P-WXPSC      00 18 15  68.8 145.1 -0.8     -30.3    77    46429   Stopped 
06 43 13  ---          00 19 16  68.9 145.7 -0.8     -29.8    60    46429           

 ---------- Following scan added by Sched for reference pointing ----------

06 43 19  P-WXPSC      00 19 22  68.9 145.8 -0.8     -29.7     0    46429   Stopped 
06 44 19  ---          00 20 22  69.0 146.4 -0.8     -29.2    60    46429           
Schedule for VLBA_FD   (Code Fd )                                   Page 199
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

06 45 00  0235+164     00 21 03  55.5 105.9 -2.3     -59.8     4    46429   06 45 00
06 51 40  ---          00 27 44  56.9 107.3 -2.2     -59.0   400    46532   06 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

06 52 00  0235+164     00 28 04  57.0 107.4 -2.2     -59.0    14    46532   06 52 00
06 55 20  ---          00 31 24  57.7 108.2 -2.1     -58.6   200    46583   06 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

06 57 12  P-WXPSC      00 33 17  70.4 154.6 -0.6     -22.3    72    46583   Stopped 
06 58 12  ---          00 34 17  70.5 155.2 -0.5     -21.7    60    46583           

 ---------- Following scan added by Sched for reference pointing ----------

06 58 18  P-WXPSC      00 34 23  70.5 155.3 -0.5     -21.6     0    46583   Stopped 
06 59 18  ---          00 35 23  70.6 156.0 -0.5     -21.0    60    46583           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 00 00  0235+164     00 36 05  58.6 109.3 -2.1     -58.0     1    46583   07 00 00
07 06 40  ---          00 42 46  60.0 111.0 -1.9     -57.0   400    46686   07 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

07 07 00  0235+164     00 43 06  60.1 111.1 -1.9     -56.9    14    46686   07 07 00
07 10 20  ---          00 46 27  60.7 112.0 -1.9     -56.4   200    46737   07 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page 200
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 12 22  3C84         00 48 29  57.7  59.6 -2.5     -97.3    77    46737   Stopped 
07 13 22  ---          00 49 29  57.8  59.6 -2.5     -97.5    60    46737           

 ---------- Following scan added by Sched for reference pointing ----------

07 13 28  3C84         00 49 35  57.9  59.6 -2.5     -97.5     0    46737   Stopped 
07 14 28  ---          00 50 35  58.0  59.5 -2.5     -97.7    60    46737           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 15 00  3C111        00 51 08  46.9  65.4 -3.5     -83.7     2    46737   07 15 00
07 21 40  ---          00 57 49  48.3  65.6 -3.4     -84.6   400    46840   07 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

07 22 00  3C111        00 58 09  48.3  65.7 -3.4     -84.6    14    46840   07 22 00
07 25 20  ---          01 01 29  49.0  65.7 -3.3     -85.1   200    46891   07 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 27 22  3C84         01 03 31  60.4  58.8 -2.3    -100.5    92    46891   Stopped 
07 28 22  ---          01 04 32  60.6  58.7 -2.3    -100.8    60    46891           

 ---------- Following scan added by Sched for reference pointing ----------

07 28 28  3C84         01 04 38  60.6  58.7 -2.3    -100.8     0    46891   Stopped 
07 29 28  ---          01 05 38  60.8  58.6 -2.3    -101.0    60    46891           
Schedule for VLBA_FD   (Code Fd )                                   Page 201
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 30 00  3C111        01 06 10  49.9  65.9 -3.2     -85.7     3    46891   07 30 00
07 36 40  ---          01 12 51  51.2  66.0 -3.1     -86.6   400    46994   07 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

07 37 00  3C111        01 13 11  51.3  66.0 -3.1     -86.7    14    46994   07 37 00
07 40 20  ---          01 16 32  51.9  66.1 -3.0     -87.1   200    47045   07 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 42 22  3C84         01 18 34  63.2  57.5 -2.0    -104.1    92    47045   Stopped 
07 43 22  ---          01 19 34  63.4  57.4 -2.0    -104.4    60    47045           

 ---------- Following scan added by Sched for reference pointing ----------

07 43 28  3C84         01 19 40  63.4  57.4 -2.0    -104.4     0    47045   Stopped 
07 44 28  ---          01 20 40  63.6  57.3 -2.0    -104.7    60    47045           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

07 45 00  3C111        01 21 13  52.8  66.1 -3.0     -87.8     3    47045   07 45 00
07 51 40  ---          01 27 54  54.2  66.2 -2.9     -88.8   400    47147   07 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

07 52 00  3C111        01 28 14  54.2  66.2 -2.9     -88.8    14    47147   07 52 00
07 55 20  ---          01 31 34  54.9  66.2 -2.8     -89.3   200    47199   07 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 202
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

07 57 48  3C84         01 34 02  66.0  55.6 -1.8    -108.4   119    47199   Stopped 
07 58 48  ---          01 35 03  66.1  55.4 -1.8    -108.7    60    47199           

 ---------- Following scan added by Sched for reference pointing ----------

07 58 54  3C84         01 35 09  66.2  55.4 -1.8    -108.8     0    47199   Stopped 
07 59 54  ---          01 36 09  66.3  55.3 -1.7    -109.1    60    47199           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 00 00  3C84         01 36 15  66.4  55.3 -1.7    -109.1     0    47199   08 00 00
08 06 40  ---          01 42 56  67.5  54.2 -1.6    -111.2   400    47301   08 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 07 00  3C84         01 43 16  67.6  54.1 -1.6    -111.3    14    47301   08 07 00
08 10 20  ---          01 46 37  68.2  53.5 -1.6    -112.4   200    47353   08 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 12 22  3C84         01 48 39  68.5  53.1 -1.5    -113.2   115    47353   Stopped 
08 13 22  ---          01 49 39  68.7  52.9 -1.5    -113.5    60    47353           

 ---------- Following scan added by Sched for reference pointing ----------

08 13 28  3C84         01 49 45  68.7  52.9 -1.5    -113.5     0    47353   Stopped 
08 14 28  ---          01 50 45  68.9  52.7 -1.5    -113.9    60    47353           
Schedule for VLBA_FD   (Code Fd )                                   Page 203
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 15 00  3C111        01 51 17  58.8  66.1 -2.5     -92.5     4    47353   08 15 00
08 21 40  ---          01 57 59  60.1  66.0 -2.4     -93.6   400    47455   08 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 22 00  3C111        01 58 19  60.1  66.0 -2.4     -93.7    14    47455   08 22 00
08 25 20  ---          02 01 39  60.8  65.9 -2.3     -94.3   200    47506   08 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 27 22  3C84         02 03 41  71.0  49.5 -1.3    -119.0    94    47506   Stopped 
08 28 22  ---          02 04 41  71.2  49.2 -1.3    -119.4    60    47506           

 ---------- Following scan added by Sched for reference pointing ----------

08 28 28  3C84         02 04 47  71.2  49.2 -1.3    -119.5     0    47506   Stopped 
08 29 28  ---          02 05 48  71.4  48.9 -1.3    -119.9    60    47506           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 30 00  3C111        02 06 20  61.7  65.7 -2.2     -95.1     5    47506   08 30 00
08 36 40  ---          02 13 01  63.0  65.4 -2.1     -96.4   400    47609   08 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 37 00  3C111        02 13 21  63.1  65.4 -2.1     -96.5    14    47609   08 37 00
08 40 20  ---          02 16 42  63.7  65.2 -2.0     -97.1   200    47660   08 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 204
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 42 22  3C84         02 18 44  73.4  44.5 -1.0    -126.2    95    47660   Stopped 
08 43 22  ---          02 19 44  73.6  44.1 -1.0    -126.8    60    47660           

 ---------- Following scan added by Sched for reference pointing ----------

08 43 28  3C84         02 19 50  73.6  44.1 -1.0    -126.8     0    47660   Stopped 
08 44 28  ---          02 20 50  73.7  43.7 -1.0    -127.4    60    47660           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

08 45 00  3C111        02 21 22  64.7  64.9 -2.0     -98.1     6    47660   08 45 00
08 51 40  ---          02 28 04  66.0  64.5 -1.9     -99.6   400    47763   08 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

08 52 00  3C111        02 28 24  66.0  64.4 -1.8     -99.7    14    47763   08 52 00
08 55 20  ---          02 31 44  66.7  64.1 -1.8    -100.4   200    47814   08 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

08 56 58  P-TXCAM      02 33 22  53.6  34.5 -2.5    -118.8    64    47814   Stopped 
08 57 58  ---          02 34 22  53.7  34.4 -2.5    -119.1    60    47814           

 ---------- Following scan added by Sched for reference pointing ----------

08 58 04  P-TXCAM      02 34 28  53.7  34.4 -2.5    -119.2     0    47814   Stopped 
08 59 04  ---          02 35 28  53.8  34.3 -2.4    -119.5    60    47814           
Schedule for VLBA_FD   (Code Fd )                                   Page 205
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 00 00  3C111        02 36 25  67.6  63.7 -1.7    -101.6    22    47814   09 00 00
09 06 40  ---          02 43 06  68.9  62.9 -1.6    -103.3   400    47917   09 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 07 00  3C111        02 43 26  68.9  62.9 -1.6    -103.4    14    47917   09 07 00
09 10 20  ---          02 46 47  69.6  62.4 -1.5    -104.3   200    47968   09 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 12 48  3C84         02 49 15  77.4  28.0 -0.5    -147.3   116    47968   Stopped 
09 13 48  ---          02 50 15  77.5  27.3 -0.5    -148.2    60    47968           

 ---------- Following scan added by Sched for reference pointing ----------

09 13 54  3C84         02 50 21  77.5  27.2 -0.5    -148.3     0    47968   Stopped 
09 14 54  ---          02 51 21  77.6  26.5 -0.5    -149.2    60    47968           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 15 00  3C84         02 51 27  77.6  26.4 -0.5    -149.3     0    47968   09 15 00
09 21 40  ---          02 58 08  78.2  21.1 -0.4    -155.5   400    48070   09 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 22 00  3C84         02 58 28  78.2  20.8 -0.4    -155.9    14    48070   09 22 00
09 25 20  ---          03 01 49  78.4  18.0 -0.3    -159.2   200    48122   09 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 206
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 27 49  P-IKTAU      03 04 18  67.6 146.2 -0.8     -29.2    50    48122   Stopped 
09 28 49  ---          03 05 19  67.7 146.8 -0.8     -28.8    60    48122           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 30 00  3C111        03 06 30  73.3  58.8 -1.2    -110.9     0    48122   09 30 00
09 36 40  ---          03 13 11  74.5  57.0 -1.1    -113.6   400    48224   09 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 37 00  3C111        03 13 31  74.5  56.9 -1.1    -113.8    14    48224   09 37 00
09 40 20  ---          03 16 52  75.1  55.8 -1.0    -115.3   200    48276   09 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 42 39  P-IKTAU      03 19 11  69.2 155.1 -0.6     -21.7    61    48276   Stopped 
09 43 39  ---          03 20 11  69.2 155.8 -0.6     -21.1    60    48276           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

09 45 00  3C111        03 21 32  76.0  54.2 -1.0    -117.6     1    48276   09 45 00
09 51 40  ---          03 28 13  77.1  51.4 -0.9    -121.4   400    48378   09 45 01
Schedule for VLBA_FD   (Code Fd )                                   Page 207
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

09 52 00  3C111        03 28 33  77.2  51.2 -0.8    -121.6    14    48378   09 52 00
09 55 20  ---          03 31 54  77.7  49.6 -0.8    -123.7   200    48429   09 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

09 56 44  3C84         03 33 18  78.8 -12.1  0.2     166.1    33    48429   Stopped 
09 57 44  ---          03 34 18  78.7 -13.0  0.2     165.0    60    48429           

 ---------- Following scan added by Sched for reference pointing ----------

09 57 50  3C84         03 34 24  78.7 -13.1  0.2     164.9     0    48429   Stopped 
09 58 50  ---          03 35 25  78.7 -14.0  0.2     163.8    60    48429           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 00 00  3C111        03 36 35  78.5  47.0 -0.7    -126.9    19    48429   10 00 00
10 06 40  ---          03 43 16  79.5  42.6 -0.6    -132.3   400    48532   10 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 07 00  3C111        03 43 36  79.5  42.4 -0.6    -132.5    14    48532   10 07 00
10 10 20  ---          03 46 56  80.0  39.8 -0.5    -135.6   200    48583   10 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page 208
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 12 36  3C84         03 49 13  77.7 -25.7  0.5     150.1    83    48583   Stopped 
10 13 36  ---          03 50 13  77.6 -26.4  0.5     149.2    60    48583           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 15 00  3C111        03 51 37  80.6  35.7 -0.5    -140.3    31    48583   10 15 00
10 21 40  ---          03 58 18  81.4  28.9 -0.4    -148.1   400    48686   10 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 22 00  3C111        03 58 38  81.4  28.5 -0.3    -148.5    14    48686   10 22 00
10 25 20  ---          04 01 59  81.8  24.6 -0.3    -152.9   200    48737   10 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 27 33  3C84         04 04 13  76.0 -35.6  0.7     137.9    83    48737   Stopped 
10 28 33  ---          04 05 13  75.9 -36.2  0.7     137.2    60    48737           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 30 00  3C111        04 06 40  82.1  18.6 -0.2    -159.6    39    48737   10 30 00
10 36 40  ---          04 13 21  82.5   9.1 -0.1    -170.1   400    48840   10 30 01
Schedule for VLBA_FD   (Code Fd )                                   Page 209
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 37 00  3C111        04 13 41  82.5   8.6 -0.1    -170.6    14    48840   10 37 00
10 40 20  ---          04 17 01  82.6   3.6 -0.0    -176.1   200    48891   10 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 41 45  3C84         04 18 26  74.1 -42.7  1.0     128.7    44    48891   Stopped 
10 42 45  ---          04 19 27  73.9 -43.2  1.0     128.1    60    48891           

 ---------- Following scan added by Sched for reference pointing ----------

10 42 51  3C84         04 19 33  73.9 -43.2  1.0     128.1     0    48891   Stopped 
10 43 51  ---          04 20 33  73.8 -43.6  1.0     127.5    60    48891           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

10 45 00  3C111        04 21 42  82.6  -3.6  0.0     176.1    32    48891   10 45 00
10 51 40  ---          04 28 23  82.3 -13.5  0.2     165.3   400    48994   10 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

10 52 00  3C111        04 28 43  82.3 -13.9  0.2     164.7    14    48994   10 52 00
10 55 20  ---          04 32 04  82.1 -18.6  0.2     159.6   200    49045   10 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 210
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

10 57 00  3C84         04 33 44  71.7 -48.3  1.2     120.9    71    49045   Stopped 
10 58 00  ---          04 34 44  71.6 -48.6  1.2     120.4    60    49045           

 ---------- Following scan added by Sched for reference pointing ----------

10 58 06  3C84         04 34 50  71.5 -48.6  1.2     120.4     0    49045   Stopped 
10 59 06  ---          04 35 50  71.4 -48.9  1.3     119.9    60    49045           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 00 00  3C111        04 36 45  81.8 -24.6  0.3     153.0    25    49045   11 00 00
11 06 40  ---          04 43 26  81.1 -32.1  0.4     144.5   400    49147   11 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 07 00  3C111        04 43 46  81.0 -32.5  0.4     144.1    14    49147   11 07 00
11 10 20  ---          04 47 06  80.6 -35.7  0.5     140.3   200    49199   11 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 15 18  3C84         04 52 05  68.7 -52.9  1.5     113.5   268    49199   Stopped 
11 16 18  ---          04 53 05  68.5 -53.1  1.5     113.1    60    49199           

 ---------- Following scan added by Sched for reference pointing ----------

11 16 24  3C84         04 53 11  68.5 -53.1  1.5     113.1     0    49199   Stopped 
11 17 24  ---          04 54 11  68.3 -53.3  1.6     112.7    60    49199           
Schedule for VLBA_FD   (Code Fd )                                   Page 211
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 17 30  3C84         04 54 17  68.3 -53.3  1.6     112.7     0    49199   11 17 30
11 24 10  ---          05 00 59  67.1 -54.6  1.7     110.5   400    49301   11 17 31

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 24 30  3C84         05 01 19  67.1 -54.6  1.7     110.4    14    49301   11 24 30
11 27 50  ---          05 04 39  66.5 -55.2  1.7     109.3   200    49352   11 24 31

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 28 29  3C84         05 05 18  66.4 -55.3  1.7     109.1    33    49352   Stopped 
11 29 29  ---          05 06 19  66.2 -55.4  1.8     108.8    60    49352           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 30 01  3C111        05 06 51  77.7 -49.6  0.8     123.7     1    49352   11 30 01
11 36 41  ---          05 13 32  76.6 -52.7  0.9     119.6   400    49455   11 30 02

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 37 01  3C111        05 13 52  76.5 -52.9  0.9     119.4    14    49455   11 37 01
11 40 21  ---          05 17 12  76.0 -54.2  1.0     117.6   200    49506   11 37 02
Schedule for VLBA_FD   (Code Fd )                                   Page 212
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 43 38  P-RCNC       05 20 30  45.0 105.0 -2.9     -58.1    76    49506   Stopped 
11 44 38  ---          05 21 30  45.2 105.2 -2.9     -58.0    60    49506           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

11 45 00  OJ287        05 21 52  41.0  89.2 -3.6     -66.3     2    49506   11 45 00
11 51 40  ---          05 28 33  42.4  90.1 -3.5     -66.3   400    49609   11 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

11 52 00  OJ287        05 28 53  42.5  90.1 -3.4     -66.3    14    49609   11 52 00
11 55 20  ---          05 32 14  43.2  90.6 -3.4     -66.3   200    49660   11 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

11 58 29  3C84         05 35 23  60.9 -58.6  2.2     101.1    75    49660   Stopped 
11 59 29  ---          05 36 24  60.7 -58.6  2.3     100.9    60    49660           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 00 01  3C111        05 36 55  72.4 -59.8  1.3     109.1     1    49660   12 00 01
12 06 41  ---          05 43 37  71.1 -61.1  1.4     106.9   400    49763   12 00 02
Schedule for VLBA_FD   (Code Fd )                                   Page 213
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 07 01  3C111        05 43 57  71.1 -61.2  1.4     106.8    14    49763   12 07 01
12 10 21  ---          05 47 17  70.5 -61.7  1.5     105.7   200    49814   12 07 02

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 13 12  P-RLEO       05 50 08  31.9  95.7 -4.0     -60.9    51    49814   Stopped 
12 14 12  ---          05 51 09  32.1  95.8 -4.0     -60.8    60    49814           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 15 00  1055+018     05 51 57  12.1  95.5 -5.1     -59.0     1    49814   12 15 00
12 21 40  ---          05 58 38  13.5  96.4 -5.0     -58.8   400    49917   12 15 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 28 36  P-RCNC       06 05 35  54.1 114.7 -2.2     -53.0   330    49917   Stopped 
12 29 36  ---          06 06 35  54.3 114.9 -2.2     -52.8    60    49917           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 30 00  OJ287        06 06 59  50.7  95.4 -2.8     -65.8     2    49917   12 30 00
12 36 40  ---          06 13 40  52.1  96.5 -2.7     -65.5   400    50019   12 30 01
Schedule for VLBA_FD   (Code Fd )                                   Page 214
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 37 00  OJ287        06 14 01  52.2  96.5 -2.7     -65.5    14    50019   12 37 00
12 40 20  ---          06 17 21  52.9  97.0 -2.6     -65.4   200    50070   12 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 42 06  P-RLEO       06 19 07  38.0  99.9 -3.5     -59.8    68    50070   Stopped 
12 43 06  ---          06 20 07  38.3 100.1 -3.5     -59.8    60    50070           

 ---------- Following scan added by Sched for reference pointing ----------

12 43 12  P-RLEO       06 20 13  38.3 100.1 -3.5     -59.8     0    50070   Stopped 
12 44 12  ---          06 21 13  38.5 100.3 -3.5     -59.7    60    50070           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

12 45 00  1055+018     06 22 02  18.5  99.6 -4.6     -58.1     1    50070   12 45 00
12 51 40  ---          06 28 43  19.9 100.5 -4.5     -57.8   400    50173   12 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

12 52 00  1055+018     06 29 03  20.0 100.6 -4.5     -57.8    14    50173   12 52 00
12 55 20  ---          06 32 24  20.7 101.0 -4.4     -57.7   200    50224   12 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 215
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

12 58 35  P-RCNC       06 35 39  59.8 123.3 -1.7     -47.2   111    50224   Stopped 
12 59 35  ---          06 36 39  60.0 123.7 -1.7     -47.0    60    50224           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 00 00  OJ287        06 37 04  57.1 100.5 -2.3     -64.2     1    50224   13 00 00
13 06 40  ---          06 43 45  58.5 101.8 -2.2     -63.7   400    50327   13 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 07 00  OJ287        06 44 05  58.6 101.8 -2.2     -63.7    14    50327   13 07 00
13 10 20  ---          06 47 26  59.3 102.5 -2.1     -63.4   200    50378   13 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 12 05  P-RLEO       06 49 12  44.4 105.0 -3.0     -58.0    67    50378   Stopped 
13 13 05  ---          06 50 12  44.6 105.2 -3.0     -57.9    60    50378           

 ---------- Following scan added by Sched for reference pointing ----------

13 13 11  P-RLEO       06 50 18  44.6 105.2 -3.0     -57.9     0    50378   Stopped 
13 14 11  ---          06 51 18  44.8 105.4 -3.0     -57.8    60    50378           
Schedule for VLBA_FD   (Code Fd )                                   Page 216
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 15 00  1055+018     06 52 07  24.8 103.9 -4.1     -56.7     1    50378   13 15 00
13 21 40  ---          06 58 48  26.2 105.0 -4.0     -56.3   400    50481   13 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 22 00  1055+018     06 59 08  26.3 105.0 -4.0     -56.2    14    50481   13 22 00
13 25 20  ---          07 02 28  27.0 105.5 -3.9     -56.0   200    50532   13 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 27 26  P-RCNC       07 04 35  64.6 134.4 -1.2     -38.9    44    50532   Stopped 
13 28 26  ---          07 05 35  64.8 134.9 -1.2     -38.5    60    50532           

 ---------- Following scan added by Sched for reference pointing ----------

13 28 32  P-RCNC       07 05 41  64.8 134.9 -1.2     -38.5     0    50532   Stopped 
13 29 32  ---          07 06 41  65.0 135.4 -1.2     -38.1    60    50532           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 30 00  OJ287        07 07 09  63.4 107.0 -1.8     -61.1     0    50532   13 30 00
13 36 40  ---          07 13 50  64.8 108.8 -1.7     -60.1   400    50635   13 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 37 00  OJ287        07 14 10  64.8 108.9 -1.7     -60.1    14    50635   13 37 00
13 40 20  ---          07 17 31  65.5 109.8 -1.6     -59.5   200    50686   13 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 217
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 42 05  P-RLEO       07 19 17  50.5 111.0 -2.5     -55.0    67    50686   Stopped 
13 43 05  ---          07 20 17  50.7 111.2 -2.5     -54.9    60    50686           

 ---------- Following scan added by Sched for reference pointing ----------

13 43 11  P-RLEO       07 20 23  50.7 111.3 -2.5     -54.9     0    50686   Stopped 
13 44 11  ---          07 21 23  50.9 111.5 -2.4     -54.7    60    50686           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

13 45 00  1055+018     07 22 12  31.0 108.7 -3.6     -54.6     1    50686   13 45 00
13 51 40  ---          07 28 53  32.4 109.9 -3.5     -54.0   400    50788   13 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

13 52 00  1055+018     07 29 13  32.5 109.9 -3.5     -54.0    14    50788   13 52 00
13 55 20  ---          07 32 33  33.1 110.5 -3.4     -53.7   200    50840   13 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

13 57 05  P-RLEO       07 34 19  53.5 114.5 -2.2     -53.0    58    50840   Stopped 
13 58 05  ---          07 35 19  53.7 114.8 -2.2     -52.8    60    50840           

 ---------- Following scan added by Sched for reference pointing ----------

13 58 11  P-RLEO       07 35 25  53.7 114.8 -2.2     -52.8     0    50840   Stopped 
13 59 11  ---          07 36 25  53.9 115.1 -2.2     -52.7    60    50840           
Schedule for VLBA_FD   (Code Fd )                                   Page 218
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 00 00  1055+018     07 37 14  34.1 111.4 -3.4     -53.3     1    50840   14 00 00
14 06 40  ---          07 43 55  35.4 112.6 -3.3     -52.6   400    50942   14 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 07 00  1055+018     07 44 15  35.5 112.6 -3.2     -52.6    14    50942   14 07 00
14 10 20  ---          07 47 36  36.1 113.3 -3.2     -52.2   200    50993   14 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 12 06  P-RLEO       07 49 22  56.4 118.5 -2.0     -50.5    58    50993   Stopped 
14 13 06  ---          07 50 22  56.6 118.8 -2.0     -50.3    60    50993           

 ---------- Following scan added by Sched for reference pointing ----------

14 13 12  P-RLEO       07 50 28  56.6 118.8 -2.0     -50.3     0    50993   Stopped 
14 14 12  ---          07 51 28  56.8 119.1 -1.9     -50.1    60    50993           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 15 00  1055+018     07 52 17  37.1 114.2 -3.1     -51.7     2    50993   14 15 00
14 21 40  ---          07 58 58  38.4 115.5 -3.0     -51.0   400    51096   14 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 22 00  1055+018     07 59 18  38.4 115.6 -3.0     -50.9    14    51096   14 22 00
14 25 20  ---          08 02 38  39.1 116.2 -2.9     -50.5   200    51147   14 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 219
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 27 06  P-RLEO       08 04 24  59.2 123.1 -1.7     -47.4    59    51147   Stopped 
14 28 06  ---          08 05 24  59.3 123.4 -1.7     -47.1    60    51147           

 ---------- Following scan added by Sched for reference pointing ----------

14 28 12  P-RLEO       08 05 31  59.4 123.4 -1.7     -47.1     0    51147   Stopped 
14 29 12  ---          08 06 31  59.5 123.8 -1.7     -46.9    60    51147           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 30 00  1055+018     08 07 19  40.0 117.2 -2.9     -50.0     2    51147   14 30 00
14 36 40  ---          08 14 00  41.2 118.6 -2.8     -49.1   400    51250   14 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 37 00  1055+018     08 14 20  41.3 118.7 -2.7     -49.0    14    51250   14 37 00
14 40 20  ---          08 17 41  41.9 119.4 -2.7     -48.6   200    51301   14 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 42 06  P-RLEO       08 19 27  61.8 128.3 -1.5     -43.5    59    51301   Stopped 
14 43 06  ---          08 20 27  62.0 128.7 -1.5     -43.2    60    51301           

 ---------- Following scan added by Sched for reference pointing ----------

14 43 12  P-RLEO       08 20 33  62.0 128.7 -1.5     -43.2     0    51301   Stopped 
14 44 12  ---          08 21 33  62.2 129.1 -1.4     -42.9    60    51301           
Schedule for VLBA_FD   (Code Fd )                                   Page 220
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

14 45 00  1055+018     08 22 22  42.8 120.5 -2.6     -47.9     2    51301   14 45 00
14 51 40  ---          08 29 03  44.0 122.1 -2.5     -46.8   400    51404   14 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

14 52 00  1055+018     08 29 23  44.1 122.1 -2.5     -46.8    14    51404   14 52 00
14 55 20  ---          08 32 43  44.7 122.9 -2.4     -46.2   200    51455   14 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

14 57 18  P-RCNC       08 34 42  70.6 192.9  0.3      11.3    59    51455   Stopped 
14 58 18  ---          08 35 42  70.6 193.6  0.3      11.9    60    51455           

 ---------- Following scan added by Sched for reference pointing ----------

14 58 24  P-RCNC       08 35 48  70.6 193.7  0.3      12.0     0    51455   Stopped 
14 59 24  ---          08 36 48  70.5 194.4  0.3      12.6    60    51455           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 00 00  OJ287        08 37 24  78.6 157.7 -0.3     -20.3     2    51455   15 00 00
15 06 40  ---          08 44 05  79.1 165.5 -0.2     -13.3   400    51558   15 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 07 00  OJ287        08 44 25  79.1 165.9 -0.2     -12.9    14    51558   15 07 00
15 10 20  ---          08 47 46  79.3 170.0 -0.1      -9.1   200    51609   15 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page 221
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 12 07  P-RLEO       08 49 33  66.4 141.6 -1.0     -33.0    73    51609   Stopped 
15 13 07  ---          08 50 33  66.5 142.1 -1.0     -32.6    60    51609           

 ---------- Following scan added by Sched for reference pointing ----------

15 13 13  P-RLEO       08 50 39  66.5 142.2 -1.0     -32.6     0    51609   Stopped 
15 14 13  ---          08 51 39  66.7 142.7 -0.9     -32.1    60    51609           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 15 00  1055+018     08 52 26  48.2 128.0 -2.1     -42.7     3    51609   15 15 00
15 21 40  ---          08 59 08  49.3 129.9 -2.0     -41.3   400    51711   15 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 22 00  1055+018     08 59 28  49.3 130.0 -2.0     -41.2    14    51711   15 22 00
15 25 20  ---          09 02 48  49.9 131.0 -1.9     -40.5   200    51763   15 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 27 08  P-RLEO       09 04 36  68.2 149.9 -0.7     -26.1    64    51763   Stopped 
15 28 08  ---          09 05 36  68.3 150.5 -0.7     -25.6    60    51763           

 ---------- Following scan added by Sched for reference pointing ----------

15 28 14  P-RLEO       09 05 42  68.3 150.6 -0.7     -25.5     0    51763   Stopped 
15 29 14  ---          09 06 42  68.4 151.2 -0.7     -25.0    60    51763           
Schedule for VLBA_FD   (Code Fd )                                   Page 222
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 30 00  1055+018     09 07 29  50.6 132.4 -1.9     -39.5     3    51763   15 30 00
15 36 40  ---          09 14 10  51.7 134.5 -1.8     -37.9   400    51865   15 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 37 00  1055+018     09 14 30  51.7 134.6 -1.7     -37.8    14    51865   15 37 00
15 40 20  ---          09 17 51  52.2 135.7 -1.7     -37.0   200    51917   15 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 42 09  P-RLEO       09 19 40  69.6 159.4 -0.5     -18.0    67    51917   Stopped 
15 43 09  ---          09 20 40  69.7 160.1 -0.5     -17.4    60    51917           

 ---------- Following scan added by Sched for reference pointing ----------

15 43 15  P-RLEO       09 20 46  69.7 160.2 -0.5     -17.3     0    51917   Stopped 
15 44 15  ---          09 21 46  69.8 160.9 -0.4     -16.7    60    51917           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

15 45 00  1055+018     09 22 31  52.9 137.2 -1.6     -35.8     4    51917   15 45 00
15 51 40  ---          09 29 13  53.9 139.5 -1.5     -34.0   400    52019   15 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

15 52 00  1055+018     09 29 33  53.9 139.6 -1.5     -33.9    14    52019   15 52 00
15 55 20  ---          09 32 53  54.4 140.8 -1.4     -32.9   200    52070   15 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 223
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

15 57 21  P-RCNC       09 34 54  63.9 227.6  1.3      40.5    51    52070   Stopped 
15 58 21  ---          09 35 54  63.7 228.0  1.3      40.8    60    52070           

 ---------- Following scan added by Sched for reference pointing ----------

15 58 27  P-RCNC       09 36 00  63.7 228.1  1.3      40.8     0    52070   Stopped 
15 59 27  ---          09 37 00  63.6 228.5  1.3      41.2    60    52070           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 00 00  OJ287        09 37 34  75.8 224.2  0.7      39.7     1    52070   16 00 00
16 06 40  ---          09 44 15  74.8 228.8  0.8      43.6   400    52173   16 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 07 00  OJ287        09 44 35  74.7 229.0  0.8      43.8    14    52173   16 07 00
16 10 20  ---          09 47 56  74.2 231.1  0.9      45.5   200    52224   16 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 12 12  P-RLEO       09 49 48  70.7 181.1  0.0       1.0    68    52224   Stopped 
16 13 12  ---          09 50 48  70.7 181.8  0.0       1.6    60    52224           

 ---------- Following scan added by Sched for reference pointing ----------

16 13 18  P-RLEO       09 50 54  70.7 181.9  0.0       1.7     0    52224   Stopped 
16 14 18  ---          09 51 54  70.7 182.6  0.1       2.3    60    52224           
Schedule for VLBA_FD   (Code Fd )                                   Page 224
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 15 00  1055+018     09 52 36  56.9 148.4 -1.1     -26.8     6    52224   16 15 00
16 21 40  ---          09 59 17  57.6 151.2 -1.0     -24.5   400    52327   16 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 22 00  1055+018     09 59 37  57.6 151.3 -1.0     -24.4    14    52327   16 22 00
16 25 20  ---          10 02 58  57.9 152.7 -0.9     -23.2   200    52378   16 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 27 15  P-RLEO       10 04 53  70.3 192.1  0.3      10.6    80    52378   Stopped 
16 28 15  ---          10 05 53  70.3 192.9  0.3      11.3    60    52378           

 ---------- Following scan added by Sched for reference pointing ----------

16 28 21  P-RLEO       10 05 59  70.3 192.9  0.3      11.3     0    52378   Stopped 
16 29 21  ---          10 06 59  70.2 193.6  0.3      11.9    60    52378           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 30 00  1055+018     10 07 39  58.4 154.8 -0.9     -21.5     4    52378   16 30 00
16 36 40  ---          10 14 20  59.0 157.8 -0.7     -19.0   400    52481   16 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 37 00  1055+018     10 14 40  59.0 158.0 -0.7     -18.8    14    52481   16 37 00
16 40 20  ---          10 18 01  59.3 159.5 -0.7     -17.5   200    52532   16 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 225
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 42 16  P-RLEO       10 19 57  69.4 202.5  0.5      19.6    78    52532   Stopped 
16 43 16  ---          10 20 57  69.3 203.2  0.5      20.2    60    52532           

 ---------- Following scan added by Sched for reference pointing ----------

16 43 22  P-RLEO       10 21 03  69.3 203.2  0.5      20.2     0    52532   Stopped 
16 44 22  ---          10 22 03  69.2 203.9  0.6      20.8    60    52532           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

16 45 00  1055+018     10 22 41  59.6 161.7 -0.6     -15.7     0    52532   16 45 00
16 51 40  ---          10 29 22  60.0 164.9 -0.5     -12.9   400    52634   16 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

16 52 00  1055+018     10 29 42  60.0 165.1 -0.5     -12.8    14    52634   16 52 00
16 55 20  ---          10 33 03  60.2 166.7 -0.4     -11.4   200    52686   16 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

16 57 20  P-RCNC       10 35 04  53.0 246.8  2.3      53.8    56    52686   Stopped 
16 58 20  ---          10 36 04  52.8 247.0  2.3      54.0    60    52686           

 ---------- Following scan added by Sched for reference pointing ----------

16 58 26  P-RCNC       10 36 10  52.7 247.0  2.3      54.0     0    52686   Stopped 
16 59 26  ---          10 37 10  52.5 247.3  2.3      54.1    60    52686           
Schedule for VLBA_FD   (Code Fd )                                   Page 226
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 00 00  OJ287        10 37 44  64.7 251.3  1.7      60.2     2    52686   17 00 00
17 06 40  ---          10 44 25  63.3 253.1  1.8      61.2   400    52788   17 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 07 00  OJ287        10 44 45  63.3 253.1  1.8      61.2    14    52788   17 07 00
17 10 20  ---          10 48 05  62.6 254.0  1.9      61.7   200    52840   17 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 12 15  P-RLEO       10 50 00  66.0 219.9  1.0      34.2    82    52840   Stopped 
17 13 15  ---          10 51 01  65.9 220.4  1.0      34.6    60    52840           

 ---------- Following scan added by Sched for reference pointing ----------

17 13 21  P-RLEO       10 51 07  65.9 220.4  1.0      34.7     0    52840   Stopped 
17 14 21  ---          10 52 07  65.7 220.9  1.1      35.1    60    52840           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 15 00  1055+018     10 52 46  60.8 176.7 -0.1      -2.9     0    52840   17 15 00
17 21 40  ---          10 59 27  60.9 180.1  0.0       0.1   400    52942   17 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 22 00  1055+018     10 59 47  60.9 180.3  0.0       0.2    14    52942   17 22 00
17 25 20  ---          11 03 08  60.8 182.0  0.1       1.7   200    52993   17 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 227
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 27 15  P-RLEO       11 05 03  63.8 226.8  1.3      39.8    76    52993   Stopped 
17 28 15  ---          11 06 03  63.6 227.2  1.3      40.1    60    52993           

 ---------- Following scan added by Sched for reference pointing ----------

17 28 21  P-RLEO       11 06 10  63.6 227.3  1.3      40.1     0    52993   Stopped 
17 29 21  ---          11 07 10  63.4 227.7  1.3      40.5    60    52993           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 30 00  1055+018     11 07 49  60.8 184.4  0.1       3.8     0    52993   17 30 00
17 36 40  ---          11 14 30  60.6 187.8  0.3       6.7   400    53096   17 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 37 00  1055+018     11 14 50  60.6 188.0  0.3       6.8    14    53096   17 37 00
17 40 20  ---          11 18 10  60.5 189.6  0.3       8.3   200    53147   17 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 42 15  P-RLEO       11 20 05  61.3 232.7  1.5      44.3    77    53147   Stopped 
17 43 15  ---          11 21 06  61.1 233.1  1.5      44.6    60    53147           

 ---------- Following scan added by Sched for reference pointing ----------

17 43 21  P-RLEO       11 21 12  61.1 233.1  1.5      44.6     0    53147   Stopped 
17 44 21  ---          11 22 12  60.9 233.5  1.6      44.9    60    53147           
Schedule for VLBA_FD   (Code Fd )                                   Page 228
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

17 45 00  1055+018     11 22 51  60.3 192.0  0.4      10.3     2    53147   17 45 00
17 51 40  ---          11 29 32  60.0 195.3  0.5      13.1   400    53250   17 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

17 52 00  1055+018     11 29 52  60.0 195.4  0.5      13.2    14    53250   17 52 00
17 55 20  ---          11 33 13  59.8 197.1  0.6      14.6   200    53301   17 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

17 57 24  P-RLEO       11 35 17  58.6 237.9  1.8      48.0    87    53301   Stopped 
17 58 24  ---          11 36 17  58.4 238.2  1.8      48.2    60    53301           

 ---------- Following scan added by Sched for reference pointing ----------

17 58 30  P-RLEO       11 36 23  58.4 238.2  1.8      48.3     0    53301   Stopped 
17 59 30  ---          11 37 23  58.2 238.6  1.8      48.5    60    53301           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 00 00  OJ287        11 37 54  52.1 263.6  2.7      65.5     5    53301   18 00 00
18 06 40  ---          11 44 35  50.6 264.6  2.8      65.8   400    53404   18 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 07 00  OJ287        11 44 55  50.6 264.7  2.8      65.8    14    53404   18 07 00
18 10 20  ---          11 48 15  49.9 265.2  2.9      65.9   200    53455   18 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page 229
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 12 16  P-RLEO       11 50 12  55.8 242.3  2.0      51.0    92    53455   Stopped 
18 13 16  ---          11 51 12  55.6 242.6  2.0      51.2    60    53455           

 ---------- Following scan added by Sched for reference pointing ----------

18 13 22  P-RLEO       11 51 18  55.6 242.6  2.0      51.2     0    53455   Stopped 
18 14 22  ---          11 52 18  55.4 242.9  2.1      51.4    60    53455           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 15 00  1055+018     11 52 56  58.2 206.1  0.9      22.3     4    53455   18 15 00
18 21 40  ---          11 59 37  57.5 209.0  1.0      24.7   400    53558   18 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 22 00  1055+018     11 59 57  57.5 209.2  1.0      24.8    14    53558   18 22 00
18 25 20  ---          12 03 18  57.1 210.5  1.1      25.9   200    53609   18 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 27 18  P-RLEO       12 05 16  52.9 246.2  2.3      53.4    85    53609   Stopped 
18 28 18  ---          12 06 16  52.7 246.4  2.3      53.5    60    53609           

 ---------- Following scan added by Sched for reference pointing ----------

18 28 24  P-RLEO       12 06 22  52.7 246.4  2.3      53.6     0    53609   Stopped 
18 29 24  ---          12 07 22  52.5 246.7  2.3      53.7    60    53609           
Schedule for VLBA_FD   (Code Fd )                                   Page 230
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 30 00  1055+018     12 07 59  56.6 212.5  1.1      27.5     4    53609   18 30 00
18 36 40  ---          12 14 40  55.8 215.1  1.3      29.7   400    53711   18 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 37 00  1055+018     12 15 00  55.8 215.2  1.3      29.8    14    53711   18 37 00
18 40 20  ---          12 18 20  55.4 216.5  1.3      30.8   200    53763   18 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 42 19  P-RLEO       12 20 20  49.9 249.6  2.5      55.4    88    53763   Stopped 
18 43 19  ---          12 21 20  49.7 249.8  2.5      55.5    60    53763           

 ---------- Following scan added by Sched for reference pointing ----------

18 43 25  P-RLEO       12 21 26  49.7 249.9  2.6      55.5     0    53763   Stopped 
18 44 25  ---          12 22 26  49.5 250.1  2.6      55.6    60    53763           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

18 45 00  1055+018     12 23 01  54.7 218.2  1.4      32.2     4    53763   18 45 00
18 51 40  ---          12 29 42  53.8 220.6  1.5      34.1   400    53865   18 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

18 52 00  1055+018     12 30 02  53.8 220.8  1.5      34.2    14    53865   18 52 00
18 55 20  ---          12 33 23  53.3 221.9  1.6      35.1   200    53917   18 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page 231
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

18 57 30  P-RLEO       12 35 33  46.8 252.8  2.8      56.9   101    53917   Stopped 
18 58 30  ---          12 36 33  46.6 252.9  2.8      57.0    60    53917           

 ---------- Following scan added by Sched for reference pointing ----------

18 58 36  P-RLEO       12 36 39  46.6 253.0  2.8      57.0     0    53917   Stopped 
18 59 36  ---          12 37 40  46.4 253.2  2.8      57.1    60    53917           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 00 00  OJ287        12 38 03  39.1 271.8  3.7      66.3     2    53917   19 00 00
19 06 40  ---          12 44 45  37.7 272.6  3.8      66.2   400    54019   19 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 07 00  OJ287        12 45 05  37.6 272.7  3.8      66.2    14    54019   19 07 00
19 10 20  ---          12 48 25  36.9 273.1  3.9      66.2   200    54070   19 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 12 23  P-RLEO       12 50 28  43.7 255.5  3.0      58.2   101    54070   Stopped 
19 13 23  ---          12 51 28  43.5 255.7  3.1      58.3    60    54070           

 ---------- Following scan added by Sched for reference pointing ----------

19 13 29  P-RLEO       12 51 34  43.5 255.7  3.1      58.3     0    54070   Stopped 
19 14 29  ---          12 52 35  43.3 255.9  3.1      58.3    60    54070           
Schedule for VLBA_FD   (Code Fd )                                   Page 232
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 15 00  1055+018     12 53 06  50.3 228.2  1.9      39.9     4    54070   19 15 00
19 21 40  ---          12 59 47  49.2 230.2  2.0      41.4   400    54173   19 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 22 00  1055+018     13 00 07  49.2 230.3  2.0      41.5    14    54173   19 22 00
19 25 20  ---          13 03 28  48.6 231.2  2.1      42.2   200    54224   19 22 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 27 24  P-RLEO       13 05 32  40.6 258.1  3.3      59.2    97    54224   Stopped 
19 28 24  ---          13 06 32  40.4 258.3  3.3      59.2    60    54224           

 ---------- Following scan added by Sched for reference pointing ----------

19 28 30  P-RLEO       13 06 38  40.3 258.3  3.3      59.3     0    54224   Stopped 
19 29 30  ---          13 07 39  40.1 258.5  3.3      59.3    60    54224           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 30 00  1055+018     13 08 08  47.8 232.5  2.1      43.1     3    54224   19 30 00
19 36 40  ---          13 14 49  46.7 234.3  2.3      44.4   400    54327   19 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 37 00  1055+018     13 15 10  46.6 234.4  2.3      44.4    14    54327   19 37 00
19 40 20  ---          13 18 30  46.0 235.3  2.3      45.0   200    54378   19 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page 233
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 42 26  P-RLEO       13 20 36  37.4 260.5  3.5      60.0   100    54378   Stopped 
19 43 26  ---          13 21 36  37.2 260.7  3.6      60.0    60    54378           

 ---------- Following scan added by Sched for reference pointing ----------

19 43 32  P-RLEO       13 21 42  37.2 260.7  3.6      60.0     0    54378   Stopped 
19 44 32  ---          13 22 42  36.9 260.9  3.6      60.1    60    54378           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

19 45 00  1055+018     13 23 11  45.2 236.4  2.4      45.8     3    54378   19 45 00
19 51 40  ---          13 29 52  44.0 238.0  2.5      46.9   400    54481   19 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

19 52 00  1055+018     13 30 12  43.9 238.1  2.5      47.0    14    54481   19 52 00
19 55 20  ---          13 33 33  43.3 238.9  2.6      47.5   200    54532   19 52 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

19 57 31  P-RLEO       13 35 44  34.2 262.8  3.8      60.5   106    54532   Stopped 
19 58 31  ---          13 36 44  34.0 262.9  3.8      60.6    60    54532           

 ---------- Following scan added by Sched for reference pointing ----------

19 58 37  P-RLEO       13 36 50  33.9 263.0  3.8      60.6     0    54532   Stopped 
19 59 37  ---          13 37 51  33.7 263.1  3.8      60.6    60    54532           
Schedule for VLBA_FD   (Code Fd )                                   Page 234
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 00 00  OJ287        13 38 13  26.3 278.7  4.7      64.9     0    54532   20 00 00
20 06 40  ---          13 44 54  24.8 279.5  4.8      64.6   400    54634   20 00 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 07 00  OJ287        13 45 14  24.8 279.5  4.8      64.6    14    54634   20 07 00
20 10 20  ---          13 48 35  24.1 279.9  4.9      64.5   200    54686   20 07 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

20 12 28  P-RLEO       13 50 43  31.0 264.9  4.0      60.9   106    54686   Stopped 
20 13 28  ---          13 51 43  30.8 265.1  4.1      61.0    60    54686           

 ---------- Following scan added by Sched for reference pointing ----------

20 13 34  P-RLEO       13 51 49  30.7 265.1  4.1      61.0     0    54686   Stopped 
20 14 34  ---          13 52 50  30.5 265.2  4.1      61.0    60    54686           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 15 00  1055+018     13 53 16  39.6 243.2  2.9      50.2     0    54686   20 15 00
20 21 40  ---          13 59 57  38.3 244.6  3.0      51.0   400    54788   20 15 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 22 00  1055+018     14 00 17  38.2 244.7  3.0      51.1    14    54788   20 22 00
20 25 20  ---          14 03 37  37.6 245.3  3.1      51.5   200    54840   20 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page 235
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

20 27 28  P-RLEO       14 05 45  27.7 267.0  4.3      61.2   101    54840   Stopped 
20 28 28  ---          14 06 45  27.5 267.1  4.3      61.2    60    54840           

 ---------- Following scan added by Sched for reference pointing ----------

20 28 34  P-RLEO       14 06 52  27.5 267.1  4.3      61.2     0    54840   Stopped 
20 29 34  ---          14 07 52  27.3 267.3  4.3      61.2    60    54840           

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 30 00  1055+018     14 08 18  36.6 246.2  3.2      52.0     0    54840   20 30 00
20 36 40  ---          14 14 59  35.3 247.5  3.3      52.7   400    54942   20 30 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 37 00  1055+018     14 15 19  35.3 247.6  3.3      52.7    14    54942   20 37 00
20 40 20  ---          14 18 40  34.6 248.2  3.3      53.0   200    54993   20 37 01

 ---------- Following scan added by Sched for reference pointing ----------

 Next scan frequencies:  43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
                         43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
 Next BBC frequencies:     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
                           784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00

20 42 16  3C279        14 20 36  48.4 212.3  1.4      27.5    81    54993   Stopped 
20 43 16  ---          14 21 37  48.3 212.6  1.4      27.8    60    54993           

 ---------- Following scan added by Sched for reference pointing ----------

20 43 22  3C279        14 21 43  48.2 212.7  1.4      27.8     0    54993   Stopped 
20 44 22  ---          14 22 43  48.1 213.0  1.4      28.1    60    54993           
Schedule for VLBA_FD   (Code Fd )                                   Page 236
               GMVA Sep 25-29, 2014
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  29 Sep 2014   Day 272 ---

 Next scan frequencies:  86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
                         86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
 Next BBC frequencies:     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
                           752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00

20 45 00  1055+018     14 23 21  33.7 249.0  3.4      53.5     1    54993   20 45 00
20 51 40  ---          14 30 02  32.3 250.2  3.5      54.1   400    55096   20 45 01

 Next scan frequencies:  43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
                         43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
 Next BBC frequencies:     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
                           752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00

20 52 00  1055+018     14 30 22  32.2 250.3  3.5      54.1    14    55096   20 52 00
20 55 20  ---          14 33 42  31.6 250.8  3.6      54.4   200    55147   20 52 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: /aux/vlb056a/p459kri/sched-11.3/setups/ptr7mm.set
   Matching groups in 3mmfreq_RDBE.dat:
     v7mm_c8

   Setup group:   28         Station: VLBA_FD           Total bit rate:  2048
   Format: NONE              Bits per sample: 2         Sample rate: 64.000
   Number of channels: 16    DBE type: RDBE_PFB

   Setup not used for recording data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
            42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         L         L         L         L         L         L         L         L
                   L         L         L         L         L         L         L         L
   IF SB =         U         U         U         U         U         U         U         U
                   U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
                RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
                   9        10        11        12        13        14        15        16
   BBC SB=         L         L         L         L         L         L         L         L
                   L         L         L         L         L         L         L         L
   IF    =        A         C         A         C         A         C         A         C 
                  A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=  15.1      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   5  Setup file default.  Used with CRDFREQ or CRDDOP.  Used with PCAL = off
   LO sum=   43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
             43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
   BBC fr=     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
               784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  2 channels based on RDBE channels:   1  2
   CRD fr=     719.80    719.80
   CRD bw=       2.00      2.00
    Matching frequency sets:   5   6   7   8   9  29  30  31

   Frequency Set:  10  Setup file default.  Used with CRDFREQ or CRDDOP.  Used with PCAL = off
   LO sum=   43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
             43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
   BBC fr=     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
               784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  2 channels based on RDBE channels:   1  2
   CRD fr=     724.96    724.96
   CRD bw=       2.00      2.00
    Matching frequency sets:  10  11  12  82  83  84  85  86

   Frequency Set:  32  Setup file default.  Used with PCAL = 1MHz
   LO sum=   43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
             43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
   BBC fr=     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
               784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   5  6 11 12
   CRD fr=     840.01    840.01    744.01    744.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  32  33  34  35  36  37  38  57

   Frequency Set:  41  Setup file default.  Used with CRDFREQ or CRDDOP.  Used with PCAL = off
   LO sum=   43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
             43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
   BBC fr=     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
               784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  2 channels based on RDBE channels:   1  2
   CRD fr=     716.89    716.89
   CRD bw=       2.00      2.00
    Matching frequency sets:  41  42  95  96  97  98  99 122

   Frequency Set:  43  Setup file default.  Used with CRDFREQ or CRDDOP.  Used with PCAL = off
   LO sum=   43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
             43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
   BBC fr=     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
               784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  2 channels based on RDBE channels:   1  2
   CRD fr=     722.65    722.65
   CRD bw=       2.00      2.00
    Matching frequency sets:  43  44  45  46  47  56 129 130

   Frequency Set:  49  Setup file default.  Used with CRDFREQ or CRDDOP.  Used with PCAL = off
   LO sum=   43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
             43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
   BBC fr=     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
               784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  2 channels based on RDBE channels:   1  2
   CRD fr=     725.26    725.26
   CRD bw=       2.00      2.00
    Matching frequency sets:  49  50  51  52  53  54  55 106

   Frequency Set:  58  Setup file default.  Used with CRDFREQ or CRDDOP.  Used with PCAL = off
   LO sum=   43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
             43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
   BBC fr=     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
               784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  2 channels based on RDBE channels:   1  2
   CRD fr=     719.61    719.61
   CRD bw=       2.00      2.00
    Matching frequency sets:  58  59  60  61  62 123 124 125

   Frequency Set:  63  Setup file default.  Used with CRDFREQ or CRDDOP.  Used with PCAL = off
   LO sum=   43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
             43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
   BBC fr=     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
               784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  2 channels based on RDBE channels:   1  2
   CRD fr=     722.99    722.99
   CRD bw=       2.00      2.00
    Matching frequency sets:  63  64  65  66  67  68  69  70

   Frequency Set:  71  Setup file default.  Used with CRDFREQ or CRDDOP.  Used with PCAL = off
   LO sum=   43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
             43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
   BBC fr=     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
               784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  2 channels based on RDBE channels:   1  2
   CRD fr=     724.27    724.27
   CRD bw=       2.00      2.00
    Matching frequency sets:  71  72  73  74  75  79  80  81

   Frequency Set:  76  Setup file default.  Used with CRDFREQ or CRDDOP.  Used with PCAL = off
   LO sum=   43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
             43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
   BBC fr=     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
               784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  2 channels based on RDBE channels:   1  2
   CRD fr=     725.40    725.40
   CRD bw=       2.00      2.00
    Matching frequency sets:  76  77  78 101 109 110 111 112

   Frequency Set:  87  Setup file default.  Used with CRDFREQ or CRDDOP.  Used with PCAL = off
   LO sum=   43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
             43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
   BBC fr=     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
               784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  2 channels based on RDBE channels:   1  2
   CRD fr=     717.65    717.65
   CRD bw=       2.00      2.00
    Matching frequency sets:  87  88  89  90  91  92  93  94

   Frequency Set: 100  Setup file default.  Used with CRDFREQ or CRDDOP.  Used with PCAL = off
   LO sum=   43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
             43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
   BBC fr=     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
               784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  2 channels based on RDBE channels:   1  2
   CRD fr=     724.82    724.82
   CRD bw=       2.00      2.00
    Matching frequency sets: 100 102 103 104 105 107 108

   Frequency Set: 113  Setup file default.  Used with CRDFREQ or CRDDOP.  Used with PCAL = off
   LO sum=   43312.00  43312.00  43280.00  43280.00  43248.00  43248.00  43216.00  43216.00
             43184.00  43184.00  43152.00  43152.00  43120.00  43120.00  43088.00  43088.00
   BBC fr=     912.00    912.00    880.00    880.00    848.00    848.00    816.00    816.00
               784.00    784.00    752.00    752.00    720.00    720.00    688.00    688.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  2 channels based on RDBE channels:   1  2
   CRD fr=     723.09    723.09
   CRD bw=       2.00      2.00
    Matching frequency sets: 113 114 115 116 117 119 120 121


 ======== Setup file: 3mm_RDBE.set
   Matching groups in 3mmfreq_RDBE.dat:
     v3mm_ff

   Setup group:    1         Station: VLBA_FD           Total bit rate:  2048
   Format: MARK5B            Bits per sample: 2         Sample rate: 64.000
   Number of channels: 16    DBE type: RDBE_PFB         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  85500.00  85500.00  85500.00  85500.00  85500.00  85500.00  85500.00  85500.00
            85500.00  85500.00  85500.00  85500.00  85500.00  85500.00  85500.00  85500.00
   Net SB=         L         L         L         L         L         L         L         L
                   L         L         L         L         L         L         L         L
   IF SB =         U         U         U         U         U         U         U         U
                   U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
                RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
                   9        10        11        12        13        14        15        16
   BBC SB=         L         L         L         L         L         L         L         L
                   L         L         L         L         L         L         L         L
   IF    =        B         D         B         D         B         D         B         D 
                  B         D         B         D         B         D         B         D 

   VLBA FE=     omit     3mm      omit     3mm 
   VLBA Synth=  12.9     15.4     12.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  13  Setup file default.  Used with PCAL = 1MHz
   LO sum=   86380.00  86380.00  86348.00  86348.00  86316.00  86316.00  86284.00  86284.00
             86252.00  86252.00  86220.00  86220.00  86188.00  86188.00  86156.00  86156.00
   BBC fr=     880.00    880.00    848.00    848.00    816.00    816.00    784.00    784.00
               752.00    752.00    720.00    720.00    688.00    688.00    656.00    656.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   5  6 11 12
   CRD fr=     808.01    808.01    712.01    712.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  13  14  15  16  17  18  19  20

   Track assignments are: 
    track1=   2,  4,  6,  8, 10, 12, 14, 16, 18, 20, 22, 24, 26, 28, 30, 32
    barrel=roll_off 


 ======== Setup file: 7mm_RDBE.set
   Matching groups in 3mmfreq_RDBE.dat:
     v7mm_c8

   Setup group:   17         Station: VLBA_FD           Total bit rate:  2048
   Format: MARK5B            Bits per sample: 2         Sample rate: 64.000
   Number of channels: 16    DBE type: RDBE_PFB         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
            42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         L         L         L         L         L         L         L         L
                   L         L         L         L         L         L         L         L
   IF SB =         U         U         U         U         U         U         U         U
                   U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
                RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
                   9        10        11        12        13        14        15        16
   BBC SB=         L         L         L         L         L         L         L         L
                   L         L         L         L         L         L         L         L
   IF    =        A         C         A         C         A         C         A         C 
                  A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=  15.1      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  21  Setup file default.  Used with PCAL = 1MHz
   LO sum=   43024.00  43024.00  43056.00  43056.00  43088.00  43088.00  43120.00  43120.00
             43152.00  43152.00  43184.00  43184.00  43216.00  43216.00  43248.00  43248.00
   BBC fr=     624.00    624.00    656.00    656.00    688.00    688.00    720.00    720.00
               752.00    752.00    784.00    784.00    816.00    816.00    848.00    848.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
                32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   5  6 11 12
   CRD fr=     680.01    680.01    776.01    776.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  21  22  23  24  25  26  27  28

   Track assignments are: 
    track1=   2,  4,  6,  8, 10, 12, 14, 16, 18, 20, 22, 24, 26, 28, 30, 32
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   J0238+1636        02 35 52.630215   * 02 38 38.930107     02 39 29.546281       0.10
 * 0235+164          16 24 04.01608    * 16 36 59.27450      16 40 47.35595        0.10
   J0238+16          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 64883 observations

   J0319+4130        03 16 29.567260   * 03 19 48.160090     03 20 48.736093       1.30
   0316+413          41 19 51.91699    * 41 30 42.10412      41 33 43.86618        2.72
 * 3C84              /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
   J0319+41          GSFC 2011B astro solution      9957 Observations

   J0418+3801        04 15 00.610264   * 04 18 21.277237     04 19 21.901416       0.15
   0415+379          37 54 19.28071    * 38 01 35.80018      38 03 31.81280        0.13
 * 3C111             /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
   J0418+38          rfc_2012b Petrov, 2012, unpublished 200 observations

   J0423-0120        04 20 43.539850   * 04 23 15.800727     04 24 01.603324       0.10
 * 0420-014         -01 27 28.70025    *-01 20 33.06555     -01 18 30.54184        0.10
   J0423-01          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 38616 observations

   J0433+0521        04 30 31.602058   * 04 33 11.095527     04 33 59.027425       0.47
   0430+052          05 14 59.61643    * 05 21 15.61921      05 23 04.11346        0.35
 * 3C120             /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
   J0433+05          GSFC 2011B astro solution      8163 Observations

   J0721+7120        07 16 13.029741   * 07 21 53.448476     07 23 32.281461       0.31
 * 0716+714          71 26 15.17406    * 71 20 36.36340      71 18 29.34509        0.10
   J0721+71          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 27599 observations

   J0830+2410        08 27 54.398594   * 08 30 52.086193     08 31 43.837154       0.11
 * 0827+243          24 21 07.66368    * 24 10 59.82027      24 07 52.05727        0.10
   J0830+24          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 3170 observations

   J0841+7053        08 36 21.556645   * 08 41 24.365283     08 42 50.153051       0.31
 * 0836+710          71 04 22.42740    * 70 53 42.17302      70 50 11.18578        0.10
   J0841+70          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 4322 observations

   J0854+2006        08 51 57.250618   * 08 54 48.874930     08 55 38.754449       0.11
   0851+202          20 17 58.41733    * 20 06 30.64078      20 03 01.58098        0.10
   J0854+20          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
 * OJ287             rfc_2012b Petrov, 2012, unpublished 191510 observations

   J0927+3902        09 23 55.319217   * 09 27 03.013938     09 27 57.029645       0.13
   0923+392          39 15 23.56637    * 39 02 20.85177      38 58 20.28425        0.10
 * 4C39.25           /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
   J0927+39          rfc_2012b Petrov, 2012, unpublished 239566 observations

   J1058+0133        10 55 55.313729   * 10 58 29.605207     10 59 14.188851       0.10
 * 1055+018          01 50 03.53709    * 01 33 58.82359      01 29 17.69873        0.10
   J1058+01          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 7989 observations

   J1310+3220        13 08 07.560132   * 13 10 28.663851     13 11 08.733090       0.12
 * 1308+326          32 36 40.23870    * 32 20 43.78277      32 16 12.16202        0.10
   J1310+32          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 117803 observations

   J1512-0905        15 10 08.900178   * 15 12 50.532926     15 13 37.711432       0.10
 * 1510-089         -08 54 47.61966    *-09 05 59.82981     -09 09 05.71434        0.10
   J1512-09          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 6238 observations

   J1635+3808        16 33 30.625100   * 16 35 15.492975     16 35 45.799857       0.13
 * 1633+38           38 14 10.08266    * 38 08 04.50043      38 06 41.75745        0.10
   1633+382          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
   J1635+38          rfc_2012b Petrov, 2012, unpublished 16451 observations

   J1642+3948        16 41 17.606228   * 16 42 58.809965     16 43 28.068391       0.77
 * 3C345             39 54 10.81496    * 39 48 36.99402      39 47 24.14420        0.52
   1641+399          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
   J1642+39          GSFC 2011B astro solution     52621 Observations

   J1959+4044        19 57 44.453094   * 19 59 28.368821     20 00 00.162641     167.68
 * CYG-A             40 35 46.31273    * 40 44 02.04732      40 46 54.63726      120.15
   CYGNUS-A          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
   J1959+40          rfc_2012b Petrov, 2012, unpublished 3 observations
   1957+405
   1957+404

   J2015+3710        20 13 37.014489   * 20 15 28.729775     20 16 02.901294       0.16
 * 2013+370          37 01 44.45943    * 37 10 59.51531      37 14 08.58485        0.16
                     /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 282 observations

   J2202+4216        22 00 39.362504   * 22 02 43.291371     22 03 21.964533       0.14
 * BLLAC             42 02 08.59073    * 42 16 39.97987      42 21 16.36996        0.10
   2200+420          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
   J2202+42          rfc_2012b Petrov, 2012, unpublished 59418 observations
   VR422201

   J2232+1143        22 30 07.803947   * 22 32 36.408905     22 33 21.779312       0.10
 * CTA102            11 28 22.81066    * 11 43 50.90394      11 48 39.77864        0.10
   2230+114          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
   J2232+11          rfc_2012b Petrov, 2012, unpublished 5100 observations

   J2253+1608        22 51 29.519738   * 22 53 57.747937     22 54 43.138069       0.68
 * 3C454.3           15 52 54.34810    * 16 08 53.56093      16 13 50.78539        0.72
   2251+158          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
   J2253+16          GSFC 2011B astro solution     39747 Observations



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  0235+164   3mm_RDBE.set          1 2 3 13                          1.444    63.111
             7mm_RDBE.set          21 39 40                          0.722    25.167
  3C84       3mm_RDBE.set          1 2 3 4 13 118                    7.678   243.224
             7mm_RDBE.set          21 39 40 48                       2.333    89.611
  3C111      3mm_RDBE.set          1 2 3 4 13 118                    2.589   120.397
             7mm_RDBE.set          21 39 40 48                       1.167    42.500
  0420-014   3mm_RDBE.set          1 2 3 13 118                      0.778    24.778
             7mm_RDBE.set          21 39 40                          0.278     8.667
  3C120      3mm_RDBE.set          1 2 3 13 118                      2.000    64.222
             7mm_RDBE.set          21 39 40                          0.667    19.333
  0716+714   3mm_RDBE.set          1 2 3 13 118 126                  2.211   163.276
             7mm_RDBE.set          21 39 40                          0.778    35.000
  0827+243   3mm_RDBE.set          13                                1.050    26.949
             7mm_RDBE.set          21                                0.500    12.833
  0836+710   3mm_RDBE.set          1 2 3 13 118 126                  0.444    46.666
             7mm_RDBE.set          21 39 40                          0.222    10.000
  OJ287      3mm_RDBE.set          1 2 3 4 13 118                    7.456   253.127
             7mm_RDBE.set          21 39 40                          2.611    85.278
  4C39.25    3mm_RDBE.set          1 2 3 4 13                        5.200   163.210
             7mm_RDBE.set          21 39 40                          1.389    49.667
  1055+018   3mm_RDBE.set          1 2 3 13                          3.111    88.321
             7mm_RDBE.set          21 39 40                          1.389    39.278
  1308+326   3mm_RDBE.set          1 2 3 4                           0.556     3.333
  1510-089   3mm_RDBE.set          2 3 13 118                        3.706   100.636
             7mm_RDBE.set          21 40                             1.833    43.944
  1633+38    3mm_RDBE.set          1 2 3 13 118                      1.222    63.933
             7mm_RDBE.set          21 39 40                          0.556    21.500
  3C345      3mm_RDBE.set          1 2 3 13 118                      1.222    71.111
             7mm_RDBE.set          21 39 40                          0.611    23.500
  CYG-A      3mm_RDBE.set          1 2 3 4 13                        5.583   171.335
  2013+370   3mm_RDBE.set          1 2 3 4 13                        2.400    72.186
  BLLAC      3mm_RDBE.set          1 2 3 4 13 118 126                4.922   175.412
             7mm_RDBE.set          21 39 40                          1.889    62.333
  CTA102     3mm_RDBE.set          1 2 3 13 118                      1.333    38.111
             7mm_RDBE.set          21 39 40                          0.444    13.833
  3C454.3    3mm_RDBE.set          1 2 3 4 13 118                    4.289    85.105
             7mm_RDBE.set          21 39 40                          1.000    28.167

 POSITIONS OF ADDITIONAL SOURCES USED ONLY IN NON-RECORDING SCANS

     An unused dummy source of a scan that becomes a geodetic segment will show up here.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   J1256-0547        12 53 35.831299   * 12 56 11.166567     12 56 56.123349       0.69
 * 3C279            -05 31 07.99595    *-05 47 21.52481     -05 52 00.28635        0.92
   1253-055          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
   J1256-05          GSFC 2011B astro solution      7402 Observations

   J1337-1257        13 34 59.803872   * 13 37 39.782777     13 38 26.238909       0.10
 * 1334-127         -12 42 09.74318    *-12 57 24.69345     -13 01 45.59164        0.10
   J1337-12          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 89827 observations

 * P-WXPSC           01 03 48.086953   * 01 06 25.990000     01 07 14.277031       0.00
                     12 19 51.25224    * 12 35 53.16000      12 40 42.73734        0.00
                     /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.pointing
                     Mopra catalogue, via Krichbaum
                     Doppler based on LSR frame and radio definition.  Velocities:
                          7.80     7.80

 * P-IKTAU           03 50 43.603662   * 03 53 28.710000     03 54 18.563402       0.00
   SIO-IKTAU         11 15 31.94775    * 11 24 22.60000      11 26 56.16462        0.00
   IKTAU             /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.pointing
                      SEST pos & vel.
                     Doppler based on LSR frame and radio definition.  Velocities:
                         35.00    35.00

 * P-TXCAM           04 56 41.340435   * 05 00 51.127000     05 02 06.332104       0.00
   SIO-TXCAM         56 06 29.52902    * 56 10 53.98000      56 11 50.99794        0.00
   TXCAM             /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.pointing
                     Baudry pos.
                     Doppler based on LSR frame and radio definition.  Velocities:
                          7.50     7.50

 * P-ORINEW2         05 32 47.025524   * 05 35 14.505000     05 35 58.502766       0.00
   SIO-ORIIRC2      -05 24 23.87948    *-05 22 30.45000     -05 21 57.08442        0.00
   ORIIRC2           /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.pointing
                     3mm test peakup @1MHz BW
                     Doppler based on LSR frame and radio definition.  Velocities:
                         -5.00    -5.00

 * P-RCNC            08 13 48.479873   * 08 16 33.826000     08 17 22.152481       0.00
                     11 52 51.97435    * 11 43 34.60000      11 40 45.20111        0.00
                     /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.pointing
                     Baudry pos, sest vel
                     Doppler based on LSR frame and radio definition.  Velocities:
                         14.00    14.00

 * P-RLMI            09 42 34.567622   * 09 45 34.100000     09 46 25.741235       0.00
   SIO-RLMI          34 44 34.72079    * 34 30 43.90000      34 26 31.65515        0.00
                     /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.pointing
                     sest
                     Doppler based on LSR frame and radio definition.  Velocities:
                          2.00     2.00

 * P-RLEO            09 44 52.219425   * 09 47 33.490000     09 48 20.195754       0.00
   SIO-RLEO          11 39 40.09214    * 11 25 43.99000      11 21 35.88536        0.00
   RLEO              /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.pointing
                     baudry pos, sest vel.
                     Doppler based on LSR frame and radio definition.  Velocities:
                          3.00     3.00

 * P-RHYA          * 13 49 58.500000     13 52 45.611058     13 53 34.270125       0.00
                   *-23 01 25.00000     -23 16 11.22637     -23 20 24.96957        0.00
                     /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.pointing
                     Jewell.
                     Doppler based on LSR frame and radio definition.  Velocities:
                        -11.30   -11.30

 * P-UHER            16 23 34.717051   * 16 25 47.520000     16 26 26.266271       0.00
   SIO-UHER          19 00 17.57350    * 18 53 32.80000      18 51 54.82927        0.00
                     /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.pointing
                     Doppler based on LSR frame and radio definition.  Velocities:
                        -14.00   -14.00

 * P-VXSGR           18 05 02.981516   * 18 08 04.062000     18 08 57.756608       0.00
   SIO-VXSGR        -22 13 54.77916    *-22 13 26.10000     -22 13 06.54348        0.00
   VXSGRSIO          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.pointing
                      baudry pos, sest vel 2MHz BW
                     Doppler based on LSR frame and radio definition.  Velocities:
                          5.00     5.00

 * P-GYAQL           19 47 24.550758   * 19 50 06.350000     19 50 54.814737       0.00
   SIO-GYAQL        -07 44 30.74822    *-07 36 52.80000     -07 34 21.90838        0.00
                     /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.pointing
                      sest
                     Doppler based on LSR frame and radio definition.  Velocities:
                         30.00    30.00

 * P-RRAQL           19 55 00.381041   * 19 57 36.160000     19 58 22.901603       0.00
                    -02 01 17.53981    *-01 53 10.50000     -01 50 29.42116        0.00
                     /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.pointing
                     sest
                     Doppler based on LSR frame and radio definition.  Velocities:
                         26.90    26.90



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   0235+164           141.9
   3C84               122.7
   3C111              113.9
   0420-014           118.1
   3C120              115.8
   0716+714            86.5
   0827+243            60.4
   0836+710            80.5
   OJ287               53.9
   4C39.25             56.3
   1055+018            19.7
   3C279               10.8
   1308+326            36.4
   1334-127            23.1
   1510-089            44.6
   1633+38             71.6
   3C345               73.5
   CYG-A              110.5
   2013+370           114.5
   BLLAC              129.7
   CTA102             152.5
   3C454.3            155.2
   P-WXPSC            163.5
   P-IKTAU            125.2
   P-TXCAM            101.8
   P-ORINEW2          100.0
   P-RCNC              61.0
   P-RLMI              50.6
   P-RLEO              39.2
   P-RHYA              31.8
   P-UHER              64.7
   P-VXSGR             87.5
   P-GYAQL            113.0
   P-RRAQL            115.3

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

