  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: The nuclear structure of 3C84 with Space VLBI - II Epoch
 Exp. Code:  gg080   


Schedule Version:       1.10
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Gabriele Giovannini

Address:  Istituto di Radioastronomia - INAF
          via Gobetti 101
          40129 Bologna, Italy
 

Phone:    +390516399415
EMAIL:    ggiovann@ira.inaf.it
Fax:
Phone during observation: +79165452842

Observing mode: K/C-band, dual-pol

Notes:    K/C-band, Radioastron-compatible frequency setup
          P-CAL is ON
          Tsys is ON
          auto-level (AGC) is ON

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               The nuclear structure of 3C84 with Space VLBI - II Epoch
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Sep 2016   Day 256 ---

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00
 Next scan bandwidths:      16.00     16.00     16.00     16.00

05 00 30  0316+413     21 31 16  21.5  53.5 -5.8     -67.5     0        0   05 00 30
05 15 00  ---          21 45 48  24.1  54.5 -5.6     -69.5   870       28   05 00 31

 ---------- CUQX-band VLBI scans. Ground-only segment 04 ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

05 16 00  0316+413     21 46 49  24.2  54.6 -5.6     -69.7    54       28   05 16 00
05 26 00  ---          21 56 50  26.0  55.3 -5.4     -71.0   600       47   05 16 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

05 27 00  0316+413     21 57 50  26.2  55.4 -5.4     -71.2    54       47   05 27 00
05 36 00  ---          22 06 52  27.8  56.0 -5.2     -72.4   540       65   05 27 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

05 37 00  0316+413     22 07 52  28.0  56.0 -5.2     -72.5    54       65   05 37 00
05 46 00  ---          22 16 54  29.6  56.6 -5.1     -73.8   540       82   05 37 01

 Next scan frequencies:  8367.25  8367.25  8367.25  8367.25
 Next BBC frequencies:    767.25   767.25   767.25   767.25

05 47 00  0316+413     22 17 54  29.8  56.7 -5.1     -73.9    54       82   05 47 00
05 56 00  ---          22 26 55  31.4  57.2 -4.9     -75.1   540      100   05 47 01

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

05 57 00  0316+413     22 27 55  31.6  57.2 -4.9     -75.3    54      100   05 57 00
06 06 00  ---          22 36 57  33.2  57.7 -4.7     -76.5   540      117   05 57 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

06 07 00  0316+413     22 37 57  33.4  57.8 -4.7     -76.6    54      117   06 07 00
06 16 00  ---          22 46 58  35.0  58.2 -4.6     -77.9   540      134   06 07 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

06 17 00  0316+413     22 47 59  35.2  58.3 -4.5     -78.0    54      134   06 17 00
06 26 00  ---          22 57 00  36.9  58.7 -4.4     -79.3   540      152   06 17 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               The nuclear structure of 3C84 with Space VLBI - II Epoch
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Sep 2016   Day 256 ---

 Next scan frequencies:  8367.25  8367.25  8367.25  8367.25
 Next BBC frequencies:    767.25   767.25   767.25   767.25

06 27 00  0316+413     22 58 00  37.1  58.7 -4.4     -79.4    54      152   06 27 00
06 36 00  ---          23 07 02  38.7  59.1 -4.2     -80.7   540      169   06 27 01

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

06 37 00  0316+413     23 08 02  38.9  59.1 -4.2     -80.8    54      169   06 37 00
06 46 00  ---          23 17 03  40.6  59.5 -4.1     -82.1   540      186   06 37 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

06 47 00  0316+413     23 18 04  40.8  59.5 -4.0     -82.3    54      186   06 47 00
06 56 00  ---          23 27 05  42.4  59.8 -3.9     -83.6   540      204   06 47 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

06 57 00  0316+413     23 28 05  42.6  59.8 -3.9     -83.7    54      204   06 57 00
07 06 00  ---          23 37 07  44.3  60.0 -3.7     -85.1   540      221   06 57 01

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

07 06 30  0300+470     23 37 37  47.3  51.8 -3.5     -93.9    16      221   07 06 30
07 16 00  ---          23 47 08  49.0  51.6 -3.3     -95.8   570      240   07 06 31

07 16 30  0300+470     23 47 38  49.0  51.6 -3.3     -95.9    24      240   07 16 30
07 26 00  ---          23 57 10  50.6  51.3 -3.1     -97.9   570      258   07 16 31

07 26 30  0300+470     23 57 40  50.7  51.3 -3.1     -98.0    24      258   07 26 30
07 36 00  ---          00 07 12  52.3  50.9 -3.0    -100.1   570      276   07 26 31

 ---------- CUQX-band VLBI scans cont. Ground-only segment 04 ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

07 36 30  0316+413     00 07 42  50.0  60.4 -3.2     -89.9    15      276   07 36 30
07 46 30  ---          00 17 43  51.9  60.4 -3.1     -91.6   600      296   07 36 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

07 47 30  0316+413     00 18 44  52.1  60.4 -3.0     -91.7    54      296   07 47 30
07 56 30  ---          00 27 45  53.8  60.2 -2.9     -93.3   540      313   07 47 31
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               The nuclear structure of 3C84 with Space VLBI - II Epoch
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Sep 2016   Day 256 ---

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

07 57 30  0316+413     00 28 45  54.0  60.2 -2.9     -93.5    54      313   07 57 30
08 06 30  ---          00 37 47  55.6  60.0 -2.7     -95.2   540      330   07 57 31

 Next scan frequencies:  8367.25  8367.25  8367.25  8367.25
 Next BBC frequencies:    767.25   767.25   767.25   767.25

08 07 30  0316+413     00 38 47  55.8  60.0 -2.7     -95.4    54      330   08 07 30
08 16 30  ---          00 47 48  57.5  59.6 -2.6     -97.2   540      348   08 07 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

08 17 30  0316+413     00 48 48  57.7  59.6 -2.5     -97.4    54      348   08 17 30
08 26 30  ---          00 57 50  59.4  59.1 -2.4     -99.3   540      365   08 17 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

08 27 30  0316+413     00 58 50  59.5  59.1 -2.4     -99.5    54      365   08 27 30
08 36 30  ---          01 07 52  61.2  58.4 -2.2    -101.5   540      383   08 27 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

08 37 30  0316+413     01 08 52  61.4  58.4 -2.2    -101.7    54      383   08 37 30
08 46 30  ---          01 17 53  63.0  57.6 -2.1    -104.0   540      400   08 37 31

 Next scan frequencies:  8367.25  8367.25  8367.25  8367.25
 Next BBC frequencies:    767.25   767.25   767.25   767.25

08 47 30  0316+413     01 18 53  63.2  57.4 -2.0    -104.2    54      400   08 47 30
08 56 30  ---          01 27 55  64.8  56.4 -1.9    -106.6   540      417   08 47 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

08 57 30  0316+413     01 28 55  65.0  56.3 -1.9    -106.9    54      417   08 57 30
09 04 00  ---          01 35 26  66.2  55.4 -1.8    -108.8   390      430   08 57 31

 ---------- C-band VLBA scans. Space segment 05 ----------

09 05 00  0316+413     01 36 26  66.4  55.2 -1.7    -109.1    54      430   09 05 00
09 20 00  ---          01 51 29  69.0  52.5 -1.5    -114.1   900      459   09 05 01

09 20 30  0316+413     01 51 59  69.1  52.4 -1.5    -114.3    24      459   09 20 30
09 35 00  ---          02 06 31  71.5  48.7 -1.2    -120.2   870      487   09 20 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               The nuclear structure of 3C84 with Space VLBI - II Epoch
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Sep 2016   Day 256 ---

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

09 35 30  0316+413     02 07 01  71.6  48.6 -1.2    -120.4    24      487   09 35 30
09 50 00  ---          02 21 34  73.8  43.4 -1.0    -127.7   870      515   09 35 31

09 50 30  0316+413     02 22 04  73.9  43.2 -1.0    -128.0    24      515   09 50 30
10 05 00  ---          02 36 36  75.9  36.2 -0.7    -137.3   870      543   09 50 31

 ---------- CUQX-band VLBI scans. Ground-only segment 05 ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

10 06 00  0316+413     02 37 36  76.0  35.6 -0.7    -138.0    54      543   10 06 00
10 16 00  ---          02 47 38  77.2  29.2 -0.6    -145.9   600      562   10 06 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

10 17 00  0316+413     02 48 38  77.3  28.5 -0.5    -146.7    54      562   10 17 00
10 26 00  ---          02 57 40  78.1  21.6 -0.4    -155.0   540      580   10 17 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

10 27 00  0316+413     02 58 40  78.2  20.8 -0.4    -155.9    54      580   10 27 00
10 36 00  ---          03 07 41  78.7  12.8 -0.2    -165.3   540      597   10 27 01

 Next scan frequencies:  8367.25  8367.25  8367.25  8367.25
 Next BBC frequencies:    767.25   767.25   767.25   767.25

10 37 00  0316+413     03 08 41  78.8  11.9 -0.2    -166.3    54      597   10 37 00
10 46 00  ---          03 17 43  79.0   3.2 -0.1    -176.4   540      614   10 37 01

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

10 47 00  0316+413     03 18 43  79.1   2.2 -0.0    -177.5    54      614   10 47 00
10 56 00  ---          03 27 44  79.0  -6.7  0.1     172.3   540      632   10 47 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

10 57 00  0316+413     03 28 45  79.0  -7.7  0.1     171.2    54      632   10 57 00
11 06 00  ---          03 37 46  78.6 -16.1  0.3     161.4   540      649   10 57 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

11 07 00  0316+413     03 38 46  78.5 -17.0  0.3     160.4    54      649   11 07 00
11 16 00  ---          03 47 48  77.8 -24.5  0.4     151.5   540      667   11 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               The nuclear structure of 3C84 with Space VLBI - II Epoch
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Sep 2016   Day 256 ---

 Next scan frequencies:  8367.25  8367.25  8367.25  8367.25
 Next BBC frequencies:    767.25   767.25   767.25   767.25

11 17 00  0316+413     03 48 48  77.7 -25.2  0.5     150.6    54      667   11 17 00
11 26 00  ---          03 57 49  76.8 -31.6  0.6     142.9   540      684   11 17 01

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

11 27 00  0316+413     03 58 50  76.7 -32.3  0.6     142.1    54      684   11 27 00
11 36 00  ---          04 07 51  75.6 -37.6  0.8     135.5   540      701   11 27 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

11 37 00  0316+413     04 08 51  75.4 -38.1  0.8     134.8    54      701   11 37 00
11 46 00  ---          04 17 53  74.2 -42.4  0.9     129.1   540      719   11 37 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

11 47 00  0316+413     04 18 53  74.0 -42.9  1.0     128.5    54      719   11 47 00
11 56 00  ---          04 27 54  72.7 -46.3  1.1     123.7   540      736   11 47 01

 Next scan frequencies:  8367.25  8367.25  8367.25  8367.25
 Next BBC frequencies:    767.25   767.25   767.25   767.25

11 57 00  0316+413     04 28 54  72.5 -46.7  1.1     123.2    54      736   11 57 00
12 06 00  ---          04 37 56  71.1 -49.5  1.3     119.1   540      754   11 57 01

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

12 07 00  0316+413     04 38 56  70.9 -49.7  1.3     118.6    54      754   12 07 00
12 16 00  ---          04 47 58  69.4 -52.0  1.5     115.0   540      771   12 07 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

12 17 00  0316+413     04 48 58  69.2 -52.2  1.5     114.7    54      771   12 17 00
12 26 00  ---          04 57 59  67.7 -54.0  1.6     111.5   540      788   12 17 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

12 27 00  0316+413     04 58 59  67.5 -54.2  1.6     111.2    54      788   12 27 00
12 36 00  ---          05 08 01  65.9 -55.6  1.8     108.3   540      806   12 27 01

 Next scan frequencies:  8367.25  8367.25  8367.25  8367.25
 Next BBC frequencies:    767.25   767.25   767.25   767.25

12 37 00  0316+413     05 09 01  65.7 -55.8  1.8     108.0    54      806   12 37 00
12 46 00  ---          05 18 03  64.1 -56.9  2.0     105.5   540      823   12 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               The nuclear structure of 3C84 with Space VLBI - II Epoch
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Sep 2016   Day 256 ---

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

12 47 00  0316+413     05 19 03  63.9 -57.0  2.0     105.2    54      823   12 47 00
12 56 00  ---          05 28 04  62.3 -57.9  2.1     102.9   540      841   12 47 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

12 57 00  0316+413     05 29 04  62.1 -58.0  2.1     102.7    54      841   12 57 00
13 06 00  ---          05 38 06  60.5 -58.7  2.3     100.6   540      858   12 57 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

13 07 00  0316+413     05 39 06  60.3 -58.8  2.3     100.3    54      858   13 07 00
13 16 00  ---          05 48 07  58.6 -59.3  2.5      98.4   540      875   13 07 01

 Next scan frequencies:  8367.25  8367.25  8367.25  8367.25
 Next BBC frequencies:    767.25   767.25   767.25   767.25

13 17 00  0316+413     05 49 08  58.4 -59.4  2.5      98.2    54      875   13 17 00
13 26 00  ---          05 58 09  56.7 -59.8  2.6      96.3   540      893   13 17 01

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

13 27 00  0316+413     05 59 09  56.6 -59.8  2.6      96.1    54      893   13 27 00
13 36 00  ---          06 08 11  54.9 -60.1  2.8      94.4   540      910   13 27 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

13 37 00  0316+413     06 09 11  54.7 -60.1  2.8      94.2    54      910   13 37 00
13 46 00  ---          06 18 12  53.0 -60.3  3.0      92.6   540      927   13 37 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

13 47 00  0316+413     06 19 13  52.8 -60.3  3.0      92.4    54      927   13 47 00
13 54 10  ---          06 26 24  51.5 -60.4  3.1      91.2   430      941   13 47 01

 ---------- K-band VLBI scans. Space segment 06 ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

13 55 00  0316+413     06 27 14  51.3 -60.4  3.1      91.0    44      941   13 55 00
14 10 00  ---          06 42 16  48.5 -60.4  3.4      88.5   900      970   13 55 01

14 10 30  0316+413     06 42 46  48.4 -60.4  3.4      88.5    24      970   14 10 30
14 25 00  ---          06 57 19  45.7 -60.2  3.6      86.2   870      998   14 10 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               The nuclear structure of 3C84 with Space VLBI - II Epoch
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Sep 2016   Day 256 ---

14 25 30  0316+413     06 57 49  45.6 -60.2  3.6      86.1    24      998   14 25 30
14 40 00  ---          07 12 21  42.9 -59.8  3.9      83.9   870     1026   14 25 31

14 40 30  0316+413     07 12 51  42.8 -59.8  3.9      83.9    24     1026   14 40 30
14 55 00  ---          07 27 24  40.1 -59.4  4.1      81.7   870     1054   14 40 31

 ---------- CUQX-band VLBI scans. Ground-only segment 05 ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

14 56 00  0316+413     07 28 24  39.9 -59.3  4.1      81.6    54     1054   14 56 00
15 06 00  ---          07 38 26  38.1 -59.0  4.3      80.2   600     1074   14 56 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

15 07 00  0316+413     07 39 26  37.9 -58.9  4.3      80.0    54     1074   15 07 00
15 16 00  ---          07 48 27  36.2 -58.5  4.5      78.8   540     1091   15 07 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

15 17 00  0316+413     07 49 27  36.0 -58.5  4.5      78.6    54     1091   15 17 00
15 26 00  ---          07 58 29  34.4 -58.1  4.6      77.4   540     1108   15 17 01

 Next scan frequencies:  8367.25  8367.25  8367.25  8367.25
 Next BBC frequencies:    767.25   767.25   767.25   767.25

15 27 00  0316+413     07 59 29  34.2 -58.0  4.6      77.2    54     1108   15 27 00
15 36 00  ---          08 08 30  32.6 -57.5  4.8      76.0   540     1126   15 27 01

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

15 37 00  0316+413     08 09 31  32.4 -57.5  4.8      75.9    54     1126   15 37 00
15 46 00  ---          08 18 32  30.7 -57.0  5.0      74.6   540     1143   15 37 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

15 47 00  0316+413     08 19 32  30.6 -56.9  5.0      74.5    54     1143   15 47 00
15 56 00  ---          08 28 34  28.9 -56.4  5.1      73.3   540     1161   15 47 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

15 57 00  0316+413     08 29 34  28.8 -56.3  5.1      73.1    54     1161   15 57 00
16 06 00  ---          08 38 35  27.2 -55.7  5.3      71.9   540     1178   15 57 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               The nuclear structure of 3C84 with Space VLBI - II Epoch
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Sep 2016   Day 256 ---

 Next scan frequencies:  8367.25  8367.25  8367.25  8367.25
 Next BBC frequencies:    767.25   767.25   767.25   767.25

16 07 00  0316+413     08 39 36  27.0 -55.7  5.3      71.8    54     1178   16 07 00
16 16 00  ---          08 48 37  25.4 -55.1  5.5      70.5   540     1195   16 07 01

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

16 17 00  0316+413     08 49 37  25.2 -55.0  5.5      70.4    54     1195   16 17 00
16 26 00  ---          08 58 39  23.6 -54.4  5.6      69.2   540     1213   16 17 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

16 27 00  0316+413     08 59 39  23.4 -54.3  5.6      69.0    54     1213   16 27 00
16 36 00  ---          09 08 40  21.9 -53.6  5.8      67.8   540     1230   16 27 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

16 37 00  0316+413     09 09 40  21.7 -53.5  5.8      67.7    54     1230   16 37 00
16 46 00  ---          09 18 42  20.1 -52.8  6.0      66.4   540     1248   16 37 01

 Next scan frequencies:  8367.25  8367.25  8367.25  8367.25
 Next BBC frequencies:    767.25   767.25   767.25   767.25

16 47 00  0316+413     09 19 42  20.0 -52.8  6.0      66.3    54     1248   16 47 00
16 56 00  ---          09 28 44  18.4 -52.0  6.1      65.0   540     1265   16 47 01

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

16 57 00  0316+413     09 29 44  18.3 -51.9  6.1      64.9    54     1265   16 57 00
17 06 00  ---          09 38 45  16.7 -51.2  6.3      63.6   540     1282   16 57 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

17 07 00  0316+413     09 39 45  16.6 -51.1  6.3      63.5    54     1282   17 07 00
17 16 00  ---          09 48 47  15.1 -50.3  6.5      62.2   540     1300   17 07 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

17 17 00  0316+413     09 49 47  14.9 -50.2  6.5      62.0    54     1300   17 17 00
17 26 00  ---          09 58 49  13.4 -49.3  6.6      60.8   540     1317   17 17 01

 Next scan frequencies:  8367.25  8367.25  8367.25  8367.25
 Next BBC frequencies:    767.25   767.25   767.25   767.25

17 27 00  0316+413     09 59 49  13.3 -49.3  6.6      60.6    54     1317   17 27 00
17 36 00  ---          10 08 50  11.8 -48.4  6.8      59.3   540     1335   17 27 01
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               The nuclear structure of 3C84 with Space VLBI - II Epoch
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Sep 2016   Day 256 ---

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

17 37 00  0316+413     10 09 50  11.6 -48.3  6.8      59.2    54     1335   17 37 00
17 46 00  ---          10 18 52  10.2 -47.4  7.0      57.8   540     1352   17 37 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

17 47 00  0316+413     10 19 52  10.0 -47.3  7.0      57.7    54     1352   17 47 00
17 56 00  ---          10 28 53   8.6 -46.4  7.1      56.3   540     1369   17 47 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25

17 57 00  0316+413     10 29 54   8.5 -46.3  7.1      56.2    54     1369   17 57 00
18 06 00  ---          10 38 55   7.1 -45.3  7.3      54.8   540     1387   17 57 01

 Next scan frequencies:  8367.25  8367.25  8367.25  8367.25
 Next BBC frequencies:    767.25   767.25   767.25   767.25

18 07 00  0316+413     10 39 55   6.9 -45.2  7.3      54.7    54     1387   18 07 00
18 19 00  ---          10 51 57   5.1 -43.8  7.5      52.8   720     1410   18 07 01

 ---------- K-band VLBI scans. Space segment 07 ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

18 20 00  0316+413     10 52 57   5.0 -43.7  7.5      52.7    54     1410   18 20 00
18 35 00  ---          11 08 00   2.8 -42.0  7.8  H   50.3     0     1439   18 20 01

18 35 30  0316+413     11 08 30   2.7 -41.9  7.8  H   50.2    24     1439   18 35 30
18 50 00  ---          11 23 02   0.6 -40.1  8.0  D   47.8     0     1467   18 35 31


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra1cm2.set
   Matching groups in ./gg080_freq.dat:
     v1cm_b3

   Setup group:    7         Station: VLBA_FD           Total bit rate:   256
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  20  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22236.00  22236.00  22236.00  22236.00
   BBC fr=     736.00    736.00    736.00    736.00
   Bandwd=      16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   1  2  3  4
   CRD fr=     736.01    736.01    735.99    735.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  20  21  22  23  24  25  26  27  28  69

   Track assignments are: 
    track1=   1,  2,  3,  4
    barrel=roll_off 


 ======== Setup file: ra6cm2.set
   Matching groups in ./gg080_freq.dat:
     vc_d

   Setup group:   36         Station: VLBA_FD           Total bit rate:   256
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  13.6      4.1     13.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  30  Setup file default.  Used with PCAL = 1MHz
   LO sum=   4836.00  4836.00  4836.00  4836.00
   BBC fr=    736.00   736.00   736.00   736.00
   Bandwd=     16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   1  2  3  4
   CRD fr=     736.01    736.01    735.99    735.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  30  31  32  33  34  35  36  37  38  70

   Track assignments are: 
    track1=   1,  2,  3,  4
    barrel=roll_off 


 ======== Setup file: ra2cm2.set
   Matching groups in ./gg080_freq.dat:
     v2cm_d3         Fourth 2cm filter

   Setup group:   59         Station: VLBA_FD           Total bit rate:   256
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14600.00  14600.00  14600.00  14600.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.6     10.9     10.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  40  Setup file default.  Used with PCAL = 1MHz
   LO sum=   15369.00  15369.00  15369.00  15369.00
   BBC fr=     769.00    769.00    769.00    769.00
   Bandwd=      16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   1  2  3  4
   CRD fr=     769.01    769.01    768.99    768.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  40  41  42  43  44  45  46  47  48  71

   Track assignments are: 
    track1=   1,  2,  3,  4
    barrel=roll_off 


 ======== Setup file: ra7mm2.set
   Matching groups in ./gg080_freq.dat:
     v7mm_c8

   Setup group:   70         Station: VLBA_FD           Total bit rate:   256
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=   3.9      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  50  Setup file default.  Used with PCAL = 1MHz
   LO sum=   43130.25  43130.25  43130.25  43130.25
   BBC fr=     730.25    730.25    730.25    730.25
   Bandwd=      16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   1  2  3  4
   CRD fr=     730.25    730.25    730.25    730.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  50  51  52  53  54  55  56  57  58  72

   Track assignments are: 
    track1=   1,  2,  3,  4
    barrel=roll_off 


 ======== Setup file: ra4cm2.set
   Matching groups in ./gg080_freq.dat:
     v4cm_3

   Setup group:   48         Station: VLBA_FD           Total bit rate:   256
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   7600.00   7600.00   7600.00   7600.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        B         D         B         D 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.1     15.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  60  Setup file default.  Used with PCAL = 1MHz
   LO sum=   8367.25  8367.25  8367.25  8367.25
   BBC fr=    767.25   767.25   767.25   767.25
   Bandwd=     16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   1  2  3  4
   CRD fr=     767.25    767.25    767.25    767.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  60  61  62  63  64  65  66  67  68  73

   Track assignments are: 
    track1=   1,  2,  3,  4
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 30.474820       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 31.69946        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

 * 0300+470          03 00 10.111206   * 03 03 35.242224     03 04 44.989300       0.00
   J0303+4716        47 04 33.67712    * 47 16 16.27546      47 19 54.94955        0.00
                     ./gg080_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 26473 observations, RA-AO3-04, RA-AO2-1

 * 0316+413          03 16 29.567283   * 03 19 48.160114     03 20 55.379781       0.00
   J0319+4130        41 19 51.91847    * 41 30 42.10559      41 34 04.14191        0.00
   3C84              ./gg080_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 15448 observations, RA-AO3-04, RA-AO2-1

 * 1823+568          18 23 14.951493   * 18 24 07.068371     18 24 25.083866       0.00
   J1824+5651        56 49 18.07195    * 56 51 01.49076      56 52 04.34072        0.00
                     ./gg080_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 8126 observations, RA-AO3-04, RA-AO2-12



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra1cm2.set            9                                 6.983     0.000
  0300+470   ra1cm2.set            1 2 3 4 5 6 8 10 14 15 16 1 +     2.875   346.707
  0316+413   ra1cm2.set            1 2 3 4 5 6 8 10 14 15 16 1 +    23.916  1659.187
             ra6cm2.set            29 30 74                          3.067   149.493
             ra4cm2.set            59 60                             2.150    94.250
             ra2cm2.set            39 40                             2.400   109.050
             ra7mm2.set            49 50                             2.369   107.675
  1823+568   ra1cm2.set            1 2 3 4 5 6 8 10 14 15 16 1 +     1.108    81.640


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA              81.0
   0300+470           109.3
   0316+413           109.4
   1823+568            95.0

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

