  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron AGN polarization imaging
 Exp. Code:  gg079a  


Schedule Version:       1.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Jose L. Gomez, Andrei Lobanov

Address:  Instituto de Astrofisica de Andalucia-CSIC
          Glorieta de la Astronomia
          E-18008 Granada, Spain
 

Phone:    +79165452842
EMAIL:    jlgomez@iaa.es, alobanov@mpifr-bonn.mpg.de
Fax:
Phone during observation: +79165452842

Observing mode: L-band, dual-pol

Notes:    L-band, Radioastron-compatible frequency setup
          P-CAL is ON
          Tsys is ON
          auto-level (AGC) is ON

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed  30 Mar 2016   Day  90 ---

 ---------- VLBA-only fringe finder 3C84 at X,L,U,C ----------

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00

23 00 00  3C84         04 39 15  70.8 -49.8  1.3     118.5     0        0   23 00 00
23 05 00  ---          04 44 16  70.0 -51.1  1.4     116.4   300       19   23 00 01

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

23 05 10  3C84         04 44 26  70.0 -51.2  1.4     116.4     4       19   23 05 10
23 10 10  ---          04 49 27  69.1 -52.3  1.5     114.5   300       39   23 05 11

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

23 10 20  3C84         04 49 37  69.1 -52.4  1.5     114.4     4       39   23 10 20
23 16 20  ---          04 55 38  68.1 -53.6  1.6     112.3   360       62   23 10 21

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

23 16 30  3C84         04 55 48  68.0 -53.6  1.6     112.2     4       62   23 16 30
23 20 30  ---          04 59 49  67.3 -54.3  1.6     110.9   240       77   23 16 31

 ---------- VLBA-only EVPA calibrator at C,U,L,X ----------

23 23 10  OJ287        05 02 29  36.8  86.9 -3.9     -66.1    52       77   23 23 10
23 29 10  ---          05 08 30  38.1  87.6 -3.8     -66.2   360      100   23 23 11

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

23 29 20  OJ287        05 08 40  38.1  87.6 -3.8     -66.2     4      100   23 29 20
23 38 20  ---          05 17 42  40.1  88.7 -3.6     -66.3   540      135   23 29 21

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

23 38 30  OJ287        05 17 52  40.1  88.7 -3.6     -66.3     4      135   23 38 30
23 46 30  ---          05 25 53  41.8  89.7 -3.5     -66.3   480      166   23 38 31

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

23 46 40  OJ287        05 26 03  41.9  89.8 -3.5     -66.3     4      166   23 46 40
23 54 40  ---          05 34 04  43.6  90.8 -3.4     -66.3   480      197   23 46 41
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed  30 Mar 2016   Day  90 ---

 ---------- VLBA-only EVPA calibrator OJ287 at L,C,X,U ----------

23 54 50  OJ287        05 34 14  43.6  90.8 -3.4     -66.3     4      197   23 54 50
23 59 50  ---          05 39 15  44.7  91.5 -3.3     -66.3   300      216   23 54 51

 --- Thu  31 Mar 2016   Day  91 ---

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

00 00 00  OJ287        05 39 25  44.8  91.5 -3.3     -66.3     4      216   00 00 00
00 05 00  ---          05 44 26  45.8  92.2 -3.2     -66.2   300      236   00 00 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

00 05 10  OJ287        05 44 36  45.9  92.2 -3.2     -66.2     4      236   00 05 10
00 11 10  ---          05 50 37  47.2  93.0 -3.1     -66.2   360      259   00 05 11

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

00 11 20  OJ287        05 50 47  47.2  93.1 -3.1     -66.2     4      259   00 11 20
00 15 20  ---          05 54 48  48.1  93.6 -3.0     -66.1   240      274   00 11 21

00 15 30  OJ287        05 54 58  48.1  93.6 -3.0     -66.1     4      274   00 15 30
00 19 30  ---          05 58 58  49.0  94.2 -2.9     -66.0   240      290   00 15 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

00 19 40  OJ287        05 59 08  49.0  94.2 -2.9     -66.0     4      290   00 19 40
00 25 40  ---          06 05 09  50.3  95.1 -2.8     -65.8   360      313   00 19 41

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

00 25 50  OJ287        06 05 19  50.3  95.2 -2.8     -65.8     4      313   00 25 50
00 30 50  ---          06 10 20  51.4  95.9 -2.8     -65.6   300      332   00 25 51

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

00 31 00  OJ287        06 10 30  51.4  96.0 -2.8     -65.6     4      332   00 31 00
00 36 00  ---          06 15 31  52.5  96.7 -2.7     -65.4   300      352   00 31 01

00 36 10  OJ287        06 15 41  52.5  96.8 -2.7     -65.4     4      352   00 36 10
00 41 10  ---          06 20 42  53.6  97.6 -2.6     -65.2   300      371   00 36 11
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  31 Mar 2016   Day  91 ---

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

00 41 20  OJ287        06 20 52  53.6  97.6 -2.6     -65.2     4      371   00 41 20
00 46 20  ---          06 25 53  54.7  98.5 -2.5     -64.9   300      390   00 41 21

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

00 46 30  OJ287        06 26 03  54.7  98.5 -2.5     -64.9     4      390   00 46 30
00 52 30  ---          06 32 04  56.0  99.6 -2.4     -64.6   360      414   00 46 31

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

00 52 40  OJ287        06 32 14  56.1  99.6 -2.4     -64.6     4      414   00 52 40
00 56 40  ---          06 36 14  56.9 100.3 -2.3     -64.3   240      429   00 52 41

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

00 56 50  OJ287        06 36 24  56.9 100.4 -2.3     -64.3     4      429   00 56 50
01 01 50  ---          06 41 25  58.0 101.3 -2.2     -63.9   300      448   00 56 51

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

01 02 00  OJ287        06 41 35  58.0 101.3 -2.2     -63.9     4      448   01 02 00
01 07 00  ---          06 46 36  59.1 102.3 -2.2     -63.5   300      468   01 02 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

01 07 10  OJ287        06 46 46  59.1 102.4 -2.1     -63.5     4      468   01 07 10
01 13 10  ---          06 52 47  60.4 103.6 -2.0     -62.9   360      491   01 07 11

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

01 13 20  OJ287        06 52 57  60.4 103.7 -2.0     -62.9     4      491   01 13 20
01 17 20  ---          06 56 58  61.3 104.6 -2.0     -62.4   240      506   01 13 21

01 17 30  OJ287        06 57 08  61.3 104.6 -2.0     -62.4     4      506   01 17 30
01 21 30  ---          07 01 08  62.1 105.5 -1.9     -61.9   240      522   01 17 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

01 21 40  OJ287        07 01 18  62.2 105.6 -1.9     -61.9     4      522   01 21 40
01 27 40  ---          07 07 19  63.4 107.0 -1.8     -61.1   360      545   01 21 41
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  31 Mar 2016   Day  91 ---

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

01 27 50  OJ287        07 07 29  63.4 107.1 -1.8     -61.1     4      545   01 27 50
01 32 50  ---          07 12 30  64.5 108.4 -1.7     -60.4   300      564   01 27 51

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

01 33 00  OJ287        07 12 40  64.5 108.4 -1.7     -60.3     4      564   01 33 00
01 38 00  ---          07 17 41  65.5 109.8 -1.6     -59.5   300      584   01 33 01

01 38 10  OJ287        07 17 51  65.6 109.9 -1.6     -59.5     4      584   01 38 10
01 43 10  ---          07 22 52  66.6 111.4 -1.5     -58.5   300      603   01 38 11

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

01 43 20  OJ287        07 23 02  66.6 111.4 -1.5     -58.5     4      603   01 43 20
01 48 20  ---          07 28 03  67.6 113.0 -1.5     -57.4   300      622   01 43 21

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

01 48 30  OJ287        07 28 13  67.6 113.1 -1.5     -57.4     4      622   01 48 30
01 54 30  ---          07 34 14  68.8 115.2 -1.4     -56.0   360      645   01 48 31

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

01 54 40  OJ287        07 34 24  68.8 115.2 -1.4     -55.9     4      645   01 54 40
01 58 40  ---          07 38 25  69.6 116.8 -1.3     -54.9   240      661   01 54 41

01 58 50  OJ287        07 38 35  69.6 116.8 -1.3     -54.8     4      661   01 58 50
02 06 50  ---          07 46 36  71.2 120.2 -1.2     -52.4   480      692   01 58 51

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

02 07 00  OJ287        07 46 46  71.2 120.2 -1.1     -52.3     4      692   02 07 00
02 18 40  ---          07 58 28  73.3 126.0 -1.0     -47.8   700      737   02 07 01

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

02 18 50  OJ287        07 58 38  73.3 126.1 -1.0     -47.7     4      737   02 18 50
02 30 10  ---          08 10 00  75.2 133.1 -0.8     -42.0   680      781   02 18 51
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  31 Mar 2016   Day  91 ---

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

02 30 20  OJ287        08 10 10  75.2 133.2 -0.8     -41.9     4      781   02 30 20
02 39 40  ---          08 19 31  76.6 140.3 -0.6     -35.8   560      817   02 30 21

02 39 50  OJ287        08 19 41  76.7 140.4 -0.6     -35.7     4      817   02 39 50
02 49 10  ---          08 29 03  77.8 148.8 -0.4     -28.3   560      853   02 39 51

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

02 49 20  OJ287        08 29 13  77.8 149.0 -0.4     -28.1     4      853   02 49 20
03 00 00  ---          08 39 55  78.8 160.4 -0.3     -17.8   640      894   02 49 21

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

03 00 10  OJ287        08 40 05  78.8 160.6 -0.3     -17.7     4      894   03 00 10
03 10 50  ---          08 50 46  79.3 173.7 -0.1      -5.8   640      935   03 00 11

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

03 11 00  OJ287        08 50 56  79.4 173.9 -0.1      -5.6     4      935   03 11 00
03 19 00  ---          08 58 58  79.4 184.1  0.1       3.8   480      966   03 11 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

03 19 10  OJ287        08 59 08  79.4 184.3  0.1       3.9     4      966   03 19 10
03 27 10  ---          09 07 09  79.1 194.3  0.2      13.1   480      997   03 19 11

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

03 40 30  1641+399     09 20 31   5.3  46.2 -7.4     -53.9   643      997   03 40 30
03 50 00  ---          09 30 03   6.8  47.3 -7.2     -55.3   570     1034   03 40 31

03 50 30  1641+399     09 30 33   6.8  47.3 -7.2     -55.4    24     1034   03 50 30
04 00 00  ---          09 40 04   8.4  48.3 -7.1     -56.8   570     1070   03 50 31

04 00 30  1641+399     09 40 35   8.4  48.4 -7.0     -56.8    24     1070   04 00 30
04 10 00  ---          09 50 06  10.0  49.4 -6.9     -58.2   570     1107   04 00 31

04 10 30  1641+399     09 50 36  10.1  49.4 -6.9     -58.3    24     1107   04 10 30
04 20 00  ---          10 00 08  11.6  50.4 -6.7     -59.6   570     1144   04 10 31

04 20 30  1641+399     10 00 38  11.7  50.5 -6.7     -59.7    24     1144   04 20 30
04 30 00  ---          10 10 09  13.3  51.4 -6.6     -61.0   570     1181   04 20 31
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  31 Mar 2016   Day  91 ---

04 30 30  1641+399     10 10 40  13.4  51.4 -6.5     -61.1    24     1181   04 30 30
04 40 00  ---          10 20 11  15.0  52.3 -6.4     -62.4   570     1217   04 30 31

04 40 30  1641+399     10 20 41  15.1  52.4 -6.4     -62.5    24     1217   04 40 30
04 50 00  ---          10 30 13  16.7  53.2 -6.2     -63.7   570     1254   04 40 31

04 50 30  1641+399     10 30 43  16.8  53.3 -6.2     -63.8    24     1254   04 50 30
05 00 00  ---          10 40 14  18.5  54.1 -6.1     -65.1   570     1291   04 50 31

05 00 30  1641+399     10 40 44  18.5  54.1 -6.0     -65.2    24     1291   05 00 30
05 10 00  ---          10 50 16  20.2  54.9 -5.9     -66.4   570     1327   05 00 31

05 10 30  1641+399     10 50 46  20.3  55.0 -5.9     -66.5    24     1327   05 10 30
05 17 10  ---          10 57 27  21.5  55.5 -5.8     -67.4   400     1353   05 10 31

05 17 40  1641+399     10 57 57  21.6  55.6 -5.8     -67.4    24     1353   05 17 40
05 24 20  ---          11 04 38  22.8  56.1 -5.6     -68.3   400     1379   05 17 41

 ---------- L-band VLBI scans. Space segment 04 ----------

05 25 00  1641+399     11 05 18  22.9  56.1 -5.6     -68.4    34     1379   05 25 00
05 41 20  ---          11 21 41  25.8  57.3 -5.4     -70.5   980     1442   05 25 01

05 41 50  1641+399     11 22 11  25.9  57.4 -5.4     -70.6    24     1442   05 41 50
05 58 10  ---          11 38 34  28.9  58.5 -5.1     -72.7   980     1505   05 41 51

05 58 40  1641+399     11 39 04  29.0  58.5 -5.1     -72.7    24     1505   05 58 40
06 15 00  ---          11 55 27  32.0  59.6 -4.8     -74.8   980     1568   05 58 41

 ---------- Ground-only segment 05 ----------

06 15 30  1641+399     11 55 57  32.1  59.6 -4.8     -74.9    24     1568   06 15 30
06 24 30  ---          12 04 58  33.8  60.1 -4.6     -76.1   540     1603   06 15 31

06 25 00  1641+399     12 05 28  33.9  60.1 -4.6     -76.1    24     1603   06 25 00
06 30 00  ---          12 10 29  34.8  60.4 -4.6     -76.8   300     1622   06 25 01

06 30 30  1641+399     12 10 59  34.9  60.4 -4.5     -76.8    24     1622   06 30 30
06 40 00  ---          12 20 31  36.7  60.9 -4.4     -78.1   570     1659   06 30 31

06 40 30  1641+399     12 21 01  36.8  60.9 -4.4     -78.1    24     1659   06 40 30
06 50 00  ---          12 30 32  38.6  61.4 -4.2     -79.4   570     1696   06 40 31

06 50 30  1641+399     12 31 03  38.7  61.4 -4.2     -79.5    24     1696   06 50 30
07 00 00  ---          12 40 34  40.5  61.8 -4.0     -80.7   570     1733   06 50 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  31 Mar 2016   Day  91 ---

07 00 30  1641+399     12 41 04  40.6  61.8 -4.0     -80.8    24     1733   07 00 30
07 10 00  ---          12 50 36  42.4  62.2 -3.9     -82.1   570     1769   07 00 31

07 10 30  1641+399     12 51 06  42.5  62.2 -3.9     -82.1    24     1769   07 10 30
07 20 00  ---          13 00 37  44.3  62.5 -3.7     -83.5   570     1806   07 10 31

07 20 30  1641+399     13 01 07  44.4  62.6 -3.7     -83.5    24     1806   07 20 30
07 30 00  ---          13 10 39  46.2  62.8 -3.5     -84.9   570     1843   07 20 31

07 30 30  1641+399     13 11 09  46.3  62.8 -3.5     -84.9    24     1843   07 30 30
07 40 00  ---          13 20 41  48.1  63.0 -3.4     -86.3   570     1879   07 30 31

07 40 30  1641+399     13 21 11  48.2  63.0 -3.4     -86.4    24     1879   07 40 30
07 50 00  ---          13 30 42  50.1  63.2 -3.2     -87.8   570     1916   07 40 31

07 50 30  1641+399     13 31 12  50.2  63.2 -3.2     -87.9    24     1916   07 50 30
07 59 30  ---          13 40 14  51.9  63.3 -3.1     -89.3   540     1951   07 50 31

 ---------- L-band VLBI scans. Space segment 05 ----------

08 00 00  1641+399     13 40 44  52.0  63.3 -3.0     -89.3    24     1951   08 00 00
08 16 20  ---          13 57 07  55.1  63.2 -2.8     -92.0   980     2014   08 00 01

08 16 50  1641+399     13 57 37  55.2  63.2 -2.8     -92.1    24     2014   08 16 50
08 33 10  ---          14 13 59  58.4  62.8 -2.5     -95.0   980     2077   08 16 51

08 33 40  1641+399     14 14 29  58.5  62.8 -2.5     -95.1    24     2077   08 33 40
08 50 00  ---          14 30 52  61.6  62.1 -2.2     -98.4   980     2140   08 33 41

 ---------- Ground-only segment 06 ----------

08 50 30  1641+399     14 31 22  61.7  62.1 -2.2     -98.5    24     2140   08 50 30
09 00 00  ---          14 40 54  63.5  61.4 -2.0    -100.6   570     2177   08 50 31

 ---------- VLBA-only L,C,X,U ----------

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

09 00 10  1641+399     14 41 04  63.5  61.4 -2.0    -100.6     4     2177   09 00 10
09 05 10  ---          14 46 05  64.5  61.0 -2.0    -101.8   300     2196   09 00 11
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  31 Mar 2016   Day  91 ---

 ---------- back to the program source ----------

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

09 07 20  3C286        14 48 15  73.6 -85.8  1.3      84.4    18     2196   09 07 20
09 12 20  ---          14 53 16  72.5 -85.5  1.4      84.1   300     2216   09 07 21

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

09 14 30  1641+399     14 55 26  66.2  60.0 -1.8    -104.2    19     2216   09 14 30
09 20 30  ---          15 01 27  67.3  59.2 -1.7    -105.8   360     2239   09 14 31

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

09 20 40  1641+399     15 01 37  67.4  59.2 -1.7    -105.9     4     2239   09 20 40
09 24 40  ---          15 05 38  68.1  58.6 -1.6    -107.1   240     2254   09 20 41

09 24 50  1641+399     15 05 48  68.1  58.6 -1.6    -107.1     4     2254   09 24 50
09 28 50  ---          15 09 49  68.9  58.0 -1.6    -108.4   240     2270   09 24 51

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

09 29 00  1641+399     15 09 59  68.9  57.9 -1.6    -108.4     4     2270   09 29 00
09 35 00  ---          15 16 00  70.0  56.8 -1.5    -110.4   360     2293   09 29 01

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

09 35 10  1641+399     15 16 10  70.0  56.8 -1.5    -110.4     4     2293   09 35 10
09 40 10  ---          15 21 10  70.9  55.8 -1.4    -112.2   300     2312   09 35 11

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

09 40 20  1641+399     15 21 20  70.9  55.7 -1.4    -112.3     4     2312   09 40 20
09 45 20  ---          15 26 21  71.8  54.5 -1.3    -114.2   300     2332   09 40 21

09 45 30  1641+399     15 26 31  71.9  54.5 -1.3    -114.3     4     2332   09 45 30
09 50 30  ---          15 31 32  72.7  53.1 -1.2    -116.4   300     2351   09 45 31
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  31 Mar 2016   Day  91 ---

 ---------- back to the program source ----------

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

09 52 40  3C286        15 33 42  63.9 -82.6  2.0      81.7    26     2351   09 52 40
09 57 40  ---          15 38 43  62.8 -82.2  2.1      81.4   300     2370   09 52 41

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

09 59 50  1641+399     15 40 54  74.3  50.1 -1.0    -120.8    28     2370   09 59 50
10 05 50  ---          15 46 55  75.3  47.7 -0.9    -124.0   360     2393   09 59 51

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

10 06 00  1641+399     15 47 05  75.3  47.7 -0.9    -124.1     4     2393   10 06 00
10 10 00  ---          15 51 05  75.9  45.9 -0.9    -126.5   240     2409   10 06 01

10 10 10  1641+399     15 51 15  76.0  45.8 -0.9    -126.6     4     2409   10 10 10
10 14 10  ---          15 55 16  76.6  43.8 -0.8    -129.2   240     2424   10 10 11

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

10 14 20  1641+399     15 55 26  76.6  43.7 -0.8    -129.3     4     2424   10 14 20
10 20 20  ---          16 01 27  77.5  40.3 -0.7    -133.6   360     2448   10 14 21

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

10 20 30  1641+399     16 01 37  77.5  40.2 -0.7    -133.7     4     2448   10 20 30
10 25 30  ---          16 06 38  78.2  36.9 -0.6    -137.7   300     2467   10 20 31

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

10 25 40  1641+399     16 06 48  78.2  36.8 -0.6    -137.9     4     2467   10 25 40
10 30 40  ---          16 11 49  78.8  33.1 -0.5    -142.3   300     2486   10 25 41

10 30 50  1641+399     16 11 59  78.8  33.0 -0.5    -142.5     4     2486   10 30 50
10 35 50  ---          16 17 00  79.4  28.8 -0.4    -147.4   300     2506   10 30 51
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  31 Mar 2016   Day  91 ---

 ----------  Pol. calibrator at L ----------

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

10 38 00  3C286        16 19 10  54.2 -79.3  2.8      78.7    45     2506   10 38 00
10 43 00  ---          16 24 11  53.1 -79.0  2.9      78.4   300     2525   10 38 01

 ---------- back to the program source ----------

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

10 45 10  1641+399     16 26 21  80.2  19.8 -0.3    -157.7    51     2525   10 45 10
10 51 10  ---          16 32 22  80.6  13.2 -0.2    -165.2   360     2548   10 45 11

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

10 51 20  1641+399     16 32 32  80.6  13.0 -0.2    -165.4     4     2548   10 51 20
10 55 20  ---          16 36 33  80.7   8.4 -0.1    -170.6   240     2564   10 51 21

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

10 55 30  1641+399     16 36 43  80.8   8.2 -0.1    -170.8     4     2564   10 55 30
11 00 00  ---          16 41 13  80.8   2.8 -0.0    -176.9   270     2581   10 55 31


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra4cm2.set
   Matching groups in ./gg079a_freq.dat:
     v4cm_3

   Setup group:   43         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.1     15.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  15  Setup file default.  Used with PCAL = 1MHz
   LO sum=   8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
   BBC fr=    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     792.99    856.99    825.01    825.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  15  16  17  18  19  20  21  22  23  24

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra18cm2.set
   Matching groups in ./gg079a_freq.dat:
     v20cm_2         FD filtered above 1760.  SC filtered above 1740.

   Setup group:    8         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         L         L         L         L         L         L         L         L
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         L         L         U         U         L         L
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  14.6      2.4     14.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  25  Setup file default.  Used with PCAL = 1MHz
   LO sum=   1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
   BBC fr=    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     764.01    764.01    731.99    731.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  25  26  27  28  29  30  31  32  33  34

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra2cm2.set
   Matching groups in ./gg079a_freq.dat:
     v2cm_d3         Fourth 2cm filter

   Setup group:   53         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.6     10.9     10.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  35  Setup file default.  Used with PCAL = 1MHz
   LO sum=   15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
   BBC fr=     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00
   Bandwd=      16.00     16.00     16.00     16.00     16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     736.99    800.99    769.01    769.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  35  36  37  38  39  40  41  42  43  44

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra6cm2.set
   Matching groups in ./gg079a_freq.dat:
     vc_d

   Setup group:   33         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  13.6      4.1     13.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  45  Setup file default.  Used with PCAL = 1MHz
   LO sum=   4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
   BBC fr=    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     703.99    767.99    736.01    736.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  45  46  47  48  49  50  51  52  53  54

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 56.741257       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 38.38204        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

   1328+307          13 28 49.657778   * 13 31 08.288070     13 31 54.206774       0.00
   J1331+3030        30 45 58.64060    * 30 30 32.95924      30 25 28.58949        0.00
 * 3C286             ./gg079a_sources.radioastron
                     WSRT calibrator, not for 92cm, rfc_2013d Petrov, 2013, unpublished 542 observati

   0316+413          03 16 29.567283   * 03 19 48.160114     03 20 51.642341       0.00
   J0319+4130        41 19 51.91847    * 41 30 42.10559      41 34 05.47448        0.00
 * 3C84              ./gg079a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 15448 observations, RA-AO3-04, RA-AO2-1

   0851+202          08 51 57.250618   * 08 54 48.874930     08 55 44.920816       0.00
   J0854+2006        20 17 58.41733    * 20 06 30.64078      20 02 37.68080        0.00
 * OJ287             ./gg079a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 213710 observations, RA-AO3-04, RA-AO3-

 * 1641+399          16 41 17.606226   * 16 42 58.809963     16 43 32.203998       0.00
   J1642+3948        39 54 10.81479    * 39 48 36.99385      39 46 41.97815        0.00
   3C345             ./gg079a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 51938 observations, RA-AO3-04, RA-AO3-0



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra18cm2.set           12                                4.083     0.000
  3C286      ra18cm2.set           1 2 3 4 5 6 7 8 11 13 14 25       0.883    55.135
  3C84       ra18cm2.set           25                                0.083     3.750
             ra6cm2.set            45                                0.067     3.000
             ra4cm2.set            15                                0.083     3.750
             ra2cm2.set            35                                0.100     4.500
  OJ287      ra18cm2.set           25                                1.000    29.800
             ra6cm2.set            45                                0.767    21.933
             ra4cm2.set            15                                0.944    28.967
             ra2cm2.set            35                                1.256    34.817
  1641+399   ra18cm2.set           1 2 3 4 5 6 7 8 11 13 14 25 +    10.694  1261.236
             ra6cm2.set            45                                0.333    15.000
             ra4cm2.set            15                                0.417    18.750
             ra2cm2.set            35                                0.500    22.475


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA              90.7
   3C286              143.1
   3C84                51.7
   OJ287              119.8
   1641+399           109.0

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

