  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: BNS merger counterpart
 Exp. Code:  gg084b  


Schedule Version:       2.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Giancarlo Ghirlanda

Address:  JIVE
          Oude Hoogeveensedijk 4
          Dwingeloo
          Netherlands

Phone:    +31 521 596 536
EMAIL:    zparagi@jive.eu
Fax:      +31 521 596 539
Phone during observation: +31 521 596 530

Observing mode:

Notes:    Second epoch global observations
 
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  26 May 2018   Day 146 ---

 Next scan frequencies:  4740.00  4740.00  4804.00  4804.00  4868.00  4868.00  4932.00  4932.00
 Next BBC frequencies:    640.00   640.00   704.00   704.00   768.00   768.00   832.00   832.00
 Next scan bandwidths:     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00

23 48 30  EM170817     09 10 42  11.0 126.0 -4.0     -49.4     0        0   23 48 30
23 51 00  ---          09 13 13  11.5 126.3 -4.0     -49.1   150       39   23 48 31

23 51 00  J1311-2329   09 13 13  11.1 126.2 -4.0     -49.3    -8       39   23 51 08
23 52 30  ---          09 14 43  11.3 126.4 -4.0     -49.1    82       60   23 51 01

23 52 30  EM170817     09 14 43  11.7 126.6 -3.9     -48.9    -9       60   23 52 39
23 55 00  ---          09 17 13  12.2 127.0 -3.9     -48.6   141       96   23 52 31

23 55 30  J1311-2329   09 17 43  11.9 126.8 -3.9     -48.7    22       96   23 55 30
23 56 30  ---          09 18 44  12.0 127.0 -3.9     -48.6    60      112   23 55 31

23 56 30  EM170817     09 18 44  12.4 127.2 -3.9     -48.4    -9      112   23 56 39
23 59 00  ---          09 21 14  12.8 127.6 -3.8     -48.0   141      148   23 56 31

 --- Start: Sat  26 May 2018   Day 146 -- Stop: Sun  27 May 2018   Day 147 ---

23 59 00  J1311-2329   09 21 14  12.5 127.4 -3.9     -48.2    -8      148   23 59 08
00 00 30  ---          09 22 44  12.7 127.6 -3.8     -48.0    82      169   23 59 01

00 00 30  J1312-2350   09 22 44  12.3 127.7 -3.9     -48.1    -9      169   00 00 39
00 03 00  ---          09 25 15  12.7 128.1 -3.8     -47.8   141      205   00 00 31

00 03 40  J1311-2329   09 25 55  13.2 128.1 -3.8     -47.6    31      205   00 03 40
00 04 40  ---          09 26 55  13.4 128.3 -3.8     -47.5    60      221   00 03 41

00 04 40  EM170817     09 26 55  13.8 128.5 -3.7     -47.2    -9      221   00 04 49
00 07 10  ---          09 29 25  14.2 128.9 -3.7     -46.9   141      257   00 04 41

00 07 10  J1311-2329   09 29 25  13.8 128.7 -3.7     -47.1    -8      257   00 07 18
00 08 40  ---          09 30 56  14.1 128.9 -3.7     -46.9    82      278   00 07 11

00 08 40  EM170817     09 30 56  14.5 129.1 -3.7     -46.7    -9      278   00 08 49
00 11 10  ---          09 33 26  14.9 129.5 -3.6     -46.3   141      315   00 08 41

00 11 40  J1311-2329   09 33 56  14.6 129.4 -3.6     -46.5    22      315   00 11 40
00 12 40  ---          09 34 56  14.8 129.6 -3.6     -46.4    60      330   00 11 41

00 12 40  EM170817     09 34 56  15.1 129.8 -3.6     -46.1    -8      330   00 12 48
00 15 10  ---          09 37 27  15.6 130.2 -3.6     -45.8   142      367   00 12 41
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

00 15 10  J1311-2329   09 37 27  15.2 130.0 -3.6     -46.0    -8      367   00 15 18
00 16 40  ---          09 38 57  15.4 130.2 -3.6     -45.8    82      388   00 15 11

00 16 40  J1312-2350   09 38 57  15.0 130.3 -3.6     -45.9    -9      388   00 16 49
00 19 10  ---          09 41 27  15.4 130.7 -3.5     -45.5   141      424   00 16 41

00 19 10  J1311-2329   09 41 27  15.8 130.7 -3.5     -45.4    -9      424   00 19 19
00 20 40  ---          09 42 58  16.1 130.9 -3.5     -45.2    81      445   00 19 11

00 20 40  J1303-2405   09 42 58  17.0 132.7 -3.4     -43.8   -10      445   00 20 50
00 23 10  ---          09 45 28  17.4 133.2 -3.3     -43.5   140      481   00 20 41

00 23 50  J1311-2329   09 46 08  16.6 131.4 -3.4     -44.7    30      481   00 23 50
00 24 50  ---          09 47 08  16.8 131.6 -3.4     -44.6    60      496   00 23 51

00 25 00  J1337-1257   09 47 18  19.3 119.1 -3.9     -50.5    -7      496   00 25 07
00 28 00  =1334-127    09 50 19  19.9 119.6 -3.8     -50.2   173      541   00 25 01

00 28 30  J1259-2310   09 50 49  19.5 134.2 -3.2     -42.2    12      541   00 28 30
00 29 30  =1256-229    09 51 49  19.7 134.4 -3.1     -42.0    60      556   00 28 31

00 29 30  J1311-2329   09 51 49  17.5 132.4 -3.3     -43.9   -12      556   00 29 42
00 31 00  ---          09 53 19  17.7 132.7 -3.3     -43.7    78      577   00 29 31

00 31 00  EM170817     09 53 19  18.1 132.9 -3.3     -43.4    -8      577   00 31 08
00 33 30  ---          09 55 50  18.5 133.4 -3.2     -43.0   142      613   00 31 01

00 33 30  J1311-2329   09 55 50  18.1 133.1 -3.3     -43.3    -8      613   00 33 38
00 35 00  ---          09 57 20  18.4 133.4 -3.3     -43.0    82      634   00 33 31

00 35 00  EM170817     09 57 20  18.7 133.6 -3.2     -42.8    -8      634   00 35 08
00 37 30  ---          09 59 50  19.1 134.1 -3.2     -42.4   142      671   00 35 01

00 38 00  J1259-2310   10 00 20  21.0 136.0 -3.0     -40.6    18      671   00 38 00
00 39 00  =1256-229    10 01 21  21.1 136.2 -3.0     -40.5    60      686   00 38 01

00 39 00  J1311-2329   10 01 21  19.0 134.1 -3.2     -42.4   -12      686   00 39 12
00 40 30  ---          10 02 51  19.2 134.4 -3.2     -42.2    78      706   00 39 01

00 40 30  EM170817     10 02 51  19.6 134.6 -3.1     -41.9    -8      706   00 40 38
00 43 00  ---          10 05 21  20.0 135.1 -3.1     -41.5   142      743   00 40 31

00 43 00  J1311-2329   10 05 21  19.6 134.8 -3.1     -41.8    -8      743   00 43 08
00 44 30  ---          10 06 51  19.8 135.1 -3.1     -41.5    82      764   00 43 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

00 44 30  EM170817     10 06 51  20.2 135.3 -3.1     -41.3    -8      764   00 44 38
00 47 00  ---          10 09 22  20.6 135.8 -3.0     -40.8   142      801   00 44 31

00 47 30  J1259-2310   10 09 52  22.4 137.8 -2.8     -39.0    19      801   00 47 30
00 48 30  =1256-229    10 10 52  22.5 138.0 -2.8     -38.8    60      816   00 47 31

00 48 30  J1311-2329   10 10 52  20.4 135.8 -3.0     -40.9   -12      816   00 48 42
00 50 00  ---          10 12 22  20.7 136.1 -3.0     -40.6    78      836   00 48 31

00 50 00  EM170817     10 12 22  21.0 136.4 -3.0     -40.3    -8      836   00 50 08
00 52 30  ---          10 14 53  21.4 136.8 -2.9     -39.9   142      873   00 50 01

00 52 30  J1311-2329   10 14 53  21.0 136.6 -3.0     -40.2    -8      873   00 52 38
00 54 00  ---          10 16 23  21.3 136.9 -2.9     -39.9    82      894   00 52 31

00 54 00  EM170817     10 16 23  21.6 137.1 -2.9     -39.7    -8      894   00 54 08
00 56 30  ---          10 18 53  22.0 137.6 -2.9     -39.2   142      931   00 54 01

00 57 00  J1259-2310   10 19 24  23.7 139.6 -2.7     -37.3    19      931   00 57 00
00 58 00  =1256-229    10 20 24  23.9 139.8 -2.7     -37.2    60      946   00 57 01

00 58 00  J1311-2329   10 20 24  21.8 137.6 -2.9     -39.3   -12      946   00 58 12
00 59 30  ---          10 21 54  22.1 137.9 -2.8     -39.0    78      966   00 58 01

00 59 30  EM170817     10 21 54  22.4 138.2 -2.8     -38.7    -8      966   00 59 38
01 02 00  ---          10 24 24  22.8 138.7 -2.8     -38.3   142     1003   00 59 31

01 02 00  J1311-2329   10 24 24  22.4 138.4 -2.8     -38.6    -8     1003   01 02 08
01 03 30  ---          10 25 55  22.6 138.7 -2.8     -38.3    82     1024   01 02 01

01 03 30  J1312-2350   10 25 55  22.2 138.7 -2.8     -38.4    -9     1024   01 03 39
01 04 30  ---          10 26 55  22.3 138.9 -2.8     -38.3    51     1037   01 03 31

01 05 00  J1259-2310   10 27 25  24.8 141.3 -2.5     -35.9    17     1037   01 05 00
01 06 00  =1256-229    10 28 25  25.0 141.5 -2.5     -35.7    60     1052   01 05 01

01 06 00  J1311-2329   10 28 25  23.0 139.2 -2.7     -37.9   -12     1052   01 06 12
01 07 30  ---          10 29 55  23.2 139.5 -2.7     -37.6    78     1073   01 06 01

01 07 30  EM170817     10 29 55  23.6 139.8 -2.7     -37.3    -8     1073   01 07 38
01 10 00  ---          10 32 26  23.9 140.3 -2.6     -36.9   142     1109   01 07 31

01 10 00  J1311-2329   10 32 26  23.6 140.0 -2.7     -37.2    -8     1109   01 10 08
01 11 30  ---          10 33 56  23.8 140.3 -2.6     -36.9    82     1130   01 10 01
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

01 11 30  EM170817     10 33 56  24.1 140.6 -2.6     -36.6    -8     1130   01 11 38
01 14 00  ---          10 36 26  24.4 141.1 -2.6     -36.1   142     1167   01 11 31

01 14 30  J1259-2310   10 36 56  26.1 143.3 -2.4     -34.1    19     1167   01 14 30
01 15 30  =1256-229    10 37 57  26.2 143.5 -2.4     -33.9    60     1182   01 14 31

01 15 30  J1311-2329   10 37 57  24.3 141.1 -2.6     -36.2   -12     1182   01 15 42
01 17 00  ---          10 39 27  24.5 141.4 -2.6     -35.9    78     1202   01 15 31

01 17 00  EM170817     10 39 27  24.8 141.7 -2.5     -35.6    -8     1202   01 17 08
01 19 30  ---          10 41 57  25.2 142.2 -2.5     -35.1   142     1239   01 17 01

01 19 30  J1311-2329   10 41 57  24.8 141.9 -2.5     -35.4    -8     1239   01 19 38
01 21 00  ---          10 43 27  25.0 142.2 -2.5     -35.1    82     1260   01 19 31

01 21 00  EM170817     10 43 27  25.4 142.5 -2.5     -34.8    -8     1260   01 21 08
01 23 30  ---          10 45 58  25.7 143.0 -2.4     -34.3   142     1297   01 21 01

01 24 00  J1259-2310   10 46 28  27.3 145.3 -2.2     -32.2    19     1297   01 24 00
01 25 00  =1256-229    10 47 28  27.4 145.5 -2.2     -32.0    60     1312   01 24 01

01 25 00  J1311-2329   10 47 28  25.6 143.0 -2.4     -34.4   -12     1312   01 25 12
01 26 30  ---          10 48 58  25.8 143.4 -2.4     -34.1    78     1332   01 25 01

01 26 30  EM170817     10 48 58  26.1 143.7 -2.4     -33.8    -8     1332   01 26 38
01 29 00  ---          10 51 29  26.4 144.2 -2.3     -33.3   142     1369   01 26 31

01 29 00  J1311-2329   10 51 29  26.1 143.9 -2.4     -33.6    -8     1369   01 29 08
01 30 30  ---          10 52 59  26.3 144.2 -2.3     -33.3    82     1390   01 29 01

01 30 30  EM170817     10 52 59  26.6 144.5 -2.3     -33.0    -8     1390   01 30 38
01 33 00  ---          10 55 29  26.9 145.1 -2.3     -32.5   142     1427   01 30 31

01 33 30  J1259-2310   10 56 00  28.4 147.4 -2.1     -30.3    19     1427   01 33 30
01 34 30  =1256-229    10 57 00  28.5 147.6 -2.1     -30.1    60     1442   01 33 31

01 34 30  J1311-2329   10 57 00  26.8 145.1 -2.3     -32.5   -11     1442   01 34 41
01 36 00  ---          10 58 30  27.0 145.4 -2.2     -32.2    79     1462   01 34 31

01 36 00  EM170817     10 58 30  27.3 145.7 -2.2     -31.9    -8     1462   01 36 08
01 38 30  ---          11 01 00  27.6 146.3 -2.2     -31.4   142     1499   01 36 01

01 38 30  J1311-2329   11 01 00  27.3 145.9 -2.2     -31.7    -8     1499   01 38 38
01 40 00  ---          11 02 31  27.4 146.3 -2.2     -31.4    82     1520   01 38 31
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

01 40 00  J1312-2350   11 02 31  27.0 146.2 -2.2     -31.6    -9     1520   01 40 09
01 41 00  ---          11 03 31  27.1 146.4 -2.2     -31.4    51     1533   01 40 01

01 41 30  J1259-2310   11 04 01  29.3 149.3 -1.9     -28.6    18     1533   01 41 30
01 42 30  =1256-229    11 05 01  29.4 149.5 -1.9     -28.4    60     1549   01 41 31

01 42 30  J1311-2329   11 05 01  27.7 146.8 -2.1     -30.9   -11     1549   01 42 41
01 44 00  ---          11 06 31  27.9 147.2 -2.1     -30.6    79     1569   01 42 31

01 44 00  EM170817     11 06 31  28.2 147.5 -2.1     -30.3    -8     1569   01 44 08
01 46 30  ---          11 09 02  28.5 148.1 -2.0     -29.7   142     1606   01 44 01

01 46 30  J1311-2329   11 09 02  28.2 147.7 -2.1     -30.1    -8     1606   01 46 38
01 48 00  ---          11 10 32  28.4 148.1 -2.0     -29.8    82     1627   01 46 31

01 48 00  EM170817     11 10 32  28.7 148.4 -2.0     -29.4    -8     1627   01 48 08
01 50 30  ---          11 13 02  29.0 149.0 -2.0     -28.9   142     1663   01 48 01

01 51 00  J1259-2310   11 13 32  30.3 151.5 -1.8     -26.6    19     1663   01 51 00
01 52 00  =1256-229    11 14 33  30.4 151.7 -1.8     -26.3    60     1679   01 51 01

01 52 00  J1311-2329   11 14 33  28.8 149.0 -2.0     -28.9   -11     1679   01 52 11
01 53 30  ---          11 16 03  29.0 149.3 -1.9     -28.6    79     1699   01 52 01

01 53 30  EM170817     11 16 03  29.3 149.7 -1.9     -28.3    -8     1699   01 53 38
01 56 00  ---          11 18 33  29.6 150.3 -1.9     -27.7   142     1736   01 53 31

01 56 00  J1311-2329   11 18 33  29.3 149.9 -1.9     -28.1    -8     1736   01 56 08
01 57 30  ---          11 20 03  29.4 150.2 -1.9     -27.8    82     1757   01 56 01

01 57 30  EM170817     11 20 03  29.7 150.6 -1.8     -27.4    -8     1757   01 57 38
02 00 00  ---          11 22 34  30.0 151.2 -1.8     -26.9   142     1793   01 57 31

02 00 30  J1259-2310   11 23 04  31.3 153.8 -1.6     -24.4    20     1793   02 00 30
02 01 30  =1256-229    11 24 04  31.4 154.0 -1.6     -24.2    60     1809   02 00 31

02 01 30  J1311-2329   11 24 04  29.8 151.2 -1.8     -26.9   -11     1809   02 01 41
02 03 00  ---          11 25 34  30.0 151.5 -1.8     -26.6    79     1829   02 01 31

02 03 00  EM170817     11 25 34  30.3 151.9 -1.8     -26.2    -8     1829   02 03 08
02 05 30  ---          11 28 05  30.5 152.5 -1.7     -25.7   142     1866   02 03 01

02 05 30  J1311-2329   11 28 05  30.3 152.1 -1.7     -26.0    -8     1866   02 05 38
02 07 00  ---          11 29 35  30.4 152.5 -1.7     -25.7    82     1887   02 05 31
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

02 07 00  EM170817     11 29 35  30.7 152.9 -1.7     -25.3    -8     1887   02 07 08
02 09 30  ---          11 32 05  30.9 153.5 -1.6     -24.8   142     1924   02 07 01

02 10 00  J1259-2310   11 32 35  32.1 156.1 -1.5     -22.3    20     1924   02 10 00
02 11 00  =1256-229    11 33 36  32.2 156.4 -1.4     -22.0    60     1939   02 10 01

02 11 00  J1311-2329   11 33 36  30.8 153.5 -1.7     -24.8   -11     1939   02 11 11
02 12 30  ---          11 35 06  30.9 153.8 -1.6     -24.5    79     1959   02 11 01

02 12 30  EM170817     11 35 06  31.2 154.2 -1.6     -24.1    -8     1959   02 12 38
02 15 00  ---          11 37 36  31.5 154.8 -1.6     -23.5   142     1996   02 12 31

02 15 00  J1311-2329   11 37 36  31.2 154.4 -1.6     -23.9    -8     1996   02 15 08
02 16 30  ---          11 39 07  31.3 154.8 -1.6     -23.6    82     2017   02 15 01

02 16 30  J1312-2350   11 39 07  30.9 154.7 -1.6     -23.7    -9     2017   02 16 39
02 17 30  ---          11 40 07  31.0 154.9 -1.6     -23.5    51     2030   02 16 31

02 18 00  J1259-2310   11 40 37  32.8 158.2 -1.3     -20.4    18     2030   02 18 00
02 19 00  =1256-229    11 41 37  32.9 158.4 -1.3     -20.1    60     2046   02 18 01

02 19 00  J1311-2329   11 41 37  31.5 155.4 -1.5     -23.0   -11     2046   02 19 11
02 20 30  ---          11 43 07  31.7 155.8 -1.5     -22.6    79     2066   02 19 01

02 20 30  EM170817     11 43 07  31.9 156.2 -1.5     -22.2    -8     2066   02 20 38
02 23 00  ---          11 45 38  32.2 156.8 -1.4     -21.7   142     2103   02 20 31

02 23 00  J1311-2329   11 45 38  31.9 156.4 -1.4     -22.1    -8     2103   02 23 08
02 24 30  ---          11 47 08  32.0 156.8 -1.4     -21.7    82     2124   02 23 01

02 24 30  EM170817     11 47 08  32.3 157.2 -1.4     -21.3    -8     2124   02 24 38
02 27 00  ---          11 49 38  32.5 157.8 -1.4     -20.7   142     2160   02 24 31

02 27 30  J1259-2310   11 50 08  33.5 160.6 -1.2     -18.1    20     2160   02 27 30
02 28 30  =1256-229    11 51 09  33.6 160.9 -1.1     -17.8    60     2176   02 27 31

02 28 30  J1311-2329   11 51 09  32.4 157.8 -1.4     -20.8   -10     2176   02 28 40
02 30 00  ---          11 52 39  32.5 158.2 -1.3     -20.4    80     2196   02 28 31

02 30 00  EM170817     11 52 39  32.7 158.6 -1.3     -20.0    -8     2196   02 30 08
02 32 30  ---          11 55 09  32.9 159.3 -1.3     -19.4   142     2233   02 30 01

02 32 30  J1311-2329   11 55 09  32.7 158.8 -1.3     -19.8    -8     2233   02 32 38
02 34 00  ---          11 56 39  32.8 159.2 -1.3     -19.5    82     2254   02 32 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

02 34 00  EM170817     11 56 39  33.0 159.6 -1.2     -19.0    -8     2254   02 34 08
02 36 30  ---          11 59 10  33.2 160.3 -1.2     -18.4   142     2291   02 34 01

02 37 00  J1259-2310   11 59 40  34.2 163.2 -1.0     -15.7    20     2291   02 37 00
02 38 00  =1256-229    12 00 40  34.2 163.4 -1.0     -15.5    60     2306   02 37 01

02 38 00  J1311-2329   12 00 40  33.1 160.3 -1.2     -18.5   -10     2306   02 38 10
02 39 30  ---          12 02 10  33.2 160.6 -1.2     -18.1    80     2327   02 38 01

02 39 30  EM170817     12 02 10  33.4 161.1 -1.1     -17.7    -8     2327   02 39 38
02 42 00  ---          12 04 41  33.6 161.7 -1.1     -17.1   142     2363   02 39 31

02 42 00  J1311-2329   12 04 41  33.4 161.3 -1.1     -17.5    -8     2363   02 42 08
02 43 30  ---          12 06 11  33.5 161.7 -1.1     -17.2    82     2384   02 42 01

02 43 30  EM170817     12 06 11  33.7 162.1 -1.1     -16.7    -8     2384   02 43 38
02 46 00  ---          12 08 41  33.9 162.8 -1.0     -16.1   142     2421   02 43 31

02 46 30  J1259-2310   12 09 11  34.7 165.7 -0.8     -13.3    20     2421   02 46 30
02 47 30  =1256-229    12 10 12  34.8 166.0 -0.8     -13.1    60     2436   02 46 31

02 47 30  J1311-2329   12 10 12  33.7 162.8 -1.0     -16.2   -10     2436   02 47 40
02 49 00  ---          12 11 42  33.8 163.2 -1.0     -15.8    80     2457   02 47 31

02 49 00  EM170817     12 11 42  34.1 163.6 -1.0     -15.4    -8     2457   02 49 08
02 51 30  ---          12 14 12  34.2 164.3 -0.9     -14.7   142     2494   02 49 01

02 51 30  J1311-2329   12 14 12  34.0 163.8 -1.0     -15.2    -8     2494   02 51 38
02 53 00  ---          12 15 43  34.1 164.2 -0.9     -14.8    82     2515   02 51 31

02 53 00  J1312-2350   12 15 43  33.7 164.0 -1.0     -15.0    -9     2515   02 53 09
02 54 00  ---          12 16 43  33.7 164.3 -1.0     -14.8    51     2528   02 53 01

02 54 30  J1259-2310   12 17 13  35.1 167.9 -0.7     -11.3    19     2528   02 54 30
02 55 30  =1256-229    12 18 13  35.2 168.2 -0.7     -11.0    60     2543   02 54 31

02 55 30  J1311-2329   12 18 13  34.2 164.9 -0.9     -14.2   -10     2543   02 55 40
02 57 00  ---          12 19 43  34.3 165.3 -0.9     -13.8    80     2564   02 55 31

02 57 00  EM170817     12 19 43  34.5 165.8 -0.9     -13.3    -8     2564   02 57 08
02 59 30  ---          12 22 14  34.6 166.4 -0.8     -12.7   142     2601   02 57 01

02 59 30  J1311-2329   12 22 14  34.4 166.0 -0.8     -13.2    -8     2601   02 59 38
03 01 00  ---          12 23 44  34.5 166.4 -0.8     -12.8    82     2622   02 59 31
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

03 01 00  EM170817     12 23 44  34.7 166.8 -0.8     -12.3    -8     2622   03 01 08
03 03 30  ---          12 26 14  34.8 167.5 -0.7     -11.7   142     2658   03 01 01

03 04 00  J1259-2310   12 26 44  35.5 170.6 -0.6      -8.8    20     2658   03 04 00
03 05 00  =1256-229    12 27 45  35.5 170.9 -0.5      -8.6    60     2674   03 04 01

03 05 00  J1311-2329   12 27 45  34.7 167.5 -0.7     -11.8   -10     2674   03 05 10
03 06 30  ---          12 29 15  34.8 167.9 -0.7     -11.4    80     2694   03 05 01

03 06 30  EM170817     12 29 15  35.0 168.4 -0.7     -10.9    -8     2694   03 06 38
03 09 00  ---          12 31 45  35.1 169.0 -0.7     -10.3   142     2731   03 06 31

03 09 00  J1311-2329   12 31 45  34.9 168.6 -0.7     -10.7    -8     2731   03 09 08
03 10 30  ---          12 33 15  35.0 169.0 -0.7     -10.3    82     2752   03 09 01

03 10 30  EM170817     12 33 15  35.1 169.5 -0.6      -9.9    -8     2752   03 10 38
03 13 00  ---          12 35 46  35.2 170.2 -0.6      -9.2   142     2789   03 10 31

03 13 30  J1259-2310   12 36 16  35.8 173.2 -0.4      -6.3    20     2789   03 13 30
03 14 30  =1256-229    12 37 16  35.8 173.5 -0.4      -6.1    60     2804   03 13 31

03 14 30  J1311-2329   12 37 16  35.1 170.1 -0.6      -9.3   -10     2804   03 14 40
03 16 00  ---          12 38 46  35.2 170.5 -0.6      -8.9    80     2825   03 14 31

03 16 00  EM170817     12 38 46  35.3 171.0 -0.5      -8.4    -8     2825   03 16 08
03 18 30  ---          12 41 17  35.4 171.7 -0.5      -7.8   142     2861   03 16 01

03 18 30  J1311-2329   12 41 17  35.2 171.2 -0.5      -8.3    -8     2861   03 18 38
03 20 00  ---          12 42 47  35.3 171.6 -0.5      -7.9    82     2882   03 18 31

03 20 00  EM170817     12 42 47  35.5 172.1 -0.5      -7.4    -8     2882   03 20 08
03 22 30  ---          12 45 17  35.5 172.8 -0.4      -6.7   142     2919   03 20 01

03 23 00  J1259-2310   12 45 47  36.0 175.9 -0.2      -3.8    20     2919   03 23 00
03 24 00  =1256-229    12 46 48  36.0 176.2 -0.2      -3.5    60     2935   03 23 01

03 24 00  J1311-2329   12 46 48  35.4 172.7 -0.4      -6.8   -10     2935   03 24 10
03 25 30  ---          12 48 18  35.5 173.2 -0.4      -6.4    80     2955   03 24 01

03 25 30  EM170817     12 48 18  35.6 173.6 -0.4      -6.0    -8     2955   03 25 38
03 28 00  ---          12 50 48  35.7 174.4 -0.3      -5.3   142     2992   03 25 31

03 28 00  J1311-2329   12 50 48  35.5 173.9 -0.4      -5.8    -8     2992   03 28 08
03 29 30  ---          12 52 19  35.5 174.3 -0.3      -5.4    82     3013   03 28 01
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

03 29 30  J1312-2350   12 52 19  35.2 174.0 -0.4      -5.7    -8     3013   03 29 38
03 30 30  ---          12 53 19  35.2 174.3 -0.3      -5.4    52     3026   03 29 31

03 31 00  J1259-2310   12 53 49  36.1 178.2 -0.1      -1.7    19     3026   03 31 00
03 32 00  =1256-229    12 54 49  36.1 178.5 -0.1      -1.4    60     3042   03 31 01

03 32 00  J1311-2329   12 54 49  35.6 175.0 -0.3      -4.7   -10     3042   03 32 10
03 33 30  ---          12 56 19  35.6 175.4 -0.3      -4.3    80     3062   03 32 01

03 33 30  EM170817     12 56 19  35.8 175.9 -0.2      -3.8    -8     3062   03 33 38
03 36 00  ---          12 58 50  35.8 176.6 -0.2      -3.2   142     3099   03 33 31

03 36 00  J1311-2329   12 58 50  35.7 176.1 -0.2      -3.7    -8     3099   03 36 08
03 37 30  ---          13 00 20  35.7 176.5 -0.2      -3.3    82     3120   03 36 01

03 37 30  EM170817     13 00 20  35.8 177.0 -0.2      -2.8    -8     3120   03 37 38
03 40 00  ---          13 02 50  35.9 177.7 -0.1      -2.1   142     3157   03 37 31

03 40 30  J1259-2310   13 03 20  36.1 180.9  0.1       0.9    20     3157   03 40 30
03 41 30  =1256-229    13 04 21  36.1 181.2  0.1       1.1    60     3172   03 40 31

03 41 30  J1311-2329   13 04 21  35.7 177.7 -0.1      -2.2   -10     3172   03 41 40
03 43 00  ---          13 05 51  35.7 178.1 -0.1      -1.8    80     3193   03 41 31

03 43 00  EM170817     13 05 51  35.9 178.6 -0.1      -1.3    -8     3193   03 43 08
03 45 30  ---          13 08 21  35.9 179.3 -0.0      -0.6   142     3229   03 43 01

03 45 30  J1311-2329   13 08 21  35.8 178.8 -0.1      -1.1    -8     3229   03 45 38
03 47 00  ---          13 09 51  35.8 179.2 -0.0      -0.7    82     3250   03 45 31

03 47 00  EM170817     13 09 51  35.9 179.7 -0.0      -0.3    -8     3250   03 47 08
03 49 30  ---          13 12 22  35.9 180.4  0.0       0.4   142     3287   03 47 01

03 50 00  J1259-2310   13 12 52  36.0 183.6  0.2       3.4    20     3287   03 50 00
03 51 00  =1256-229    13 13 52  36.0 183.9  0.2       3.7    60     3302   03 50 01

03 51 00  J1311-2329   13 13 52  35.8 180.4  0.0       0.3   -10     3302   03 51 10
03 52 30  ---          13 15 22  35.8 180.8  0.0       0.7    80     3323   03 51 01

03 52 30  EM170817     13 15 22  35.9 181.3  0.1       1.2    -8     3323   03 52 38
03 55 00  ---          13 17 53  35.9 182.0  0.1       1.9   142     3360   03 52 31

03 55 00  J1311-2329   13 17 53  35.8 181.5  0.1       1.4    -8     3360   03 55 08
03 56 30  ---          13 19 23  35.7 181.9  0.1       1.8    82     3381   03 55 01
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

03 56 30  EM170817     13 19 23  35.8 182.4  0.1       2.3    -8     3381   03 56 38
03 59 00  ---          13 21 53  35.8 183.1  0.2       2.9   142     3417   03 56 31

03 59 30  J1259-2310   13 22 23  35.8 186.3  0.4       5.9    20     3417   03 59 30
04 00 30  =1256-229    13 23 24  35.8 186.6  0.4       6.2    60     3433   03 59 31

04 00 30  J1311-2329   13 23 24  35.7 183.0  0.2       2.9   -10     3433   04 00 40
04 02 00  ---          13 24 54  35.7 183.5  0.2       3.3    80     3453   04 00 31

04 02 00  EM170817     13 24 54  35.8 184.0  0.2       3.7    -8     3453   04 02 08
04 04 30  ---          13 27 24  35.7 184.7  0.3       4.4   142     3490   04 02 01

04 04 30  J1311-2329   13 27 24  35.7 184.2  0.2       3.9    -8     3490   04 04 38
04 06 00  ---          13 28 55  35.6 184.6  0.3       4.3    82     3511   04 04 31

04 06 00  J1312-2350   13 28 55  35.3 184.2  0.3       4.0    -8     3511   04 06 08
04 07 00  ---          13 29 55  35.3 184.5  0.3       4.2    52     3524   04 06 01

04 07 30  J1259-2310   13 30 25  35.6 188.6  0.5       8.0    19     3524   04 07 30
04 08 30  =1256-229    13 31 25  35.6 188.8  0.5       8.3    60     3540   04 07 31

04 08 30  J1311-2329   13 31 25  35.6 185.3  0.3       5.0   -10     3540   04 08 40
04 10 00  ---          13 32 55  35.6 185.7  0.3       5.4    80     3561   04 08 31

04 10 00  EM170817     13 32 55  35.6 186.2  0.4       5.9    -8     3561   04 10 08
04 12 30  ---          13 35 26  35.6 186.9  0.4       6.5   142     3597   04 10 01

04 12 30  J1311-2329   13 35 26  35.5 186.4  0.4       6.0    -8     3597   04 12 38
04 14 00  ---          13 36 56  35.5 186.8  0.4       6.4    82     3618   04 12 31

04 14 00  EM170817     13 36 56  35.5 187.4  0.4       6.9    -8     3618   04 14 08
04 16 30  ---          13 39 26  35.5 188.1  0.5       7.6   142     3655   04 14 01

04 17 00  J1259-2310   13 39 56  35.2 191.2  0.7      10.5    20     3655   04 17 00
04 18 00  =1256-229    13 40 57  35.2 191.5  0.7      10.8    60     3670   04 17 01

04 18 00  J1311-2329   13 40 57  35.3 188.0  0.5       7.5   -10     3670   04 18 10
04 19 30  ---          13 42 27  35.3 188.4  0.5       7.9    80     3691   04 18 01

04 19 30  EM170817     13 42 27  35.4 188.9  0.5       8.3    -8     3691   04 19 38
04 22 00  ---          13 44 57  35.3 189.6  0.6       9.0   142     3728   04 19 31

04 22 00  J1311-2329   13 44 57  35.2 189.1  0.5       8.5    -8     3728   04 22 08
04 23 30  ---          13 46 27  35.2 189.5  0.6       8.9    82     3749   04 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

04 23 30  EM170817     13 46 27  35.2 190.0  0.6       9.4    -8     3749   04 23 38
04 26 00  ---          13 48 58  35.1 190.7  0.6      10.0   142     3785   04 23 31

04 26 30  J1259-2310   13 49 28  34.8 193.8  0.8      12.9    20     3785   04 26 30
04 27 30  =1256-229    13 50 28  34.8 194.1  0.8      13.2    60     3801   04 26 31

04 27 30  J1311-2329   13 50 28  35.0 190.6  0.6       9.9   -10     3801   04 27 40
04 29 00  ---          13 51 58  35.0 191.0  0.7      10.3    80     3821   04 27 31

04 29 00  EM170817     13 51 58  35.0 191.5  0.7      10.8    -8     3821   04 29 08
04 31 30  ---          13 54 29  34.9 192.2  0.7      11.5   142     3858   04 29 01

04 31 30  J1311-2329   13 54 29  34.8 191.7  0.7      11.0    -8     3858   04 31 38
04 33 00  ---          13 55 59  34.8 192.1  0.7      11.4    82     3879   04 31 31

04 33 00  EM170817     13 55 59  34.8 192.6  0.8      11.8    -8     3879   04 33 08
04 35 30  ---          13 58 29  34.7 193.3  0.8      12.5   142     3916   04 33 01

04 36 00  J1259-2310   13 58 59  34.3 196.4  1.0      15.3    20     3916   04 36 00
04 37 00  =1256-229    14 00 00  34.2 196.7  1.0      15.6    60     3931   04 36 01

04 37 00  J1311-2329   14 00 00  34.6 193.2  0.8      12.4   -10     3931   04 37 10
04 38 30  ---          14 01 30  34.5 193.6  0.8      12.8    80     3952   04 37 01

04 38 30  EM170817     14 01 30  34.5 194.1  0.8      13.2    -8     3952   04 38 38
04 41 00  ---          14 04 00  34.4 194.8  0.9      13.9   142     3988   04 38 31

04 41 00  J1311-2329   14 04 00  34.4 194.3  0.9      13.4    -8     3988   04 41 08
04 42 30  ---          14 05 31  34.3 194.7  0.9      13.8    82     4009   04 41 01

04 42 30  J1312-2350   14 05 31  34.0 194.3  0.9      13.4    -8     4009   04 42 38
04 43 30  ---          14 06 31  34.0 194.5  0.9      13.7    52     4023   04 42 31

04 44 00  J1259-2310   14 07 01  33.8 198.5  1.1      17.3    19     4023   04 44 00
04 45 00  =1256-229    14 08 01  33.7 198.8  1.1      17.6    60     4038   04 44 01

04 45 00  J1311-2329   14 08 01  34.2 195.4  0.9      14.4   -10     4038   04 45 10
04 46 30  ---          14 09 31  34.1 195.8  0.9      14.8    80     4059   04 45 01

04 46 30  EM170817     14 09 31  34.1 196.3  1.0      15.3    -8     4059   04 46 38
04 49 00  ---          14 12 02  33.9 197.0  1.0      15.9   142     4095   04 46 31

04 49 00  J1311-2329   14 12 02  33.9 196.4  1.0      15.4    -8     4095   04 49 08
04 50 30  ---          14 13 32  33.8 196.8  1.0      15.8    82     4117   04 49 01
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

04 50 30  EM170817     14 13 32  33.8 197.4  1.0      16.3    -8     4117   04 50 38
04 53 00  ---          14 16 02  33.7 198.0  1.1      16.9   142     4153   04 50 31

04 53 30  J1259-2310   14 16 32  33.1 201.0  1.3      19.6    20     4153   04 53 30
04 54 30  =1256-229    14 17 33  33.0 201.3  1.3      19.9    60     4169   04 53 31

04 54 30  J1311-2329   14 17 33  33.6 197.9  1.1      16.8   -10     4169   04 54 40
04 56 00  ---          14 19 03  33.5 198.3  1.1      17.1    80     4189   04 54 31

04 56 00  EM170817     14 19 03  33.5 198.8  1.1      17.6    -8     4189   04 56 08
04 58 30  ---          14 21 33  33.3 199.5  1.2      18.2   142     4226   04 56 01

04 58 30  J1311-2329   14 21 33  33.3 199.0  1.1      17.8    -8     4226   04 58 38
05 00 00  ---          14 23 03  33.2 199.3  1.2      18.1    82     4247   04 58 31

05 00 00  EM170817     14 23 03  33.2 199.9  1.2      18.6    -8     4247   05 00 08
05 02 30  ---          14 25 34  33.0 200.5  1.2      19.2   142     4283   05 00 01

05 03 00  J1259-2310   14 26 04  32.3 203.4  1.4      21.9    20     4283   05 03 00
05 04 00  =1256-229    14 27 04  32.2 203.7  1.4      22.1    60     4299   05 03 01

05 04 00  J1311-2329   14 27 04  32.9 200.4  1.2      19.1   -10     4299   05 04 10
05 05 30  ---          14 28 34  32.8 200.8  1.3      19.5    80     4320   05 04 01

05 05 30  EM170817     14 28 34  32.8 201.3  1.3      19.9    -8     4320   05 05 38
05 08 00  ---          14 31 05  32.6 201.9  1.3      20.5   142     4356   05 05 31

05 08 00  J1311-2329   14 31 05  32.6 201.4  1.3      20.0    -8     4356   05 08 08
05 09 30  ---          14 32 35  32.5 201.8  1.3      20.4    82     4377   05 08 01

05 09 30  EM170817     14 32 35  32.4 202.3  1.4      20.9    -8     4377   05 09 38
05 12 00  ---          14 35 05  32.2 202.9  1.4      21.5   142     4414   05 09 31

05 12 30  J1259-2310   14 35 35  31.4 205.8  1.6      24.1    20     4414   05 12 30
05 13 30  =1256-229    14 36 36  31.3 206.1  1.6      24.3    60     4429   05 12 31

05 13 30  J1311-2329   14 36 36  32.2 202.8  1.4      21.4   -10     4429   05 13 40
05 15 00  ---          14 38 06  32.0 203.2  1.4      21.7    80     4450   05 13 31

05 15 00  EM170817     14 38 06  32.0 203.7  1.5      22.2    -8     4450   05 15 08
05 17 30  ---          14 40 36  31.8 204.3  1.5      22.7   142     4487   05 15 01

05 17 30  J1311-2329   14 40 36  31.8 203.8  1.5      22.3    -8     4487   05 17 38
05 19 00  ---          14 42 07  31.7 204.2  1.5      22.6    82     4508   05 17 31
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

05 19 00  J1312-2350   14 42 07  31.5 203.7  1.5      22.3    -8     4508   05 19 08
05 20 00  ---          14 43 07  31.4 204.0  1.5      22.5    52     4521   05 19 01

05 20 30  J1259-2310   14 43 37  30.7 207.8  1.7      25.9    20     4521   05 20 30
05 21 30  =1256-229    14 44 37  30.6 208.0  1.7      26.1    60     4536   05 20 31

05 21 30  J1311-2329   14 44 37  31.5 204.8  1.5      23.2   -10     4536   05 21 40
05 23 00  ---          14 46 07  31.3 205.2  1.6      23.6    80     4557   05 21 31

05 23 00  EM170817     14 46 07  31.3 205.7  1.6      24.0    -8     4557   05 23 08
05 25 30  ---          14 48 38  31.0 206.3  1.6      24.6   142     4594   05 23 01

05 25 30  J1311-2329   14 48 38  31.1 205.8  1.6      24.1    -8     4594   05 25 38
05 27 00  ---          14 50 08  30.9 206.2  1.6      24.5    82     4615   05 25 31

05 27 00  EM170817     14 50 08  30.9 206.7  1.7      24.9    -8     4615   05 27 08
05 29 30  ---          14 52 38  30.6 207.3  1.7      25.5   142     4651   05 27 01

05 30 00  J1259-2310   14 53 08  29.7 210.0  1.9      27.9    20     4651   05 30 00
05 31 00  =1256-229    14 54 09  29.6 210.3  1.9      28.2    60     4667   05 30 01

05 31 00  J1311-2329   14 54 09  30.6 207.1  1.7      25.4   -10     4667   05 31 10
05 32 30  ---          14 55 39  30.4 207.5  1.7      25.7    80     4687   05 31 01

05 32 30  EM170817     14 55 39  30.3 208.0  1.7      26.1    -8     4687   05 32 38
05 35 00  ---          14 58 09  30.1 208.6  1.8      26.7   142     4724   05 32 31

05 35 00  J1311-2329   14 58 09  30.2 208.1  1.8      26.2    -8     4724   05 35 08
05 36 30  ---          14 59 39  30.0 208.5  1.8      26.6    82     4745   05 35 01

05 36 30  EM170817     14 59 39  29.9 208.9  1.8      27.0    -8     4745   05 36 38
05 39 00  ---          15 02 10  29.7 209.5  1.9      27.5   142     4782   05 36 31

05 39 30  J1259-2310   15 02 40  28.6 212.2  2.0      30.0    20     4782   05 39 30
05 40 30  =1256-229    15 03 40  28.5 212.4  2.1      30.2    60     4797   05 39 31

05 40 30  J1311-2329   15 03 40  29.6 209.4  1.9      27.4   -10     4797   05 40 40
05 42 00  ---          15 05 10  29.4 209.7  1.9      27.8    80     4818   05 40 31

05 42 00  EM170817     15 05 10  29.3 210.2  1.9      28.2    -8     4818   05 42 08
05 44 30  ---          15 07 41  29.1 210.8  1.9      28.7   142     4854   05 42 01

05 44 30  J1311-2329   15 07 41  29.2 210.3  1.9      28.3    -8     4854   05 44 38
05 46 00  ---          15 09 11  29.0 210.7  1.9      28.6    82     4876   05 44 31
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

05 46 00  EM170817     15 09 11  28.9 211.2  2.0      29.0    -8     4876   05 46 08
05 48 30  ---          15 11 41  28.6 211.7  2.0      29.6   142     4912   05 46 01

05 49 00  J1259-2310   15 12 11  27.5 214.3  2.2      31.9    20     4912   05 49 00
05 50 00  =1256-229    15 13 12  27.4 214.6  2.2      32.1    60     4928   05 49 01

05 50 00  J1311-2329   15 13 12  28.5 211.6  2.0      29.5   -10     4928   05 50 10
05 51 30  ---          15 14 42  28.4 211.9  2.0      29.8    80     4948   05 50 01

05 51 30  EM170817     15 14 42  28.3 212.4  2.1      30.2    -8     4948   05 51 38
05 54 00  ---          15 17 12  28.0 213.0  2.1      30.7   142     4985   05 51 31

05 54 00  J1311-2329   15 17 12  28.1 212.5  2.1      30.3    -8     4985   05 54 08
05 55 30  ---          15 18 43  27.9 212.8  2.1      30.6    82     5006   05 54 01

05 55 30  J1312-2350   15 18 43  27.8 212.4  2.1      30.3    -8     5006   05 55 38
05 56 30  ---          15 19 43  27.6 212.6  2.1      30.5    52     5019   05 55 31

05 57 00  J1259-2310   15 20 13  26.5 216.1  2.3      33.5    20     5019   05 57 00
05 58 00  =1256-229    15 21 13  26.4 216.3  2.4      33.7    60     5035   05 57 01

05 58 00  J1311-2329   15 21 13  27.6 213.4  2.1      31.1   -11     5035   05 58 11
05 59 30  ---          15 22 43  27.4 213.7  2.2      31.4    79     5055   05 58 01

05 59 30  EM170817     15 22 43  27.3 214.2  2.2      31.8    -8     5055   05 59 38
06 02 00  ---          15 25 14  27.0 214.7  2.2      32.3   142     5092   05 59 31

06 02 00  J1311-2329   15 25 14  27.1 214.3  2.2      31.9    -8     5092   06 02 08
06 03 30  ---          15 26 44  27.0 214.6  2.2      32.2    82     5113   06 02 01

06 03 30  EM170817     15 26 44  26.8 215.1  2.3      32.6    -8     5113   06 03 38
06 06 00  ---          15 29 14  26.5 215.6  2.3      33.1   142     5149   06 03 31

06 06 30  J1259-2310   15 29 44  25.2 218.1  2.5      35.3    20     5149   06 06 30
06 07 30  =1256-229    15 30 45  25.1 218.3  2.5      35.5    60     5165   06 06 31

06 07 30  J1311-2329   15 30 45  26.5 215.5  2.3      33.0   -11     5165   06 07 41
06 09 00  ---          15 32 15  26.3 215.8  2.3      33.3    79     5185   06 07 31

06 09 00  EM170817     15 32 15  26.1 216.2  2.4      33.7    -8     5185   06 09 08
06 11 30  ---          15 34 45  25.8 216.8  2.4      34.2   142     5222   06 09 01

06 11 30  J1311-2329   15 34 45  26.0 216.3  2.4      33.8    -8     5222   06 11 38
06 13 00  ---          15 36 15  25.8 216.6  2.4      34.1    82     5243   06 11 31
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

06 13 00  EM170817     15 36 15  25.6 217.1  2.4      34.5    -8     5243   06 13 08
06 15 30  ---          15 38 46  25.3 217.6  2.5      34.9   142     5280   06 13 01

06 16 00  J1259-2310   15 39 16  24.0 220.0  2.7      37.0    19     5280   06 16 00
06 17 00  =1256-229    15 40 16  23.8 220.2  2.7      37.2    60     5295   06 16 01

06 17 00  J1311-2329   15 40 16  25.2 217.5  2.5      34.8   -11     5295   06 17 11
06 18 30  ---          15 41 46  25.0 217.8  2.5      35.1    79     5315   06 17 01

06 18 30  EM170817     15 41 46  24.9 218.2  2.5      35.5    -8     5315   06 18 38
06 21 00  ---          15 44 17  24.6 218.8  2.6      36.0   142     5352   06 18 31

06 21 00  J1311-2329   15 44 17  24.7 218.3  2.5      35.6    -8     5352   06 21 08
06 22 30  ---          15 45 47  24.5 218.6  2.6      35.9    82     5373   06 21 01

06 22 30  EM170817     15 45 47  24.4 219.1  2.6      36.2    -8     5373   06 22 38
06 25 00  ---          15 48 17  24.0 219.6  2.6      36.7   142     5410   06 22 31

06 25 30  J1259-2310   15 48 47  22.6 221.9  2.8      38.7    19     5410   06 25 30
06 26 30  =1256-229    15 49 48  22.5 222.1  2.8      38.9    60     5425   06 25 31

06 26 30  J1311-2329   15 49 48  24.0 219.4  2.6      36.6   -11     5425   06 26 41
06 28 00  ---          15 51 18  23.8 219.7  2.6      36.9    79     5445   06 26 31

06 28 00  EM170817     15 51 18  23.6 220.2  2.7      37.2    -8     5445   06 28 08
06 30 30  ---          15 53 48  23.3 220.7  2.7      37.7   142     5482   06 28 01

06 30 30  J1311-2329   15 53 48  23.4 220.2  2.7      37.3    -8     5482   06 30 38
06 32 00  ---          15 55 19  23.2 220.5  2.7      37.6    82     5503   06 30 31

06 32 00  J1312-2350   15 55 19  23.1 220.1  2.7      37.3    -8     5503   06 32 08
06 33 00  ---          15 56 19  23.0 220.3  2.7      37.5    52     5517   06 32 01

06 33 30  J1259-2310   15 56 49  21.4 223.4  2.9      40.1    19     5517   06 33 30
06 34 30  =1256-229    15 57 49  21.3 223.6  3.0      40.3    60     5532   06 33 31

06 34 30  J1311-2329   15 57 49  22.9 221.0  2.8      38.0   -11     5532   06 34 41
06 36 00  ---          15 59 19  22.6 221.3  2.8      38.3    79     5552   06 34 31

06 36 00  EM170817     15 59 19  22.5 221.7  2.8      38.7    -8     5552   06 36 08
06 38 30  ---          16 01 50  22.1 222.2  2.9      39.1   142     5589   06 36 01

06 38 30  J1311-2329   16 01 50  22.3 221.8  2.8      38.7    -8     5589   06 38 38
06 40 00  ---          16 03 20  22.1 222.1  2.8      39.0    82     5610   06 38 31
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

06 40 00  EM170817     16 03 20  21.9 222.5  2.9      39.3    -8     5610   06 40 08
06 42 30  ---          16 05 50  21.5 223.0  2.9      39.8   142     5647   06 40 01

06 43 00  J1259-2310   16 06 20  20.0 225.2  3.1      41.7    19     5647   06 43 00
06 44 00  =1256-229    16 07 21  19.9 225.4  3.1      41.8    60     5662   06 43 01

06 44 00  J1311-2329   16 07 21  21.5 222.9  2.9      39.7   -11     5662   06 44 11
06 45 30  ---          16 08 51  21.3 223.1  2.9      39.9    79     5682   06 44 01

06 45 30  EM170817     16 08 51  21.1 223.6  3.0      40.3    -8     5682   06 45 38
06 48 00  ---          16 11 21  20.7 224.0  3.0      40.7   142     5719   06 45 31

06 48 00  J1311-2329   16 11 21  20.9 223.6  3.0      40.4    -8     5719   06 48 08
06 49 30  ---          16 12 51  20.7 223.9  3.0      40.6    82     5740   06 48 01

06 49 30  EM170817     16 12 51  20.5 224.3  3.0      40.9    -8     5740   06 49 38
06 52 00  ---          16 15 22  20.1 224.8  3.1      41.4   142     5777   06 49 31

06 52 30  J1259-2310   16 15 52  18.5 226.9  3.3      43.2    19     5777   06 52 30
06 53 30  =1256-229    16 16 52  18.4 227.1  3.3      43.3    60     5792   06 52 31

06 53 30  J1311-2329   16 16 52  20.1 224.6  3.1      41.3   -11     5792   06 53 41
06 55 00  ---          16 18 22  19.8 224.9  3.1      41.5    79     5813   06 53 31

06 55 00  EM170817     16 18 22  19.7 225.3  3.1      41.8    -8     5813   06 55 08
06 57 30  ---          16 20 53  19.3 225.8  3.2      42.2   142     5849   06 55 01

06 57 30  J1311-2329   16 20 53  19.5 225.4  3.1      41.9    -8     5849   06 57 38
06 59 00  ---          16 22 23  19.2 225.6  3.2      42.2    82     5870   06 57 31

06 59 00  EM170817     16 22 23  19.0 226.0  3.2      42.5    -8     5870   06 59 08
07 01 30  ---          16 24 53  18.6 226.5  3.2      42.9   142     5907   06 59 01

07 02 00  J1259-2310   16 25 23  17.0 228.6  3.4      44.6    19     5907   07 02 00
07 03 00  =1256-229    16 26 24  16.9 228.8  3.4      44.8    60     5922   07 02 01

07 03 00  J1311-2329   16 26 24  18.6 226.3  3.2      42.8   -11     5922   07 03 11
07 04 30  ---          16 27 54  18.4 226.6  3.3      43.0    79     5943   07 03 01

07 04 30  EM170817     16 27 54  18.2 227.0  3.3      43.3    -8     5943   07 04 38
07 07 00  ---          16 30 24  17.8 227.5  3.3      43.7   142     5979   07 04 31

07 07 00  J1311-2329   16 30 24  18.0 227.1  3.3      43.4    -8     5979   07 07 08
07 08 30  ---          16 31 55  17.7 227.3  3.3      43.6    82     6000   07 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  27 May 2018   Day 147 ---

07 08 30  J1312-2350   16 31 55  17.7 226.9  3.3      43.4    -8     6000   07 08 38
07 09 30  ---          16 32 55  17.5 227.0  3.3      43.5    52     6014   07 08 31

07 10 00  J1259-2310   16 33 25  15.7 229.9  3.6      45.8    19     6014   07 10 00
07 11 00  =1256-229    16 34 25  15.5 230.1  3.6      45.9    60     6029   07 10 01

07 11 00  J1311-2329   16 34 25  17.3 227.8  3.4      44.0   -12     6029   07 11 12
07 12 30  ---          16 35 55  17.1 228.0  3.4      44.3    78     6049   07 11 01

07 12 30  EM170817     16 35 55  16.9 228.4  3.4      44.6    -8     6049   07 12 38
07 15 00  ---          16 38 26  16.5 228.8  3.5      44.9   142     6086   07 12 31

07 15 00  J1311-2329   16 38 26  16.7 228.4  3.4      44.6    -8     6086   07 15 08
07 16 30  ---          16 39 56  16.5 228.7  3.5      44.9    82     6107   07 15 01

07 16 30  EM170817     16 39 56  16.2 229.1  3.5      45.1    -8     6107   07 16 38
07 19 00  ---          16 42 26  15.8 229.5  3.5      45.5   142     6144   07 16 31

07 19 30  J1259-2310   16 42 56  14.1 231.5  3.7      47.1    19     6144   07 19 30
07 20 30  =1256-229    16 43 57  14.0 231.7  3.7      47.3    60     6159   07 19 31

07 21 20  J1337-1257   16 44 47  27.5 232.8  3.1      44.7    15     6159   07 21 20
07 25 40  =1334-127    16 49 07  26.7 233.7  3.2      45.4   260     6226   07 21 21

07 27 00  3C286        16 50 28  47.6 282.9  3.3      76.5    31     6226   07 27 00
07 30 00  ---          16 53 28  47.0 283.2  3.4      76.3   180     6272   07 27 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess218.C2048glob
   Matching groups in /usr/local/sched_11.4mod/catalogs/freq_RDBE.dat:
     vc_d

   Setup group:    5         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  13.6      4.1     13.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  12  Setup file default.  Used with PCAL = off
   LO sum=   4740.00  4740.00  4804.00  4804.00  4868.00  4868.00  4932.00  4932.00
   BBC fr=    640.00   640.00   704.00   704.00   768.00   768.00   832.00   832.00
   Bandwd=     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     728.00    728.00    792.00    792.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  12  13  15  16  18  19  20  21  22  23

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * EM170817          13 07 05.876058   * 13 09 48.089000     13 10 48.059737       0.00
                    -23 06 55.47686    *-23 22 53.35000     -23 28 46.60775        0.00
                     From catalog imbedded in main SCHED input file.

 * J1303-2405        13 00 37.951987   * 13 03 19.646900     13 04 19.412523       0.00
                    -23 48 57.23719    *-24 05 03.05600     -24 10 59.73739        0.00
                     From catalog imbedded in main SCHED input file.

 * J1312-2350        13 10 05.987814   * 13 12 48.758100     13 13 48.954220       0.00
                    -23 34 53.02797    *-23 50 46.95300     -23 56 38.69325        0.00
                     From catalog imbedded in main SCHED input file.

 * J1311-2329        13 08 54.934098   * 13 11 37.413987     13 12 37.492380       0.00
                    -23 14 01.14446    *-23 29 56.64651     -23 35 48.95875        0.00
                     From catalog imbedded in main SCHED input file.

   1256-229          12 56 27.604314   * 12 59 08.462031     13 00 07.885767       0.09
 * J1259-2310       -22 54 28.11906    *-23 10 38.65427     -23 16 37.09892        0.21
                     /usr/local/sched_11.4mod/catalogs/sources.gsfc
                     GSFC 2015a astro solution, unpublished    244 observations.

 * 3C286             13 28 49.657758   * 13 31 08.288051     13 31 59.332128       0.18
   J1331+3030        30 45 58.64059    * 30 30 32.95924      30 25 04.96612        0.17
   1328+307          /usr/local/sched_11.4mod/catalogs/sources.gsfc
   J1331+30          GSFC 2015a astro solution, unpublished    225 observations.

   1334-127          13 34 59.803873   * 13 37 39.782778     13 38 38.887019       0.00
 * J1337-1257       -12 42 09.74301    *-12 57 24.69328     -13 02 58.64768        0.00
   J1337-12          /usr/local/sched_11.4mod/catalogs/sources.gsfc
                     GSFC 2015a astro solution, unpublished  91811 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  EM170817   sess218.C2048glob     1 2 4 5 6 7 8 9 10 11 12 14 +     8.000   230.990
  J1303-2405 sess218.C2048glob     1 2 4 5 6 7 8 9 10 11 12 14       0.500    10.914
  J1312-2350 sess218.C2048glob     1 2 4 5 6 7 8 9 10 11 12 14 +     1.600    32.849
  J1311-2329 sess218.C2048glob     1 2 4 5 6 7 8 9 10 11 12 14 +     5.944   158.325
  J1259-2310 sess218.C2048glob     12 14 17                          0.792    38.058
  3C286      sess218.C2048glob     12 17                             0.100     1.314
  J1337-1257 sess218.C2048glob     1 2 4 5 6 7 8 9 10 11 12 14 +     1.322    12.512


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   EM170817           137.6
   J1303-2405         136.2
   J1312-2350         138.3
   J1311-2329         138.0
   J1259-2310         135.1
   3C286              115.2
   J1337-1257         141.9

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

