  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Tracing the Evolution of Fast Jet-Driven Outflows
 Exp. Code:  GN002C  


Schedule Version:       3.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Kristina Nyland

Address:  ASTRON, Oude Hoogeveensedijk 4
          7991 PD Dwingeloo
          The Netherlands
 

Phone:    0521-595-766
EMAIL:    nyland@astron.nl
Fax:
Phone during observation: 0521-595-766

Observing mode: 21cm spectral line

Notes:    Target: 4C52
          Phase calibrator: J1545+5400
          Bandpass Calibrator: 1638+5720 (switching angle = 6.85 deg)
          Alt Bandpass Calibrator: 1549+5038 (switching angle = 2.96 deg)

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  15 Oct 2015   Day 288 ---

 Next scan frequencies:  1292.50  1292.50  1308.50  1308.50  1324.50  1324.50  1340.50  1340.50
 Next BBC frequencies:    807.50   807.50   791.50   791.50   775.50   775.50   759.50   759.50
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00

15 30 00  J1545+5400   10 09 37  27.6  41.3 -5.6     -75.1     0        0   15 30 00
15 32 00  =1544+541    10 11 37  27.9  41.4 -5.6     -75.4   120        8   15 30 01

15 32 00  4C52         10 11 37  25.1  42.0 -5.9     -71.7   -14        8   15 32 14
15 35 00  ---          10 14 37  25.5  42.1 -5.8     -72.3   166       18   15 32 01

15 35 50  J1545+5400   10 15 28  28.5  41.6 -5.5     -76.1    36       18   15 35 50
15 37 50  =1544+541    10 17 28  28.8  41.7 -5.5     -76.5   120       26   15 35 51

15 37 50  4C52         10 17 28  26.0  42.3 -5.8     -72.8   -14       26   15 38 04
15 40 50  ---          10 20 28  26.4  42.4 -5.7     -73.3   166       37   15 37 51

15 41 40  J1545+5400   10 21 18  29.3  41.8 -5.4     -77.2    36       37   15 41 40
15 42 40  =1544+541    10 22 19  29.5  41.8 -5.4     -77.4    60       41   15 41 41

15 42 40  4C52         10 22 19  26.7  42.5 -5.7     -73.6   -13       41   15 42 53
15 45 40  ---          10 25 19  27.1  42.7 -5.6     -74.2   167       51   15 42 41

15 46 30  J1545+5400   10 26 09  30.0  42.0 -5.3     -78.1    36       51   15 46 30
15 48 30  =1544+541    10 28 10  30.3  42.1 -5.3     -78.5   120       59   15 46 31

15 48 30  4C52         10 28 10  27.5  42.8 -5.6     -74.7   -13       59   15 48 43
15 51 30  ---          10 31 10  28.0  42.9 -5.5     -75.2   167       70   15 48 31

15 52 20  J1545+5400   10 32 00  30.8  42.2 -5.2     -79.2    36       70   15 52 20
15 53 20  =1544+541    10 33 00  31.0  42.2 -5.2     -79.4    60       74   15 52 21

15 53 20  4C52         10 33 00  28.2  43.0 -5.5     -75.5   -13       74   15 53 33
15 56 20  ---          10 36 01  28.7  43.1 -5.5     -76.1   167       85   15 53 21

15 57 10  J1545+5400   10 36 51  31.6  42.3 -5.2     -80.1    36       85   15 57 10
15 59 10  =1544+541    10 38 51  31.8  42.4 -5.1     -80.4   120       92   15 57 11

15 59 10  4C52         10 38 51  29.1  43.2 -5.4     -76.6   -13       92   15 59 23
16 02 10  ---          10 41 52  29.5  43.4 -5.4     -77.1   167      103   15 59 11

16 03 00  J1545+5400   10 42 42  32.4  42.5 -5.1     -81.2    37      103   16 03 00
16 04 00  =1544+541    10 43 42  32.5  42.5 -5.0     -81.4    60      107   16 03 01

16 04 00  4C52         10 43 42  29.8  43.4 -5.3     -77.5   -13      107   16 04 13
16 07 00  ---          10 46 43  30.2  43.5 -5.3     -78.0   167      118   16 04 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  15 Oct 2015   Day 288 ---

16 07 50  J1545+5400   10 47 33  33.1  42.6 -5.0     -82.1    37      118   16 07 50
16 09 50  =1544+541    10 49 33  33.4  42.7 -4.9     -82.5   120      125   16 07 51

16 09 50  4C52         10 49 33  30.7  43.6 -5.2     -78.5   -13      125   16 10 03
16 12 50  ---          10 52 34  31.1  43.8 -5.2     -79.1   167      136   16 09 51

16 13 40  J1545+5400   10 53 24  34.0  42.8 -4.9     -83.2    37      136   16 13 40
16 14 40  =1544+541    10 54 24  34.1  42.8 -4.9     -83.4    60      140   16 13 41

16 14 40  4C52         10 54 24  31.4  43.8 -5.1     -79.4   -13      140   16 14 53
16 17 40  ---          10 57 24  31.8  43.9 -5.1     -79.9   167      151   16 14 41

16 18 30  J1545+5400   10 58 15  34.7  42.8 -4.8     -84.1    37      151   16 18 30
16 20 30  =1544+541    11 00 15  35.0  42.9 -4.8     -84.5   120      159   16 18 31

16 20 30  4C52         11 00 15  32.3  44.0 -5.0     -80.5   -13      159   16 20 43
16 23 30  ---          11 03 15  32.7  44.1 -5.0     -81.0   167      169   16 20 31

16 24 20  J1545+5400   11 04 05  35.5  42.9 -4.7     -85.2    37      169   16 24 20
16 25 20  =1544+541    11 05 06  35.7  43.0 -4.7     -85.4    60      173   16 24 21

16 25 20  4C52         11 05 06  33.0  44.1 -5.0     -81.3   -13      173   16 25 33
16 28 20  ---          11 08 06  33.4  44.2 -4.9     -81.9   167      184   16 25 21

16 29 10  J1545+5400   11 08 56  36.2  43.0 -4.6     -86.2    37      184   16 29 10
16 31 10  =1544+541    11 10 57  36.5  43.0 -4.6     -86.6   120      192   16 29 11

16 31 10  4C52         11 10 57  33.9  44.3 -4.9     -82.4   -13      192   16 31 23
16 34 10  ---          11 13 57  34.3  44.4 -4.8     -83.0   167      202   16 31 11

16 35 00  J1545+5400   11 14 47  37.1  43.1 -4.5     -87.3    37      202   16 35 00
16 36 00  =1544+541    11 15 47  37.2  43.1 -4.5     -87.5    60      206   16 35 01

16 36 00  4C52         11 15 47  34.6  44.4 -4.8     -83.3   -13      206   16 36 13
16 39 00  ---          11 18 48  35.0  44.5 -4.7     -83.9   167      217   16 36 01

16 39 50  J1545+5400   11 19 38  37.8  43.1 -4.4     -88.3    37      217   16 39 50
16 41 50  =1544+541    11 21 38  38.1  43.1 -4.4     -88.7   120      225   16 39 51

16 43 07  J1638+5720   11 22 56  31.2  38.3 -5.3     -80.9    55      225   16 43 07
16 46 57  =1637+574    11 26 56  31.8  38.4 -5.2     -81.7   230      240   16 43 08

16 48 17  J1545+5400   11 28 06  39.0  43.1 -4.3     -90.0    58      240   16 48 17
16 51 07  =1544+541    11 31 07  39.5  43.1 -4.2     -90.6   170      250   16 48 18
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  15 Oct 2015   Day 288 ---

16 51 07  4C52         11 30 57  36.9  44.7 -4.5     -86.2   -13      250   16 51 20
16 54 07  ---          11 33 57  37.3  44.7 -4.5     -86.8   167      261   16 51 08

16 54 57  J1545+5400   11 34 47  40.0  43.1 -4.2     -91.3    37      261   16 54 57
16 56 57  =1544+541    11 36 48  40.3  43.1 -4.2     -91.8   120      269   16 54 58

16 56 57  4C52         11 36 48  37.8  44.7 -4.4     -87.3   -13      269   16 57 10
16 59 57  ---          11 39 48  38.2  44.7 -4.4     -87.9   167      280   16 56 58

17 00 47  J1545+5400   11 40 38  40.9  43.1 -4.1     -92.6    37      280   17 00 47
17 01 47  =1544+541    11 41 38  41.0  43.1 -4.1     -92.8    60      284   17 00 48

17 01 47  4C52         11 41 38  38.5  44.8 -4.4     -88.3   -13      284   17 02 00
17 04 47  ---          11 44 39  39.0  44.8 -4.3     -88.8   167      294   17 01 48

17 05 37  J1545+5400   11 45 29  41.6  43.0 -4.0     -93.6    37      294   17 05 37
17 07 37  =1544+541    11 47 29  41.9  43.0 -4.0     -94.0   120      302   17 05 38

17 07 37  4C52         11 47 29  39.4  44.8 -4.3     -89.4   -13      302   17 07 50
17 10 37  ---          11 50 30  39.8  44.8 -4.2     -90.0   167      313   17 07 38

17 11 27  J1545+5400   11 51 20  42.5  42.9 -3.9     -94.8    37      313   17 11 27
17 12 27  =1544+541    11 52 20  42.6  42.9 -3.9     -95.0    60      317   17 11 28

17 12 27  4C52         11 52 20  40.1  44.8 -4.2     -90.4   -13      317   17 12 40
17 15 27  ---          11 55 21  40.6  44.8 -4.1     -91.0   167      327   17 12 28

17 16 17  J1545+5400   11 56 11  43.2  42.8 -3.8     -95.9    37      327   17 16 17
17 18 17  =1544+541    11 58 11  43.5  42.8 -3.8     -96.3   120      335   17 16 18

17 18 17  4C52         11 58 11  41.0  44.8 -4.1     -91.5   -13      335   17 18 30
17 21 17  ---          12 01 12  41.5  44.7 -4.0     -92.2   167      346   17 18 18

17 22 07  J1545+5400   12 02 02  44.0  42.7 -3.7     -97.1    37      346   17 22 07
17 23 07  =1544+541    12 03 02  44.2  42.7 -3.7     -97.3    60      350   17 22 08

17 23 07  4C52         12 03 02  41.7  44.7 -4.0     -92.5   -13      350   17 23 20
17 26 07  ---          12 06 02  42.2  44.7 -4.0     -93.1   167      361   17 23 08

17 26 57  J1545+5400   12 06 53  44.7  42.6 -3.7     -98.2    37      361   17 26 57
17 28 57  =1544+541    12 08 53  45.0  42.5 -3.6     -98.6   120      368   17 26 58

17 28 57  4C52         12 08 53  42.6  44.7 -3.9     -93.7   -13      368   17 29 10
17 31 57  ---          12 11 53  43.1  44.6 -3.9     -94.4   167      379   17 28 58
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  15 Oct 2015   Day 288 ---

17 32 47  J1545+5400   12 12 44  45.6  42.4 -3.6     -99.5    37      379   17 32 47
17 33 47  =1544+541    12 13 44  45.7  42.4 -3.5     -99.7    60      383   17 32 48

17 33 47  4C52         12 13 44  43.4  44.6 -3.8     -94.8   -13      383   17 34 00
17 36 47  ---          12 16 44  43.8  44.5 -3.8     -95.4   167      394   17 33 48

17 37 37  J1545+5400   12 17 34  46.3  42.2 -3.5    -100.6    37      394   17 37 37
17 39 37  =1544+541    12 19 35  46.6  42.1 -3.4    -101.1   120      401   17 37 38

17 39 37  4C52         12 19 35  44.2  44.5 -3.7     -96.0   -13      401   17 39 49
17 42 37  ---          12 22 35  44.7  44.4 -3.7     -96.6   167      412   17 39 38

17 43 27  J1545+5400   12 23 25  47.1  42.0 -3.4    -102.0    37      412   17 43 27
17 44 27  =1544+541    12 24 25  47.3  41.9 -3.4    -102.2    60      416   17 43 28

17 44 27  4C52         12 24 25  45.0  44.4 -3.6     -97.0   -13      416   17 44 39
17 47 27  ---          12 27 26  45.4  44.3 -3.6     -97.7   167      427   17 44 28

17 48 17  J1545+5400   12 28 16  47.8  41.7 -3.3    -103.1    37      427   17 48 17
17 50 17  =1544+541    12 30 16  48.1  41.6 -3.3    -103.6   120      435   17 48 18

17 50 17  4C52         12 30 16  45.8  44.2 -3.5     -98.3   -12      435   17 50 29
17 53 17  ---          12 33 17  46.3  44.1 -3.5     -99.0   168      445   17 50 18

17 54 07  J1545+5400   12 34 07  48.7  41.4 -3.2    -104.5    38      445   17 54 07
17 55 07  =1544+541    12 35 07  48.8  41.4 -3.2    -104.8    60      449   17 54 08

17 55 07  4C52         12 35 07  46.6  44.0 -3.5     -99.4   -12      449   17 55 19
17 58 07  ---          12 38 08  47.0  43.9 -3.4    -100.1   168      460   17 55 08

17 58 57  J1545+5400   12 38 58  49.3  41.1 -3.1    -105.7    38      460   17 58 57
18 00 57  =1544+541    12 40 58  49.6  41.0 -3.1    -106.2   120      468   17 58 58

18 02 18  J1638+5720   12 42 19  41.9  38.5 -3.9     -97.5    57      468   18 02 18
18 06 08  =1637+574    12 46 20  42.4  38.4 -3.9     -98.4   230      483   18 02 19

18 07 30  J1545+5400   12 47 33  50.6  40.6 -3.0    -107.9    59      483   18 07 30
18 10 20  =1544+541    12 50 33  51.0  40.4 -2.9    -108.7   170      494   18 07 31

18 10 20  4C52         12 50 23  48.8  43.4 -3.2    -102.9   -12      494   18 10 33
18 13 20  ---          12 53 24  49.3  43.2 -3.2    -103.7   168      504   18 10 21

18 14 10  J1545+5400   12 54 14  51.5  40.1 -2.9    -109.7    38      504   18 14 10
18 16 10  =1544+541    12 56 14  51.8  39.9 -2.8    -110.2   120      512   18 14 11
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  15 Oct 2015   Day 288 ---

18 16 10  4C52         12 56 14  49.7  43.0 -3.1    -104.3   -12      512   18 16 22
18 19 10  ---          12 59 15  50.1  42.9 -3.1    -105.1   168      523   18 16 11

18 20 00  J1545+5400   13 00 05  52.3  39.6 -2.8    -111.2    38      523   18 20 00
18 21 00  =1544+541    13 01 05  52.4  39.5 -2.8    -111.5    60      527   18 20 01

18 21 00  4C52         13 01 05  50.4  42.7 -3.0    -105.5   -12      527   18 21 12
18 24 00  ---          13 04 06  50.8  42.5 -3.0    -106.3   168      538   18 21 01

18 24 50  J1545+5400   13 04 56  53.0  39.2 -2.7    -112.5    38      538   18 24 50
18 26 50  =1544+541    13 06 56  53.2  39.0 -2.7    -113.1   120      545   18 24 51

18 26 50  4C52         13 06 56  51.3  42.3 -2.9    -107.0   -12      545   18 27 02
18 29 50  ---          13 09 56  51.7  42.1 -2.9    -107.8   168      556   18 26 51

18 30 40  J1545+5400   13 10 47  53.7  38.6 -2.6    -114.2    38      556   18 30 40
18 31 40  =1544+541    13 11 47  53.9  38.5 -2.6    -114.5    60      560   18 30 41

18 31 40  4C52         13 11 47  52.0  42.0 -2.9    -108.2   -12      560   18 31 52
18 34 40  ---          13 14 47  52.4  41.8 -2.8    -109.0   168      571   18 31 41

18 35 30  J1545+5400   13 15 37  54.4  38.1 -2.5    -115.6    38      571   18 35 30
18 37 30  =1544+541    13 17 38  54.7  37.8 -2.5    -116.2   120      579   18 35 31

18 37 30  4C52         13 17 38  52.8  41.5 -2.8    -109.8   -12      579   18 37 42
18 40 30  ---          13 20 38  53.2  41.3 -2.7    -110.6   168      589   18 37 31

18 41 20  J1545+5400   13 21 28  55.2  37.4 -2.4    -117.3    38      589   18 41 20
18 42 20  =1544+541    13 22 29  55.3  37.3 -2.4    -117.6    60      593   18 41 21

18 42 20  4C52         13 22 29  53.5  41.1 -2.7    -111.1   -12      593   18 42 32
18 45 20  ---          13 25 29  53.9  40.8 -2.6    -111.9   168      604   18 42 21

18 46 10  J1545+5400   13 26 19  55.8  36.8 -2.3    -118.8    38      604   18 46 10
18 48 10  =1544+541    13 28 19  56.0  36.6 -2.3    -119.4   120      612   18 46 11

18 48 10  4C52         13 28 19  54.3  40.5 -2.6    -112.7   -11      612   18 48 22
18 51 10  ---          13 31 20  54.7  40.2 -2.5    -113.6   169      623   18 48 11

18 52 00  J1545+5400   13 32 10  56.5  36.1 -2.2    -120.6    39      623   18 52 00
18 53 00  =1544+541    13 33 10  56.7  35.9 -2.2    -120.9    60      627   18 52 01

18 53 00  4C52         13 33 10  55.0  40.0 -2.5    -114.1   -11      627   18 53 12
18 56 00  ---          13 36 11  55.4  39.7 -2.5    -114.9   169      637   18 53 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  15 Oct 2015   Day 288 ---

18 56 50  J1545+5400   13 37 01  57.1  35.4 -2.2    -122.1    39      637   18 56 50
18 58 50  =1544+541    13 39 01  57.4  35.1 -2.1    -122.8   120      645   18 56 51

18 58 50  4C52         13 39 01  55.8  39.4 -2.4    -115.8   -11      645   18 59 02
19 01 50  ---          13 42 02  56.2  39.0 -2.4    -116.7   169      656   18 58 51

19 02 40  J1545+5400   13 42 52  57.9  34.5 -2.1    -124.1    39      656   19 02 40
19 03 40  =1544+541    13 43 52  58.0  34.3 -2.0    -124.4    60      660   19 02 41

19 03 40  4C52         13 43 52  56.4  38.8 -2.3    -117.2   -11      660   19 03 51
19 06 40  ---          13 46 53  56.8  38.4 -2.3    -118.2   169      671   19 03 41

19 07 30  J1545+5400   13 47 43  58.4  33.7 -2.0    -125.7    39      671   19 07 30
19 09 30  =1544+541    13 49 43  58.7  33.4 -1.9    -126.4   120      678   19 07 31

19 09 30  4C52         13 49 43  57.2  38.0 -2.2    -119.0   -11      678   19 09 42
19 12 30  ---          13 52 43  57.6  37.6 -2.2    -120.0   169      689   19 09 31

19 13 20  J1545+5400   13 53 34  59.1  32.7 -1.9    -127.7    39      689   19 13 20
19 14 20  =1544+541    13 54 34  59.3  32.6 -1.9    -128.1    60      693   19 13 21

19 14 20  4C52         13 54 34  57.9  37.3 -2.1    -120.6   -11      693   19 14 32
19 17 20  ---          13 57 34  58.3  36.9 -2.1    -121.5   169      704   19 14 21

19 18 10  J1545+5400   13 58 24  59.7  31.9 -1.8    -129.5    39      704   19 18 10
19 20 10  =1544+541    14 00 25  59.9  31.5 -1.8    -130.2   120      712   19 18 11

19 21 32  J1638+5720   14 01 46  52.1  33.7 -2.6    -117.8    58      712   19 21 32
19 25 22  =1637+574    14 05 47  52.6  33.3 -2.5    -118.9   230      727   19 21 33

19 26 45  J1545+5400   14 07 01  60.6  30.2 -1.7    -132.6    60      727   19 26 45
19 29 35  =1544+541    14 10 01  61.0  29.6 -1.6    -133.8   170      738   19 26 46

19 29 35  4C52         14 09 51  59.8  34.9 -1.9    -125.7   -12      738   19 29 47
19 32 35  ---          14 12 52  60.2  34.3 -1.8    -126.8   168      748   19 29 36

19 33 25  J1545+5400   14 13 42  61.4  28.8 -1.5    -135.2    38      748   19 33 25
19 35 25  =1544+541    14 15 42  61.6  28.3 -1.5    -136.0   120      756   19 33 26

19 35 25  4C52         14 15 42  60.5  33.8 -1.8    -127.8   -12      756   19 35 37
19 38 25  ---          14 18 43  60.9  33.2 -1.7    -128.9   168      767   19 35 26

19 39 15  J1545+5400   14 19 33  62.0  27.5 -1.4    -137.6    38      767   19 39 15
19 40 15  =1544+541    14 20 33  62.1  27.2 -1.4    -138.0    60      771   19 39 16
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  15 Oct 2015   Day 288 ---

19 40 15  4C52         14 20 33  61.1  32.9 -1.7    -129.6   -12      771   19 40 27
19 43 15  ---          14 23 33  61.4  32.3 -1.7    -130.7   168      782   19 40 16

19 44 05  J1545+5400   14 24 24  62.4  26.3 -1.4    -139.6    38      782   19 44 05
19 46 05  =1544+541    14 26 24  62.6  25.8 -1.3    -140.4   120      789   19 44 06

19 46 05  4C52         14 26 24  61.8  31.7 -1.6    -131.8   -12      789   19 46 17
19 49 05  ---          14 29 24  62.1  31.0 -1.6    -133.0   168      800   19 46 06

19 49 55  J1545+5400   14 30 14  63.0  24.9 -1.3    -142.0    38      800   19 49 55
19 50 55  =1544+541    14 31 15  63.1  24.6 -1.2    -142.5    60      804   19 49 56

19 50 55  4C52         14 31 15  62.3  30.6 -1.5    -133.7   -12      804   19 51 07
19 53 55  ---          14 34 15  62.6  29.9 -1.5    -134.9   168      815   19 50 56

19 54 45  J1545+5400   14 35 05  63.4  23.6 -1.2    -144.1    38      815   19 54 45
19 56 45  =1544+541    14 37 06  63.6  23.1 -1.2    -145.0   120      823   19 54 46

19 56 45  4C52         14 37 06  62.9  29.2 -1.4    -136.1   -12      823   19 56 57
19 59 45  ---          14 40 06  63.2  28.5 -1.4    -137.3   168      833   19 56 46

20 00 35  J1545+5400   14 40 56  63.9  22.0 -1.1    -146.8    38      833   20 00 35
20 01 35  =1544+541    14 41 56  64.0  21.7 -1.1    -147.2    60      837   20 00 36

20 01 35  4C52         14 41 56  63.4  28.1 -1.4    -138.1   -12      837   20 01 48
20 04 35  ---          14 44 57  63.7  27.3 -1.3    -139.4   168      848   20 01 36

20 05 25  J1545+5400   14 45 47  64.3  20.6 -1.0    -149.0    38      848   20 05 25
20 07 25  =1544+541    14 47 47  64.4  20.0 -1.0    -149.9   120      856   20 05 26

20 07 25  4C52         14 47 47  64.0  26.5 -1.3    -140.6   -12      856   20 07 38
20 10 25  ---          14 50 48  64.3  25.7 -1.2    -142.0   168      867   20 07 26

20 11 15  J1545+5400   14 51 38  64.7  18.9 -0.9    -151.7    37      867   20 11 15
20 12 15  =1544+541    14 52 38  64.8  18.6 -0.9    -152.2    60      871   20 11 16

20 12 15  4C52         14 52 38  64.5  25.2 -1.2    -142.8   -13      871   20 12 28
20 15 15  ---          14 55 39  64.7  24.4 -1.1    -144.2   167      881   20 12 16

20 16 05  J1545+5400   14 56 29  65.0  17.4 -0.8    -154.1    37      881   20 16 05
20 18 05  =1544+541    14 58 29  65.1  16.8 -0.8    -155.0   120      889   20 16 06

20 18 05  4C52         14 58 29  65.0  23.5 -1.1    -145.5   -13      889   20 18 18
20 21 05  ---          15 01 30  65.2  22.6 -1.0    -146.9   167      900   20 18 06
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  15 Oct 2015   Day 288 ---

20 21 55  J1545+5400   15 02 20  65.4  15.5 -0.7    -156.9    37      900   20 21 55
20 22 55  =1544+541    15 03 20  65.4  15.2 -0.7    -157.4    60      904   20 21 56

20 22 55  4C52         15 03 20  65.4  22.1 -1.0    -147.8   -13      904   20 23 08
20 25 55  ---          15 06 20  65.6  21.1 -0.9    -149.2   167      914   20 22 56

20 26 45  J1545+5400   15 07 11  65.6  13.9 -0.6    -159.4    37      914   20 26 45
20 28 45  =1544+541    15 09 11  65.7  13.3 -0.6    -160.4   120      922   20 26 46

20 28 45  4C52         15 09 11  65.8  20.2 -0.9    -150.6   -13      922   20 28 58
20 31 45  ---          15 12 11  66.1  19.2 -0.9    -152.1   167      933   20 28 46

20 32 35  J1545+5400   15 13 01  65.9  12.0 -0.6    -162.3    37      933   20 32 35
20 33 35  =1544+541    15 14 02  66.0  11.6 -0.5    -162.9    60      937   20 32 36

20 33 35  4C52         15 14 02  66.2  18.6 -0.8    -153.0   -13      937   20 33 48
20 36 35  ---          15 17 02  66.4  17.6 -0.8    -154.5   167      948   20 33 36

20 37 25  J1545+5400   15 17 52  66.1  10.3 -0.5    -164.9    37      948   20 37 25
20 39 25  =1544+541    15 19 53  66.2   9.6 -0.4    -165.9   120      955   20 37 26

20 40 46  J1638+5720   15 21 13  60.2  21.0 -1.3    -145.1    60      955   20 40 46
20 44 36  =1637+574    15 25 14  60.5  20.1 -1.2    -146.7   230      970   20 40 47

20 45 57  J1545+5400   15 26 26  66.4   7.2 -0.3    -169.4    62      970   20 45 57
20 48 47  =1544+541    15 29 26  66.5   6.1 -0.3    -171.0   170      981   20 45 58

20 48 47  4C52         15 29 16  67.1  13.3 -0.6    -161.0   -13      981   20 49 00
20 52 07  ---          15 32 37  67.2  12.0 -0.5    -162.8   187      993   20 48 48

20 52 57  J1545+5400   15 33 27  66.6   4.7 -0.2    -173.1    37      993   20 52 57
20 55 27  =1544+541    15 35 57  66.6   3.8 -0.2    -174.5   150     1003   20 52 58

20 55 27  4C52         15 35 57  67.4  10.8 -0.5    -164.6   -13     1003   20 55 40
20 58 57  ---          15 39 28  67.5   9.4 -0.4    -166.5   197     1015   20 55 28

20 59 47  J1545+5400   15 40 18  66.6   2.1 -0.1    -176.9    37     1015   20 59 47
21 01 17  =1544+541    15 41 48  66.7   1.6 -0.1    -177.7    90     1021   20 59 48

21 01 17  4C52         15 41 48  67.6   8.5 -0.4    -167.8   -13     1021   21 01 30
21 04 37  ---          15 45 09  67.7   7.2 -0.3    -169.7   187     1033   21 01 18

21 05 27  J1545+5400   15 45 59  66.7   0.0 -0.0    -179.9    37     1033   21 05 27
21 07 57  =1544+541    15 48 29  66.7  -0.9  0.0     178.7   150     1043   21 05 28
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  15 Oct 2015   Day 288 ---

21 07 57  4C52         15 48 29  67.8   5.9 -0.2    -171.6   -13     1043   21 08 10
21 11 27  ---          15 52 00  67.8   4.5 -0.2    -173.6   197     1056   21 07 58

21 12 17  J1545+5400   15 52 50  66.6  -2.5  0.1     176.3    37     1056   21 12 17
21 13 47  =1544+541    15 54 20  66.6  -3.1  0.1     175.5    90     1061   21 12 18

21 13 47  4C52         15 54 20  67.9   3.6 -0.1    -174.9   -13     1061   21 14 00
21 17 07  ---          15 57 41  67.9   2.2 -0.1    -176.8   187     1073   21 13 48

21 17 57  J1545+5400   15 58 31  66.6  -4.6  0.2     173.3    37     1073   21 17 57
21 20 27  =1544+541    16 01 01  66.5  -5.5  0.2     171.9   150     1083   21 17 58

21 20 27  4C52         16 01 01  67.9   0.9 -0.0    -178.8   -12     1083   21 20 40
21 23 57  ---          16 04 32  67.9  -0.5  0.0     179.2   198     1096   21 20 28

21 24 47  J1545+5400   16 05 22  66.4  -7.1  0.3     169.6    38     1096   21 24 47
21 26 17  =1544+541    16 06 52  66.4  -7.6  0.3     168.8    90     1102   21 24 48

21 26 17  4C52         16 06 52  67.9  -1.5  0.1     177.9   -12     1102   21 26 30
21 29 37  ---          16 10 13  67.9  -2.8  0.1     176.0   188     1114   21 26 18

21 30 27  J1545+5400   16 11 03  66.2  -9.1  0.4     166.6    38     1114   21 30 27
21 32 57  =1544+541    16 13 34  66.1 -10.0  0.5     165.3   150     1123   21 30 28

21 32 57  4C52         16 13 34  67.9  -4.2  0.2     174.1   -12     1123   21 33 09
21 36 27  ---          16 17 04  67.8  -5.6  0.2     172.1   198     1136   21 32 58

21 37 17  J1545+5400   16 17 54  66.0 -11.5  0.5     163.0    38     1136   21 37 17
21 38 47  =1544+541    16 19 25  65.9 -12.0  0.6     162.2    90     1142   21 37 18

21 38 47  4C52         16 19 25  67.7  -6.5  0.3     170.8   -12     1142   21 38 59
21 42 07  ---          16 22 45  67.7  -7.8  0.3     168.9   188     1154   21 38 48

21 42 57  J1545+5400   16 23 35  65.7 -13.5  0.6     160.1    38     1154   21 42 57
21 45 27  =1544+541    16 26 06  65.6 -14.3  0.7     158.8   150     1164   21 42 58

21 45 27  4C52         16 26 06  67.5  -9.1  0.4     167.0   -12     1164   21 45 39
21 48 57  ---          16 29 36  67.4 -10.5  0.4     165.1   198     1177   21 45 28

21 49 47  J1545+5400   16 30 26  65.3 -15.7  0.7     156.6    38     1177   21 49 47
21 51 17  =1544+541    16 31 57  65.2 -16.2  0.8     155.9    90     1182   21 49 48

21 51 17  4C52         16 31 57  67.3 -11.3  0.5     163.8   -12     1182   21 51 29
21 54 37  ---          16 35 17  67.2 -12.6  0.5     162.0   188     1194   21 51 18
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  15 Oct 2015   Day 288 ---

21 55 27  J1545+5400   16 36 07  65.0 -17.5  0.8     153.9    38     1194   21 55 27
21 57 57  =1544+541    16 38 38  64.8 -18.3  0.9     152.6   150     1204   21 55 28

21 57 57  4C52         16 38 38  67.0 -13.8  0.6     160.2   -12     1204   21 58 10
22 01 27  ---          16 42 08  66.8 -15.1  0.6     158.3   198     1217   21 57 58

22 02 17  J1545+5400   16 42 58  64.5 -19.6  0.9     150.6    38     1217   22 02 17
22 03 47  =1544+541    16 44 29  64.4 -20.1  1.0     149.9    90     1223   22 02 18

22 03 47  4C52         16 44 29  66.7 -15.9  0.7     157.1   -13     1223   22 04 00
22 07 07  ---          16 47 49  66.5 -17.1  0.7     155.3   187     1235   22 03 48

22 07 57  J1545+5400   16 48 39  64.1 -21.3  1.0     147.9    37     1235   22 07 57
22 10 27  =1544+541    16 51 10  63.9 -22.0  1.1     146.8   150     1244   22 07 58

22 11 44  J1638+5720   16 52 26  63.2  -4.2  0.2     173.3    56     1244   22 11 44
22 15 34  =1637+574    16 56 27  63.1  -5.4  0.3     171.4   230     1259   22 11 45

22 16 51  J1545+5400   16 57 35  63.4 -23.7  1.2     143.9    57     1259   22 16 51
22 20 01  =1544+541    17 00 55  63.1 -24.6  1.2     142.5   190     1271   22 16 52

22 20 01  4C52         17 00 45  65.6 -21.3  1.0     148.9   -13     1271   22 20 14
22 23 31  ---          17 04 16  65.3 -22.4  1.0     147.2   197     1284   22 20 02

22 24 21  J1545+5400   17 05 06  62.7 -25.7  1.3     140.7    37     1284   22 24 21
22 26 51  =1544+541    17 07 36  62.4 -26.3  1.4     139.6   150     1294   22 24 22

22 26 51  4C52         17 07 36  65.0 -23.4  1.1     145.6   -13     1294   22 27 04
22 30 21  ---          17 11 07  64.7 -24.5  1.1     144.0   197     1306   22 26 52

22 31 11  J1545+5400   17 11 57  62.0 -27.3  1.4     137.9    37     1306   22 31 11
22 32 11  =1544+541    17 12 57  61.9 -27.5  1.4     137.4    60     1310   22 31 12

22 32 11  4C52         17 12 57  64.5 -25.0  1.2     143.2   -13     1310   22 32 24
22 35 41  ---          17 16 28  64.2 -26.0  1.2     141.6   197     1323   22 32 12

22 36 31  J1545+5400   17 17 18  61.5 -28.5  1.5     135.7    37     1323   22 36 31
22 39 01  =1544+541    17 19 48  61.2 -29.1  1.6     134.7   150     1333   22 36 32

22 39 01  4C52         17 19 48  63.9 -26.9  1.3     140.1   -13     1333   22 39 15
22 42 31  ---          17 23 19  63.5 -27.8  1.3     138.6   197     1345   22 39 02

22 43 21  J1545+5400   17 24 09  60.8 -30.0  1.6     133.0    37     1345   22 43 21
22 44 21  =1544+541    17 25 09  60.7 -30.2  1.7     132.7    60     1349   22 43 22
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  15 Oct 2015   Day 288 ---

22 44 21  4C52         17 25 09  63.4 -28.2  1.4     137.8   -13     1349   22 44 35
22 47 51  ---          17 28 40  63.0 -29.1  1.4     136.3   197     1362   22 44 22

22 48 41  J1545+5400   17 29 30  60.2 -31.0  1.7     131.0    37     1362   22 48 41
22 51 11  =1544+541    17 32 00  59.9 -31.5  1.8     130.1   150     1372   22 48 42

22 51 11  4C52         17 32 00  62.6 -29.9  1.5     135.0   -13     1372   22 51 25
22 54 41  ---          17 35 31  62.3 -30.7  1.5     133.6   197     1384   22 51 12

22 55 31  J1545+5400   17 36 21  59.4 -32.3  1.8     128.5    37     1384   22 55 31
22 56 31  =1544+541    17 37 21  59.3 -32.5  1.9     128.2    60     1388   22 55 32

22 56 31  4C52         17 37 21  62.1 -31.1  1.6     132.8   -13     1388   22 56 45
23 00 01  ---          17 40 52  61.7 -31.9  1.6     131.5   197     1401   22 56 32

23 00 51  J1545+5400   17 41 42  58.8 -33.3  1.9     126.7    36     1401   23 00 51
23 03 21  =1544+541    17 44 12  58.5 -33.7  2.0     125.8   150     1410   23 00 52

23 03 21  4C52         17 44 12  61.3 -32.5  1.7     130.2   -14     1410   23 03 35
23 06 51  ---          17 47 43  60.9 -33.2  1.7     128.9   196     1423   23 03 22

23 07 41  J1545+5400   17 48 33  58.0 -34.4  2.0     124.3    36     1423   23 07 41
23 08 41  =1544+541    17 49 33  57.8 -34.5  2.1     124.0    60     1427   23 07 42

23 08 41  4C52         17 49 33  60.7 -33.6  1.8     128.2   -14     1427   23 08 55
23 12 11  ---          17 53 04  60.2 -34.3  1.8     126.9   196     1440   23 08 42

23 13 01  J1545+5400   17 53 54  57.3 -35.2  2.1     122.6    36     1440   23 13 01
23 15 31  =1544+541    17 56 24  57.0 -35.5  2.2     121.7   150     1449   23 13 02

23 15 31  4C52         17 56 24  59.8 -34.9  1.9     125.8   -14     1449   23 15 45
23 19 01  ---          17 59 55  59.4 -35.5  1.9     124.5   196     1462   23 15 32

23 19 51  J1545+5400   18 00 45  56.4 -36.1  2.2     120.4    36     1462   23 19 51
23 20 51  =1544+541    18 01 45  56.3 -36.3  2.3     120.0    60     1466   23 19 52

23 20 51  4C52         18 01 45  59.2 -35.8  2.0     123.9   -14     1466   23 21 05
23 24 21  ---          18 05 16  58.7 -36.3  2.0     122.7   196     1478   23 20 52

23 25 11  J1545+5400   18 06 06  55.8 -36.8  2.3     118.7    36     1478   23 25 11
23 27 41  =1544+541    18 08 36  55.4 -37.2  2.4     117.9   150     1488   23 25 12

23 27 41  4C52         18 08 36  58.3 -36.9  2.1     121.6   -14     1488   23 27 55
23 31 11  ---          18 12 07  57.8 -37.4  2.1     120.5   196     1501   23 27 42
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  15 Oct 2015   Day 288 ---

23 32 01  J1545+5400   18 12 57  54.9 -37.7  2.4     116.6    36     1501   23 32 01
23 33 01  =1544+541    18 13 57  54.7 -37.8  2.5     116.3    60     1504   23 32 02

23 33 01  4C52         18 13 57  57.6 -37.6  2.2     119.9   -14     1504   23 33 15
23 36 31  ---          18 17 28  57.1 -38.1  2.2     118.8   196     1517   23 33 02

23 37 21  J1545+5400   18 18 18  54.2 -38.3  2.5     115.1    36     1517   23 37 21
23 39 51  =1544+541    18 20 48  53.8 -38.5  2.6     114.4   150     1527   23 37 22

23 41 01  J1638+5720   18 21 58  57.9 -26.3  1.7     135.1    53     1527   23 41 01
23 44 51  =1637+574    18 25 59  57.5 -27.0  1.8     133.6   230     1542   23 41 02

23 46 01  J1545+5400   18 26 59  53.0 -39.1  2.7     112.6    53     1542   23 46 01
23 48 51  =1544+541    18 30 00  52.6 -39.4  2.7     111.8   170     1553   23 46 02

23 48 51  4C52         18 29 50  55.5 -39.6  2.4     115.1   -14     1553   23 49 05
23 52 21  ---          18 33 20  55.0 -40.0  2.5     114.0   196     1565   23 48 52

23 53 11  J1545+5400   18 34 10  52.0 -39.8  2.8     110.7    36     1565   23 53 11
23 55 11  =1544+541    18 36 11  51.7 -39.9  2.8     110.1   120     1573   23 53 12

23 55 11  4C52         18 36 11  54.6 -40.3  2.5     113.2   -14     1573   23 55 25
23 58 41  ---          18 39 41  54.1 -40.7  2.6     112.3   196     1586   23 55 12

 --- Start: Thu  15 Oct 2015   Day 288 -- Stop: Fri  16 Oct 2015   Day 289 ---

23 59 31  J1545+5400   18 40 31  51.1 -40.3  2.9     109.0    36     1586   23 59 31
00 00 31  =1544+541    18 41 32  51.0 -40.4  2.9     108.7    60     1589   23 59 32

00 00 31  4C52         18 41 32  53.8 -40.9  2.6     111.7   -14     1589   00 00 45
00 04 01  ---          18 45 02  53.3 -41.2  2.7     110.8   196     1602   00 00 32

00 04 51  J1545+5400   18 45 52  50.4 -40.7  3.0     107.6    36     1602   00 04 51
00 06 51  =1544+541    18 47 53  50.1 -40.8  3.0     107.1   120     1610   00 04 52

00 06 51  4C52         18 47 53  52.9 -41.4  2.7     110.0   -14     1610   00 07 05
00 10 21  ---          18 51 23  52.4 -41.7  2.8     109.1   196     1622   00 06 52

00 11 11  J1545+5400   18 52 13  49.5 -41.1  3.1     106.0    36     1622   00 11 11
00 12 11  =1544+541    18 53 13  49.3 -41.1  3.1     105.7    60     1626   00 11 12

00 12 11  4C52         18 53 13  52.2 -41.9  2.8     108.6   -14     1626   00 12 25
00 15 41  ---          18 56 44  51.7 -42.1  2.9     107.7   196     1639   00 12 12
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Oct 2015   Day 289 ---

00 16 31  J1545+5400   18 57 34  48.7 -41.4  3.2     104.7    36     1639   00 16 31
00 18 31  =1544+541    18 59 35  48.4 -41.5  3.2     104.2   120     1647   00 16 32

00 18 31  4C52         18 59 35  51.2 -42.4  2.9     107.0   -14     1647   00 18 45
00 22 01  ---          19 03 05  50.7 -42.6  3.0     106.1   196     1659   00 18 32

00 22 51  J1545+5400   19 03 55  47.8 -41.7  3.3     103.1    36     1659   00 22 51
00 23 51  =1544+541    19 04 55  47.7 -41.8  3.3     102.9    60     1663   00 22 52

00 23 51  4C52         19 04 55  50.5 -42.7  3.0     105.6   -13     1663   00 24 05
00 27 21  ---          19 08 26  50.0 -42.9  3.1     104.8   197     1676   00 23 52

00 28 11  J1545+5400   19 09 16  47.1 -42.0  3.4     101.9    36     1676   00 28 11
00 30 11  =1544+541    19 11 16  46.8 -42.1  3.4     101.4   120     1683   00 28 12

00 30 11  4C52         19 11 16  49.5 -43.1  3.1     104.1   -13     1683   00 30 25
00 33 41  ---          19 14 47  49.0 -43.3  3.2     103.2   197     1696   00 30 12

00 34 31  J1545+5400   19 15 37  46.1 -42.3  3.5     100.4    36     1696   00 34 31
00 35 31  =1544+541    19 16 37  46.0 -42.3  3.5     100.2    60     1700   00 34 32

00 35 31  4C52         19 16 37  48.8 -43.4  3.2     102.8   -13     1700   00 35 45
00 39 01  ---          19 20 08  48.2 -43.6  3.3     102.0   197     1713   00 35 32

00 39 51  J1545+5400   19 20 58  45.4 -42.4  3.6      99.2    37     1713   00 39 51
00 41 51  =1544+541    19 22 58  45.1 -42.5  3.6      98.7   120     1720   00 39 52

00 41 51  4C52         19 22 58  47.8 -43.7  3.3     101.3   -13     1720   00 42 05
00 45 21  ---          19 26 29  47.3 -43.8  3.4     100.5   197     1733   00 41 52

00 46 11  J1545+5400   19 27 19  44.4 -42.6  3.7      97.8    37     1733   00 46 11
00 47 11  =1544+541    19 28 19  44.3 -42.7  3.7      97.5    60     1737   00 46 12

00 47 11  4C52         19 28 19  47.0 -43.9  3.4     100.1   -13     1737   00 47 25
00 50 41  ---          19 31 50  46.5 -44.0  3.5      99.3   197     1750   00 47 12

00 51 31  J1545+5400   19 32 40  43.7 -42.8  3.8      96.6    37     1750   00 51 31
00 53 31  =1544+541    19 34 40  43.4 -42.8  3.8      96.1   120     1757   00 51 32

00 53 31  4C52         19 34 40  46.1 -44.1  3.5      98.6   -13     1757   00 53 44
00 57 01  ---          19 38 11  45.5 -44.2  3.6      97.9   197     1770   00 53 32

00 57 51  J1545+5400   19 39 01  42.7 -42.9  3.9      95.2    37     1770   00 57 51
00 58 51  =1544+541    19 40 01  42.6 -42.9  3.9      95.0    60     1774   00 57 52
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Oct 2015   Day 289 ---

00 58 51  4C52         19 40 01  45.3 -44.3  3.6      97.5   -13     1774   00 59 04
01 02 21  ---          19 43 32  44.7 -44.4  3.7      96.7   197     1787   00 58 52

01 03 11  J1545+5400   19 44 22  41.9 -43.0  4.0      94.1    37     1787   01 03 11
01 05 11  =1544+541    19 46 22  41.7 -43.0  4.0      93.6   120     1794   01 03 12

01 06 14  J1638+5720   19 47 26  48.1 -36.4  3.1     108.9    42     1794   01 06 14
01 10 04  =1637+574    19 51 26  47.6 -36.7  3.2     107.9   230     1809   01 06 15

01 11 09  J1545+5400   19 52 21  40.8 -43.1  4.1      92.4    43     1809   01 11 09
01 13 59  =1544+541    19 55 21  40.3 -43.1  4.2      91.8   170     1820   01 11 10

01 13 59  4C52         19 55 11  43.0 -44.6  3.9      94.2   -13     1820   01 14 12
01 17 29  ---          19 58 42  42.4 -44.7  3.9      93.5   197     1833   01 14 00

01 18 19  J1545+5400   19 59 32  39.7 -43.1  4.2      90.9    37     1833   01 18 19
01 20 19  =1544+541    20 01 32  39.4 -43.1  4.3      90.5   120     1841   01 18 20

01 20 19  4C52         20 01 32  42.0 -44.7  4.0      92.9   -13     1841   01 20 32
01 23 19  ---          20 04 33  41.6 -44.7  4.0      92.3   167     1851   01 20 20

01 24 09  J1545+5400   20 05 23  38.9 -43.1  4.3      89.7    37     1851   01 24 09
01 25 09  =1544+541    20 06 23  38.7 -43.1  4.3      89.5    60     1855   01 24 10

01 25 09  4C52         20 06 23  41.3 -44.7  4.1      91.9   -13     1855   01 25 22
01 28 39  ---          20 09 54  40.8 -44.8  4.1      91.2   197     1868   01 25 10

01 29 29  J1545+5400   20 10 44  38.1 -43.1  4.4      88.7    37     1868   01 29 29
01 31 29  =1544+541    20 12 44  37.8 -43.1  4.4      88.3   120     1876   01 29 30

01 31 29  4C52         20 12 44  40.3 -44.8  4.2      90.6   -13     1876   01 31 42
01 34 29  ---          20 15 45  39.9 -44.8  4.2      90.0   167     1886   01 31 30

01 35 19  J1545+5400   20 16 35  37.2 -43.1  4.5      87.5    37     1886   01 35 19
01 36 19  =1544+541    20 17 35  37.1 -43.1  4.5      87.3    60     1890   01 35 20

01 36 19  4C52         20 17 35  39.6 -44.8  4.2      89.7   -13     1890   01 36 32
01 39 49  ---          20 21 05  39.1 -44.8  4.3      89.0   197     1903   01 36 20

01 40 39  J1545+5400   20 21 56  36.4 -43.0  4.6      86.4    37     1903   01 40 39
01 42 39  =1544+541    20 23 56  36.1 -43.0  4.6      86.1   120     1911   01 40 40

01 42 39  4C52         20 23 56  38.6 -44.8  4.3      88.4   -13     1911   01 42 52
01 45 39  ---          20 26 56  38.2 -44.7  4.4      87.8   167     1921   01 42 40
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Oct 2015   Day 289 ---

01 46 29  J1545+5400   20 27 47  35.6 -42.9  4.7      85.3    37     1921   01 46 29
01 47 29  =1544+541    20 28 47  35.4 -42.9  4.7      85.1    60     1925   01 46 30

01 47 29  4C52         20 28 47  37.9 -44.7  4.4      87.5   -13     1925   01 47 42
01 50 59  ---          20 32 17  37.4 -44.7  4.5      86.8   197     1938   01 47 30

01 51 49  J1545+5400   20 33 07  34.8 -42.9  4.8      84.3    37     1938   01 51 49
01 53 49  =1544+541    20 35 08  34.5 -42.8  4.8      83.9   120     1946   01 51 50

01 53 49  4C52         20 35 08  36.9 -44.7  4.5      86.3   -13     1946   01 54 02
01 56 49  ---          20 38 08  36.5 -44.6  4.6      85.7   167     1956   01 53 50

01 57 39  J1545+5400   20 38 58  33.9 -42.7  4.9      83.2    37     1956   01 57 39
01 58 39  =1544+541    20 39 59  33.8 -42.7  4.9      83.0    60     1960   01 57 40

01 58 39  4C52         20 39 59  36.2 -44.6  4.6      85.3   -13     1960   01 58 51
02 02 09  ---          20 43 29  35.7 -44.5  4.7      84.7   197     1973   01 58 40

02 02 59  J1545+5400   20 44 19  33.2 -42.6  5.0      82.1    37     1973   02 02 59
02 04 59  =1544+541    20 46 20  32.9 -42.6  5.0      81.8   120     1981   02 03 00

02 04 59  4C52         20 46 20  35.2 -44.5  4.7      84.1   -13     1981   02 05 11
02 07 59  ---          20 49 20  34.8 -44.4  4.8      83.6   167     1991   02 05 00

02 08 49  J1545+5400   20 50 10  32.3 -42.5  5.1      81.0    37     1991   02 08 49
02 09 49  =1544+541    20 51 10  32.2 -42.4  5.1      80.9    60     1995   02 08 50

02 09 49  4C52         20 51 10  34.5 -44.4  4.8      83.2   -13     1995   02 10 01
02 13 19  ---          20 54 41  34.0 -44.3  4.9      82.6   197     2008   02 09 50

02 14 09  J1545+5400   20 55 31  31.5 -42.3  5.2      80.0    37     2008   02 14 09
02 16 09  =1544+541    20 57 31  31.2 -42.3  5.2      79.7   120     2016   02 14 10

02 16 09  4C52         20 57 31  33.6 -44.2  4.9      82.0   -13     2016   02 16 21
02 19 09  ---          21 00 32  33.1 -44.2  5.0      81.5   167     2027   02 16 10

02 19 59  J1545+5400   21 01 22  30.7 -42.1  5.3      79.0    37     2027   02 19 59
02 20 59  =1544+541    21 02 22  30.5 -42.1  5.3      78.8    60     2030   02 20 00

02 20 59  4C52         21 02 22  32.8 -44.1  5.0      81.1   -13     2030   02 21 11
02 23 59  ---          21 05 23  32.4 -44.0  5.0      80.6   167     2041   02 21 00

02 24 49  J1545+5400   21 06 13  30.0 -42.0  5.3      78.1    37     2041   02 24 49
02 26 49  =1544+541    21 08 13  29.7 -41.9  5.4      77.7   120     2049   02 24 50
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Oct 2015   Day 289 ---

02 27 52  J1638+5720   21 09 16  37.2 -38.9  4.5      90.0    40     2049   02 27 52
02 31 42  =1637+574    21 13 17  36.7 -38.9  4.6      89.1   230     2064   02 27 53

02 32 46  J1545+5400   21 14 12  28.8 -41.7  5.5      76.6    41     2064   02 32 46
02 35 36  =1544+541    21 17 12  28.4 -41.6  5.5      76.0   170     2075   02 32 47

02 35 36  4C52         21 17 02  30.6 -43.6  5.2      78.5   -12     2075   02 35 49
02 38 56  ---          21 20 23  30.1 -43.5  5.3      77.9   188     2087   02 35 37

02 39 46  J1545+5400   21 21 13  27.8 -41.4  5.6      75.3    38     2087   02 39 46
02 41 46  =1544+541    21 23 13  27.6 -41.3  5.6      74.9   120     2094   02 39 47

02 41 46  4C52         21 23 13  29.7 -43.4  5.3      77.4   -12     2094   02 41 59
02 44 46  ---          21 26 14  29.3 -43.3  5.4      76.8   168     2105   02 41 47

02 45 36  J1545+5400   21 27 04  27.0 -41.1  5.7      74.2    38     2105   02 45 36
02 46 36  =1544+541    21 28 04  26.9 -41.1  5.7      74.1    60     2109   02 45 37

02 46 36  4C52         21 28 04  29.0 -43.2  5.4      76.5   -12     2109   02 46 48
02 49 56  ---          21 31 25  28.5 -43.1  5.5      75.9   188     2121   02 46 37

02 50 46  J1545+5400   21 32 15  26.3 -40.9  5.8      73.3    38     2121   02 50 46
02 52 46  =1544+541    21 34 15  26.0 -40.8  5.8      72.9   120     2129   02 50 47

02 52 46  4C52         21 34 15  28.1 -43.0  5.5      75.4   -12     2129   02 52 58
02 55 46  ---          21 37 15  27.7 -42.8  5.6      74.8   168     2140   02 52 47

02 56 36  J1545+5400   21 38 06  25.5 -40.6  5.9      72.2    38     2140   02 56 36
02 57 36  =1544+541    21 39 06  25.3 -40.6  5.9      72.1    60     2144   02 56 37

02 57 36  4C52         21 39 06  27.4 -42.8  5.6      74.5   -12     2144   02 57 48
03 00 56  ---          21 42 26  26.9 -42.6  5.7      73.9   188     2156   02 57 37

03 01 46  J1545+5400   21 43 16  24.7 -40.4  6.0      71.3    38     2156   03 01 46
03 03 46  =1544+541    21 45 17  24.4 -40.3  6.0      70.9   120     2164   03 01 47

03 03 46  4C52         21 45 17  26.5 -42.5  5.7      73.4   -12     2164   03 03 58
03 06 46  ---          21 48 17  26.1 -42.3  5.8      72.9   168     2174   03 03 47

03 07 36  J1545+5400   21 49 07  23.9 -40.0  6.1      70.2    38     2174   03 07 36
03 08 36  =1544+541    21 50 08  23.8 -40.0  6.1      70.1    60     2178   03 07 37

03 08 36  4C52         21 50 08  25.8 -42.2  5.8      72.6   -12     2178   03 08 48
03 11 56  ---          21 53 28  25.3 -42.1  5.8      72.0   188     2190   03 08 37
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Oct 2015   Day 289 ---

03 12 46  J1545+5400   21 54 18  23.2 -39.8  6.1      69.3    38     2190   03 12 46
03 14 46  =1544+541    21 56 19  22.9 -39.6  6.2      69.0   120     2198   03 12 47

03 14 46  4C52         21 56 19  24.9 -41.9  5.9      71.5   -12     2198   03 14 58
03 17 46  ---          21 59 19  24.5 -41.7  5.9      70.9   168     2209   03 14 47

03 18 36  J1545+5400   22 00 09  22.4 -39.4  6.2      68.3    38     2209   03 18 36
03 19 36  =1544+541    22 01 09  22.3 -39.4  6.3      68.1    60     2213   03 18 37

03 19 36  4C52         22 01 09  24.2 -41.6  6.0      70.6   -12     2213   03 19 48
03 22 56  ---          22 04 30  23.7 -41.5  6.0      70.0   188     2225   03 19 37

03 23 46  J1545+5400   22 05 20  21.7 -39.1  6.3      67.3    38     2225   03 23 46
03 25 46  =1544+541    22 07 20  21.4 -39.0  6.4      67.0   120     2233   03 23 47

03 25 46  4C52         22 07 20  23.3 -41.3  6.1      69.5   -12     2233   03 25 58
03 28 46  ---          22 10 21  22.9 -41.1  6.1      69.0   168     2243   03 25 47

03 29 36  J1545+5400   22 11 11  20.9 -38.7  6.4      66.3    38     2243   03 29 36
03 30 36  =1544+541    22 12 11  20.8 -38.7  6.4      66.1    60     2247   03 29 37

03 30 36  4C52         22 12 11  22.6 -41.0  6.1      68.7   -12     2247   03 30 48
03 33 56  ---          22 15 32  22.2 -40.8  6.2      68.1   188     2259   03 30 37

03 34 46  J1545+5400   22 16 22  20.2 -38.4  6.5      65.4    38     2259   03 34 46
03 36 46  =1544+541    22 18 22  19.9 -38.3  6.5      65.0   120     2267   03 34 47

03 36 46  4C52         22 18 22  21.8 -40.6  6.3      67.6   -12     2267   03 36 58
03 39 46  ---          22 21 23  21.3 -40.4  6.3      67.1   168     2278   03 36 47

03 40 36  J1545+5400   22 22 13  19.4 -38.0  6.6      64.3    38     2278   03 40 36
03 41 36  =1544+541    22 23 13  19.3 -38.0  6.6      64.1    60     2282   03 40 37

03 41 36  4C52         22 23 13  21.1 -40.3  6.3      66.7   -12     2282   03 41 48
03 44 36  ---          22 26 13  20.7 -40.1  6.4      66.2   168     2293   03 41 37

03 45 26  J1545+5400   22 27 04  18.8 -37.7  6.7      63.4    38     2293   03 45 26
03 47 26  =1544+541    22 29 04  18.5 -37.6  6.7      63.1   120     2300   03 45 27

03 48 29  J1638+5720   22 30 07  26.5 -37.1  5.9      73.9    39     2300   03 48 29
03 52 19  =1637+574    22 34 08  26.0 -36.9  5.9      73.1   230     2315   03 48 30

03 53 24  J1545+5400   22 35 02  17.7 -37.1  6.8      62.0    40     2315   03 53 24
03 56 14  =1544+541    22 38 03  17.4 -36.9  6.9      61.5   170     2326   03 53 25
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Oct 2015   Day 289 ---

03 56 14  4C52         22 37 53  19.1 -39.3  6.6      64.2   -11     2326   03 56 25
03 59 44  ---          22 41 24  18.6 -39.1  6.6      63.5   199     2339   03 56 15

04 00 34  J1545+5400   22 42 14  16.8 -36.6  6.9      60.7    39     2339   04 00 34
04 03 24  =1544+541    22 45 04  16.5 -36.4  7.0      60.2   170     2350   04 00 35

04 03 24  4C52         22 45 04  18.1 -38.8  6.7      62.9   -11     2350   04 03 35
04 06 54  ---          22 48 35  17.6 -38.6  6.8      62.3   199     2363   04 03 25

04 07 44  J1545+5400   22 49 25  15.9 -36.0  7.1      59.4    39     2363   04 07 44
04 09 04  =1544+541    22 50 45  15.7 -35.9  7.1      59.2    80     2368   04 07 45

04 09 04  4C52         22 50 45  17.3 -38.4  6.8      61.9   -11     2368   04 09 15
04 12 34  ---          22 54 16  16.9 -38.1  6.9      61.3   199     2381   04 09 05

04 13 24  J1545+5400   22 55 06  15.2 -35.6  7.1      58.4    39     2381   04 13 24
04 16 14  =1544+541    22 57 56  14.8 -35.4  7.2      57.9   170     2392   04 13 25

04 16 14  4C52         22 57 56  16.4 -37.9  6.9      60.6   -11     2392   04 16 25
04 19 44  ---          23 01 27  15.9 -37.6  7.0      60.0   199     2404   04 16 15

04 20 34  J1545+5400   23 02 17  14.3 -35.0  7.3      57.1    39     2404   04 20 34
04 21 54  =1544+541    23 03 37  14.1 -34.9  7.3      56.8    80     2410   04 20 35

04 21 54  4C52         23 03 37  15.6 -37.4  7.0      59.6   -11     2410   04 22 05
04 25 24  ---          23 07 08  15.2 -37.1  7.1      59.0   199     2422   04 21 55

04 26 14  J1545+5400   23 07 58  13.6 -34.5  7.4      56.0    39     2422   04 26 14
04 29 04  =1544+541    23 10 48  13.3 -34.3  7.4      55.5   170     2433   04 26 15

04 29 04  4C52         23 10 48  14.7 -36.8  7.1      58.3   -11     2433   04 29 15
04 32 34  ---          23 14 19  14.2 -36.5  7.2      57.7   199     2446   04 29 05

04 33 24  J1545+5400   23 15 09  12.7 -33.9  7.5      54.7    39     2446   04 33 24
04 34 44  =1544+541    23 16 29  12.6 -33.8  7.5      54.5    80     2451   04 33 25

04 34 44  4C52         23 16 29  14.0 -36.4  7.2      57.3   -11     2451   04 34 55
04 38 14  ---          23 20 00  13.5 -36.1  7.3      56.7   199     2464   04 34 45

04 39 04  J1545+5400   23 20 50  12.1 -33.4  7.6      53.7    39     2464   04 39 04
04 41 54  =1544+541    23 23 40  11.7 -33.2  7.6      53.2   170     2475   04 39 05

04 41 54  4C52         23 23 40  13.1 -35.7  7.3      56.0   -11     2475   04 42 04
04 45 24  ---          23 27 11  12.6 -35.4  7.4      55.4   199     2488   04 41 55
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Oct 2015   Day 289 ---

04 46 14  J1545+5400   23 28 01  11.2 -32.8  7.7      52.4    39     2488   04 46 14
04 47 34  =1544+541    23 29 21  11.1 -32.7  7.7      52.1    80     2493   04 46 15

04 47 34  4C52         23 29 21  12.3 -35.2  7.4      55.0   -11     2493   04 47 44
04 51 04  ---          23 32 52  11.9 -34.9  7.5      54.4   199     2506   04 47 35

04 51 54  J1545+5400   23 33 42  10.5 -32.2  7.8      51.3    39     2506   04 51 54
04 54 44  =1544+541    23 36 33  10.2 -32.0  7.8      50.8   170     2517   04 51 55

04 54 44  4C52         23 36 33  11.5 -34.6  7.6      53.7   -10     2517   04 54 54
04 58 14  ---          23 40 03  11.0 -34.3  7.6      53.1   200     2530   04 54 45

04 59 04  J1545+5400   23 40 53   9.7 -31.6  7.9      50.0    40     2530   04 59 04
05 00 24  =1544+541    23 42 13   9.6 -31.4  7.9      49.7    80     2535   04 59 05

05 00 24  4C52         23 42 13  10.8 -34.1  7.7      52.7   -10     2535   05 00 34
05 03 54  ---          23 45 44  10.4 -33.7  7.7      52.1   200     2548   05 00 25

05 04 44  J1545+5400   23 46 34   9.1 -31.0  8.0      48.9    40     2548   05 04 44
05 07 34  =1544+541    23 49 25   8.8 -30.7  8.1      48.4   170     2559   05 04 45

05 07 34  4C52         23 49 25   9.9 -33.4  7.8      51.4   -10     2559   05 07 44
05 11 04  ---          23 52 55   9.5 -33.1  7.8      50.7   200     2572   05 07 35

05 11 54  J1545+5400   23 53 45   8.3 -30.3  8.1      47.6    40     2572   05 11 54
05 13 14  =1544+541    23 55 06   8.2 -30.2  8.1      47.3    80     2577   05 11 55

05 13 14  4C52         23 55 06   9.2 -32.8  7.9      50.3   -10     2577   05 13 24
05 16 44  ---          23 58 36   8.8 -32.5  7.9      49.7   200     2590   05 13 15

05 17 34  J1545+5400   23 59 26   7.7 -29.7  8.2      46.5    40     2590   05 17 34
05 20 24  =1544+541    00 02 17   7.4 -29.4  8.3      46.0   170     2601   05 17 35

05 21 27  J1638+5720   00 03 20  15.1 -31.4  7.4      56.2    40     2601   05 21 27
05 25 17  =1637+574    00 07 21  14.7 -31.1  7.5      55.4   230     2615   05 21 28

05 26 21  J1545+5400   00 08 15   6.8 -28.8  8.4      44.8    41     2615   05 26 21
05 29 51  =1544+541    00 11 56   6.4 -28.4  8.4      44.1   210     2629   05 26 22


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess315.H512glob
   Matching groups in /home/guest/rmc/SCHED/sched11.4/catalogs/freq_RDBE.dat:
     v20cm_1         FD and KP filtered below 1330. SC filtered above 1440

   Setup group:    4         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00
   Net SB=         L         L         L         L         L         L         L         L
   IF SB =         L         L         L         L         L         L         L         L
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  12.9      2.1     12.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

  Frequency Set:   5  Based on FREQ, BW, and/or DOPPLER in schedule.  Used with PCAL = off
   LO sum=   1292.50  1292.50  1308.50  1308.50  1324.50  1324.50  1340.50  1340.50
   BBC fr=    807.50   807.50   791.50   791.50   775.50   775.50   759.50   759.50
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     791.50    791.50    775.50    775.50
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   5   6   7   8   9  10  11  12  13  14

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 4C52              16 01 32.849005   * 16 02 50.000000     16 03 12.250053       0.00
                     52 52 06.55530    * 52 43 54.00000      52 41 41.03224        0.00
                     From catalog imbedded in main SCHED input file.
                     Doppler based on heliocentric frame and optical definition.  Velocities:
                      31699.00 31699.00 31699.00 31699.00 31699.00 31699.00 31699.00 31699.00

   1544+541          15 44 26.760950   * 15 45 43.825751     15 46 05.839314       0.95
 * J1545+5400        54 09 58.98312    * 54 00 42.75985      53 58 08.38783        0.97
                     /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
                     GSFC 2015a astro solution, unpublished     28 observations.
                     Doppler based on other sources.

   1637+574          16 37 17.425183   * 16 38 13.456298     16 38 29.150594       0.02
 * J1638+5720        57 26 15.76131    * 57 20 23.97903      57 18 57.64130        0.01
   J1638+57          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
                     GSFC 2015a astro solution, unpublished   9070 observations.
                     Doppler based on other sources.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  4C52       sess315.H512glob      1 2 3 4 5 15                      6.997   527.978
  J1545+5400 sess315.H512glob      1 2 3 4 5 15                      4.153   333.597
  J1638+5720 sess315.H512glob      1 2 3 4 5 15                      0.639    53.986


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   4C52                70.3
   J1545+5400          69.6
   J1638+5720          77.1

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

